Contents|Index|Previous|Next

Loading on specific targets for SPARC and SPARClite

The SPARC eval boards use a host-based terminal program to load and execute programs on the target. This program, pciuh, is relatively new and it replaces the earlier ROM monitor, which had the shell in the ROM.

To use the gdb remote serial protocol to communicate with a Fujitsu SPARClite board, link your programs with the “stub” module sparc-stub.c; this module manages the communication with gdb. See The GDB remote serial protocol in Debugging with GDB in GNUPro Debugging Tools for more details.