InS_StArT
EM595.COM
1.0
^Cogent EM595 eMASTER+ PCMCIA Ethernet Card,EM595.COM,I00
?This board is software configurable, no hardware overwrites in NET.CFG
*RI00(FRAME)Media Frame Type(s)
?NOTE:	Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANS may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$OI00(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFF
InS_EnD
