InS_StArT
EM932.COM
1.0
^Cogent EM932 eMASTER+ EISA Ethernet Adapter,EM932.COM,0E0
?Hardware configuration is selected through the EISA Configuration Utility
!O0E0(SLOT)Optional Slot Number
1
2
3
4
5
6
7
8
*R0E0(FRAME)Media Frame Type(s)
?NOTE:	Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANS may be using Ethernet_802.2.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$O0E0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFF
InS_EnD
