The GPIB Software for Windows NT, version 1.30 supports the 
following GPIB interfaces (in Windows NT 3.51 or higher):

       - AT-GPIB
       - AT-GPIB/TNT
     * - AT-GPIB/TNT (Plug and Play)
     * - AT-GPIB/TNT+
       - PCI-GPIB
       - PCMCIA-GPIB
       - VXIpc Embedded Controllers

NI-488.2M Software Version 1.30 includes the following new features:

  * Support for the following hardware (for Windows NT version 4.0
    or higher only):
       - AT-GPIB/TNT (Plug and Play)
       - AT-GPIB/TNT+

NOTE: If you have either the AT-GPIB/TNT (Plug and Play) or the
      AT-GPIB/TNT+ interface, please refer to the "Getting Started
      with your AT-GPIB/TNT (PnP) and GPIB Software for Windows NT"
      manual, for information on how to enable Plug and Play support
      in Windows NT 4.0 and how to install and configure these
      particular GPIB interfaces.

The disk images are in PKZIP format. You can run the setup program from 
either floppy disks or from your hard disk. Both methods are outlined 
below.

Running the setup program from floppy disks:
--------------------------------------------
1. Unzip the disk images.  
2. Copy the unzipped files from disk1.zip onto a floppy disk, then copy 
   the unzipped files for disk2 onto a second floppy disk. 
3. To run the setup program from the floppy disks, insert the first disk
   (with the unzipped files from disk1.zip) into your floppy drive, and
   run the SETUP.EXE program.

Running the setup program from your hard disk:
----------------------------------------------
1. Create two subdirectories on your hard disk, one labeled DISK1 and the
   other labeled DISK2. 
2. Unzip disk1.zip in the DISK1 subdirectory, and disk2.zip in the DISK2 
   subdirectory.
3. To run the setup program from your hard disk, go to the DISK1 
   directory and run the SETUP.EXE program.
