  
  This version of the .CFG files are used to run the AHA-1740 series host
adapters work with EDGE triggered interupts instead of LEVEL triggered 
interrupts.  This allows the AHA-1740 series adapters to be used in some
EISA 50 Mhz systems (and faster) that do not support LEVEL triggered
interrupts.

With this .CFG file, however, only one AHA-1740 series host adapter can be
used per system in enhanced mode, unless separate hardware interrupts are 
used (selected with CNTR-R while the 'Host Adapter Interface Mode' is 
selected with the MCS (CF.EXE) utility is used.
