Installing Windows NT 4.0 CardWiz Drivers

The following instructions tell how to install the 
CardWiz drivers for your computer.

Note:  If you have a printer connected to your computer,
you can print these instructions from Notepad by 
clicking on File on the menu bar and then click on Print.


Installing CardWiz Drivers in WIN NT 4.0 APM (1st time)
-------------------------------------------------------

 1. Place the Digital System CD in the CD drive.

 2. Click on the Start button located on the 
    Windows Taskbar. 

 3. Click on Run.

 4. Enter: D:\drivers\winnt\pccard\setup.exe and 
    click on OK. (D is the letter of the CD drive.)

 5. Accept all the installation defaults until you 
    reach the "Select Socket Services" window.

 6. In the "Select Socket Services" window:
    a. UN-Select SSINTEL.
    b. Select SSCL6832. 
    c. Click NEXT.

 7. Remove the Digital System CD from the CD drive.

 8. Restart the computer when asked.

 9. After the computer restarts you will need to add
    CardWiz to the Startup group. 

10. After adding CardWiz to the Startup group, restart
    the computer. The CardWiz application should start.

