
BIOS UPGRADE

The following files must be put on a bootable floppy (Format/s a:):

Platform.bin
Phlash.exe
31g2103a.rom  (Active Matrix - VP570-575)
31g2103b.rom  (DSTN screen - VP550-560)

1. Turn the system OFF by holding down the Fn key and pressing the
   power/suspend button until a beep is heard. 
2. Release the power button first and the system should shut off. 
3. Insert the floppy and press the power button. This will cold boot
   the system and bring up the floppy to A:
4. Type   PHLASH 31G2103x.ROM<CR>  (x=A or B for DSTN or Active Matrix)
5. An information screen will come up telling of the changes that are
   being made.
6. When done, a green screen will come up to tell you to press a 
   key to reboot...   
7. The system will ask to press F2 to continue, press F2 and then <CR>
   to accept the change to factory defaults
8. Press right arrow to Exit and Save Settings. 
   The system will restart and will have the new BIOS installed. 

