                  Microsoft Windows NT 4.0
           Installing the HP OmniBook Video Driver
                              
System Installation Requirements:

      HP OmniBook 800 with Microsoft Windows NT 4.0 installed.
      HP OmniBook 800 Windows NT 4.0 video driver.  This
      video driver can be obtained from the default HP Windows 95
      build in the following directory:
      C:\OMNIBOOK\DRIVERS\NT\VIDEO\NT40\.  The driver can also be
      found on the HP OmniBook 800 recovery CD-ROM.
     
Procedure:

     Boot the HP OmniBook 800 with Microsoft Windows NT 4.0
  and logon with administrative permissions.

     Double click on the ‘My Computer’ icon then double
  click on the Control Panel icon.  From within the Control
  Panel icon, double click on the Display icon.   Choose the
  Settings tab.  Select the option Display Type by clicking
  the mouse over it.  Under the Adapter Type choose
  the Change box.  Choose the Have Disk option at the
  Change Display windows.  Enter the location of the Windows
  NT 4.0 video driver for the HP OmniBook 800 then choose
  OK.

     The following adapter should be located by using the
  correct Windows NT 4.0 video driver:  NeoMagic MagicGraph
  128/Z/ZV.  Select this driver then choose OK to continue.

     Windows NT will prompt you that you are installing a
  third-party driver.  Choose Yes to install the driver and
  continue.  Windows NT will load the necessary files and then
  will prompt you that you need to reboot in order for the
  changes to take effect.  Choose OK to continue.  Close all
  of the video display windows and then select Yes to reboot
  the HP OmniBook 800 (make sure you remove the floppy disk
  from the floppy disk drive).


     Once rebooted the video driver will not appear to be in
  effect, Microsoft Windows NT will prompt you that a new
  graphics card has been installed.  Choose OK at this
  prompt and then change the Desktop Area to 800x600.  Click
  the Test button to test the adapter at this display
  setting.  Choose Yes to confirm that the test bitmap was
  successful.  Choose OK at the display properties window
  and Windows NT will set the screen resolution.  The Windows
  NT 4.0 video driver is now installed correctly.


