                Installing Microsoft Windows
                PCMCIA Card & Socket Services



System Installation Requirements

HP OmniBook 800 installed with Windows 3.1 or Windows for
  Workgroups

HP OmniBook 800 PCMCIA Drivers.  These drivers are located
  on the OmniBook hard disk in C:\OMNIBOOK\DRIVERS\WFW\PCMCIA.
  These drivers are also located on the HP OmniBook Recovery CD 
  in the \OmniBook\DRIVERS\WFW\PCMCIA directory.
Note: If you are backing up these files to floppy disk, you
     will need two floppy disks.




Procedures

1.From the DOS prompt or Windows File Manager create a
  directory called C:\CARDWIZ.

2.Copy the PCMCIA Drivers from
  C:\OMNIBOOK\DRIVERS\WFW\PCMCIA or from your backup on
  floppy disk.

3.   Enter the following lines into your CONFIG.SYS file in
  the order shown. (The REM’ed lines need not be entered. They
  are simply for explanation of the driver.)


REM -- OmniBook Socket Services driver required for card slot support
devicehigh=C:\CARDWIZ\SS365LP.EXE

REM -- Card Services driver required for card slot support.
devicehigh=C:\CARDWIZ\CS.EXE /POLL:1

REM -- Card Services APM support required for card slot support
install=C:\CARDWIZ\CS_APM.EXE

REM -- Initial resource allocator required for card slot support
devicehigh=C:\CARDWIZ\CSALLOC.EXE

REM -- ATA card driver required for ATA cards
devicehigh=C:\CARDWIZ\ATADRV.EXE /S:2

REM -- Driver required for RAM cards
devicehigh=C:\CARDWIZ\MTSRAM.EXE

REM -- Memory card driver required for all memory cards
devicehigh=C:\CARDWIZ\MTDDRV.EXE

REM -- Card identification driver required for cards other than memory cards
devicehigh=C:\CARDWIZ\CARDID.EXE


Add the following lines to the [386Enh] section of the
SYSTEM.INI file.  (The simplest method of accomplishing this is to cut and
paste from the readme.txt file located in the c:\omnibook\drivers\wfw\pcmcia
directory.)

COM2Base=2F8
COM2Irq=3
COM1Base=3F8
COM1Irq=4
device=C:\CARDWIZ\SSVRDD.386
device=C:\CARDWIZ\SSVCD311.386
device=C:\CARDWIZ\PCCARD.386
EmmExclude=DE00-DFFF
....and after the "FileSysChange=off"
COM3Irq=5
COM3Base=3E8
COM4Irq=9
COM4Base=2E8
---and change "device=*vcd" to ";device=*vcd"

Add the following file to the c:\windows\system directory

CTL3DV2.DLL
(This file is contained in the c:\omnibook\drivers\wfw\pcmcia\windows\system
directory.)



Maximizing memory for PC Cards
1.   In the default config.sys there are two emm386 lines.
  The defaults are as follows:

device=c:\dos\emm386.exe noems x=c000-cbff i=ca00-cfff x=d000-d1ff i=d200-e7ff x=e800-efff.  
(This allots 8K of memory for PC Card support. Add the REM statement to the
beginning of this line to allot 32K of memory for PC Card support.)

REM device=c:\dos\emm386.exe noems x=c000-cbff i=ca00-cfff x=d000-d7ff i=d800-e7ff x=e800-efff.  
(This allots 32K of memory for PC Card support. Remove the REM to increase the
memory to 32K)

