                    Installing Windows 95
                        SCSI Drivers
                              
                              
                              
                              
  
  Requirements
  
HP OmniBook 800 with retail Windows 95 installed.
HP OmniBook Recovery CD and CDROM drive.
  
  Procedure
  
1.   Connect the CDROM drive to the OmniBook 800 and insert the OmniBook
     Recovery CD.
2.   Copy the SCSI.INF file from \OMNIBOOK\DRIVERS\WIN95\SCSI on the Recovery
     CD to C:\WINDOWS\INF.  If this file is not copied it is possible that an
     incorrect SCSI driver may be loaded each time a new SCSI divice is
     attatched to the OmniBook 800.
3.   In Windows 95 open Control Panel and double-click on System.
4.   Go to the Device Manager tab.
5.   Double-click on SCSI controllers.
6.   Double-click on the entry under SCSI controllers (probably PCI NCR C810
     SCSI Host Adapter).
7.   Go to the Driver tab.
8.   Click on Change Driver....
9.   Click on Have Disk....
10.  Click on Browse....
11.  Select the CDROM drive and goto \OMNIBOOK\DRIVERS\WIN95\SCSI.
12.  Select the symc8xx.inf file and click on OK until the driver database is
     rebuilt.
13.  Click on Yes to restart your computer now.

