             Installing OS/2 Warp Sound Drivers
                              
                              
                              
                              

Requirements

HP OmniBook 800 with OS/2 Warp or Warp Connect Installed.
HP OmniBook 800 drivers for the Sound.  This driver is
located on the hard drive in the C:\OMNIBOOK\DRIVERS\OS2\SOUND subdirectory.
These files are available after finishing the selection of Windows 95 or
Windows for Workgroups.  This driver is also located on the HP OmniBook
Recovery CD.

Note:     You must install the Sound drivers from floppy
     disk.  To create an OS/2 OmniBook 800 Sound drivers disk do
     the following:  Copy the contents of C:\OMNIBOOK\DRIVERS\OS2\SOUND to the
     root directory of a blank floppy disk. Label the Diskette OS/2 OmniBook
     800 Sound Drivers Disk.

Procedure

1.   Open an OS/2 full screen or windowed session.
2.   Insert the OS/2 OmniBook 800 Sound Drivers Disk.
3.   Type A:EINSTALL 1887
4.   From the IBM Multimedia Presentation Manager/2 - Installation Windows,
     Select ES1887 WinOS2/Windows Audio if you installed OS/2 WinOS2 support
     and click Install.
5.   Click Yes to Change the CONFIG.SYS
6.   Click OK to Specify 1 AudioDrive ES1887.
7.   Set the following values and click OK.

	    I/O Address              220
	    DMA Channel              1
	    DMA 2                    5
	    Interrupt Level          5

8.    Set the following values for MIDI and click OK.

	    DMA Transfer Mode        4
	    MPU-401 I/O Address      330
	    MPU-401 Interrupt Level  7

9.   Set the following values for Windows Audio Options and
     click OK.

	    I/O Address              220
	    Interrupt Level          5
	    DMA Channel              1
	    DMA 2                    5

10.  Click OK to accept changes to the SYSTEM.INI.
11.  Click OK twice.
12.  Type Exit and remove the diskette from drive A.
13.  Shutdown by selecting the Shut down button on the
     LaunchPad, and press Ctrl-Alt-Delete to reboot when prompted.

