                Installing OS/2 Warp SCSI Drivers
                                
                                
                                
                                
If you are using the OmniBook Docking station use the following
procedure to install SCSI Support.  This procedure is not
necessary if you installed OS/2 Warp from a SCSI CD-ROM drive
because the SCSI drivers are already installed.

Requirements

HP OmniBook 800 with OS/2 Warp or Warp Connect Installed.
HP OmniBook 800drivers for the SCSI.  This driver is located
  on the hard drive in the C:\OMNIBOOK\DRIVERS\OS2\SCSI
  subdirectory.  These files are available after finishing the
  selection of Windows 95 or Windows for Workgroups.  This driver
  is also located on the HP OmniBook Recovery.

Note:     You must install these drivers from floppy disk.  Copy
     the contents of C:\OMNIBOOK\DRIVERS\OS2\SCSI to a blank floppy
     disk.

Procedure

1.   Insert the Floppy disk with the SCSI drivers in the A: drive.
2.   Open the System Setup icon in the OS/2 System and double-click on
     Device Driver Install.
3.   Change the Drive to A:\ if necessary and click Install.
4.   Select NCR SDMS ™ V3.0 OS/2 2.x ADD Driver, Copywright 1993
5.   Click OK
6.   Click Exit and click Yes to confirm.
7.   Click OK.
8.   Shutdown by selecting the Shut down button on the LaunchPad,
     and press Ctrl-Alt- Delete to reboot when prompted.

