Plug and Play Kit for MS-DOS, R1.45

The MS-DOS installation must be copied onto two floppy disks.

Copy the contents of the DISK1 directory onto the first
disk, and the contents of the DISK2 directory onto the second
disk.

You may now install the Plug and Play Kit for MS-DOS by
invoking a:\INSTALL.
