[BroadbandINSFormat]

;Version number of broadband INS definition
ScriptVersion=1.1

;4-byte hexadecimal CRC value (optional)
ValidationCode=1234

;Date of script generation
ScriptDate=15-Jan-2004

;The name of the service described in this INS file.
ServiceName=* ���-����� (�����.��), ������

[PhysicalLayer]

;Preferred modulation.
;0 = Auto selection with G.Handshake preferred - default setting
;1 = Auto selection with T1.413 preferred
;2 = G.Handshake only
;3 = T1.413 only
;4 = G.hs, G.dmt Only
;5 = G.hs, G.lite Only
XdslModulation=0

;Wiring Pair Selection
;0 = Automatic
;1 = Line Tip/Ring
;2 = Line A/A1
;3 = Aux Tip/Ring
;4 = Aux A/A1
AutoSenseWiringSelection=1

;Head end DSLAM provider as defined in Annex D, ANSI T1.413 - 1998
;0 = Do not specify the Head end DSLAM provider
AdslHeadEnd=0

;Head end DSLAM provider as defined in Annex D, ANSI T1.413 - 1998
;0 = Non-Specific
;1 = No Line Driver (BNA)
AdslHeadEndEnv=0

[ATMPVCs]
;max number of defined PVC's (0-16)
MaxPVC=1

;Aggregate upstream peak cell rate
;0 = 16Kbps
;1 = 32Kbps
;n = n*32Kbs
;255 = use line rate
DslUpstreamPcr=255

;PVC #1 VPI value (default value 0)
Pvc1Vpi=1

;PVC #1 VCI value
Pvc1Vci=50

[PVCEncapsulations]
;0 = PPP over ATM VCMUX          (RFC 2364) (PPPOA)
;1 = PPP over ATM LLC            (RFC 2364) (PPPOA)
;2 = Bridged IP over ATM LLCSNAP (RFC 1483)
;3 = Routed IP over ATM LLCSNAP  (RFC 1483)
;4 = Bridged IP over ATM VCMUX   (RFC 1483)
;6 = Classical IP over ATM       (RFC 1577) (IPOA)
;7 = Native ATM
;8 = RFC_PPPOE_VCMUX		      (RFC 2516) PPP over Ethernet VCMUX
;9 = RFC_PPPOE_LLC		    	  (RFC 2516) PPP over Ethernet LLCSNAP 
;-1 = Proprietary
Pvc1Encapsulation=9

[NetworkLayer]
;This section is only used for RFC 1483 encapsulations.
;PPPOA and IPOA handle this automatically

;0 = use static IP addressing
;1 = use DHCP or PPP (according to Encapsulation Type)
Pvc1AddressAssignment=1

Pvc1StaticIp=0.0.0.0

Pvc1StaticIpMask=0.0.0.0

;Router address, to be used as default gateway
;Not Applicable if DefaultGwAlgorithm=1

DefaultGateway=0.0.0.0

;Wizard will calculate the Default Gateway address based on the IP address and IP Mask
;0 = Disabled
;1-255 = OEM defined algorithms
DefaultGwAlgorithm=0

;Address of DNS server for static IP
DnsServer=0.0.0.0

AltDnsServer=0.0.0.0

;User Name
UserName=""

;Host Name
HostName=""

;Domain Name
DomainName=""

;Enable / Disable of DHCP Proxy function
;0 = Do not answer first DHCP request if the DSL is not in ShowTime
;1 = Answer first DHCP request if the DSL is not in ShowTime
DhcpProxy=0

;Enable / Disable of auto DHCP release/renew (Win9x only)
;0 = Do not request DHCP lease (IP address) to be renewed at showtime
;1 = Request DHCP lease (IP address) to be renewed at showtime
DhcpRenewRequest=0

