[boot]
386grabber=vga.3gr
oemfonts.fon=vgaoem.fon
286grabber=vgacolor.2gr
fixedfon.fon=vgafix.fon
fonts.fon=vgasys.fon
display.drv=vga.drv
shell=progman.exe
mouse.drv=mouse.drv
network.drv=
language.dll=
sound.drv=mmsound.drv
keyboard.drv=keyboard.drv
system.drv=system.drv
drivers=mmsystem.dll power.drv msmixmgr.dll
SCRNSAVE.EXE=(None)
subtype=
type=4
keyboard.dll=
oemansi.bin=
;;The following line was changed by the FaxWorks install=
;comm.drv=comm.drv
COMM.DRV=fx-comm.drv

[boot.description]
aspect=100,96,96
display.drv=VGA
keyboard.typ=Enhanced 101 or 102 key US and Non US keyboards
mouse.drv=Microsoft, or IBM PS/2
network.drv=No Network Installed
language.dll=English (American)
system.drv=MS-DOS System with APM
codepage=437
woafont.fon=English (437)

[standard]

[NonWindowsApp]
localtsrs=dosedit,ced

[mci]
WaveAudio=mciwave.drv
Sequencer=mciseq.drv
AVIVideo=mciavi.drv
CDAudio=mcicda.drv

[drivers]
timer=timer.drv
midimapper=midimap.drv
WAVEMAPPER=MSACM.DRV
MSACM.IMAADPCM=IMAADPCM.ACM
MSACM.MSADPCM=MSADPCM.ACM
MSACM.AF10=AF10.ACM
VIDC.CVID=iccvid.drv
VIDC.MSVC=msvidc.drv
VIDC.IV31=ir32.dll
VIDC.IV32=ir32.dll
VIDC.MRLE=MSRLE.drv
VIDC.RT21=indeov.drv
VIDC.YVU9=indeov.drv
WAVE=es688win.drv
MIDI=es688win.drv
AUX=es688win.drv
mixer=es688win.drv
MIDI1=audmpio.drv

[DISPLAY]
CursorAnimation=1
HARDWARE-CURSOR=0
MONITOR-TYPE=NI
COLOR-FORMAT=8
SCREEN-SIZE=640X480
BIG-CURSOR=1

[display driver]
DisplayOrientation=0

[mciseq.drv]
disablewarning=true

[386Enh]
display=*vddvga
EGA80WOA.FON=EGA80WOA.FON
EGA40WOA.FON=EGA40WOA.FON
CGA80WOA.FON=CGA80WOA.FON
CGA40WOA.FON=CGA40WOA.FON
device=C:\TRANXIT\pcomm.386
device=dva.386
device=IBMIR.386
;======== PC DOS 6 Setup Modification - Begin ========
device=C:\DOS\SYSTEM\CPBVXD.386
;======== PC DOS 6 Setup Modification - End ========
32BitDiskAccess=OFF
device=*int13
device=*wdctrl
mouse=*vmd
network=*dosnet,*vnetbios
device=vpowerd.386
ebios=*ebios
woafont=dosapp.fon
keyboard=*vkd
device=vtdapi.386
device=*vpicd
device=vtda.386
device=*reboot
device=*vdmad
device=*vsd
device=*v86mmgr
device=*pageswap
device=*dosmgr
device=*vmpoll
device=*wshell
device=*BLOCKDEV
device=*PAGEFILE
device=*vfd
device=*parity
device=*biosxlat
device=*vcd
device=*vmcpd
device=*combuff
device=*cdpscsi
local=CON
FileSysChange=off
PagingFile=C:\WINDOWS\WIN386.SWP
MaxPagingFileSize=12288
DMABUFFERSIZE=018
DEVICE=C:\DOS\MONOUMB.386
UniqueDOSPSP=true
DEVICE=C:\FOLLOWFX\VFFWD.386
;device=IBMVCD.386
; If COM_BDA_VIRTUAL=true, virtualize BIOS Data area 40:0 -- 40:8
COM_BDA_VIRTUAL=FALSE
COMVerifyBase=false
;COM1Base=3F8
;COM2Base=2F8
;COM3Base=3E8
;COM4Base=2E8
;COM1IRQ=4
;COM2IRQ=3
;COM3IRQ=4
;COM4IRQ=3
EMMInclude=B000-B7FF
EMMExclude=CC00-CFFF
device=es688win.386
MinTimeslice=20
WinTimeslice=100,50
WinExclusive=0
Com1AutoAssign=2
Com2AutoAssign=2

[auddrive.drv]
AudioDrive=ES688
Synth=OPL3
portchoices=220,,,
irqchoices=2,5,7,10
dmachoices=0,1,3
port=220
int=7
dmachannel=1
AutoConfig=yes
VerifyInt=yes
VerifyDMA=no
Mute=No
VolumeMutes=4
VolumeMixer=31
WaveInMixer=2
VoiceMixer=2
WaveInMonitor=No
VoiceMonitor=No
VolumeMaster=32768
VolumeMasterR=32768
VolumeWave=32768
VolumeWaveR=32768
VolumeSynth=32768
VolumeSynthR=32768
VolumeLine=32768
VolumeLineR=32768
VolumeMic=32768
VolumeMicR=32768
VolumeCD=32768
VolumeCDR=32768
WaveInMic=32768
WaveInMicR=32768
WaveInLine=32768
WaveInLineR=32768
WaveInCD=32768
WaveInCDR=32768
WaveInSynth=32768
WaveInSynthR=32768
WaveInMaster=32768
WaveInMasterR=32768
VoiceMic=32768
VoiceMicR=32768
VoiceLine=32768
VoiceLineR=32768
VoiceCD=32768
VoiceCDR=32768
VoiceMaster=32768
VoiceMasterR=32768
