    Release Notes for TranXit(TM) Version 1.0
    Copyright (C) Puma Technology, 1994
  
    This document contains information that supplements the 
    user's guide, on-line help, and accompanying software.
  
    CONTENTS
  
      I.  The TranXit Setup Program
          1.  Documentation Changes
          2.  Modifications to Your SYSTEM.INI File
     II.  Installing TranXit with Remote Install
    III.  Trouble Shooting
          1.  Parallel Cable Connection
          2.  Serial Cable Connection
          3.  Infrared Connection
     IV.  Other Issues
          1.  Clipboard Transfer
  
    _________________________________________________________________
  
    I. The TranXit Setup Program
  
    1. Documentation Changes
  
    The Configure Connection Setting dialog box is not available
    during the installation procedure.  All connection configuration
    must be done while running TranXit.  Select "Setup" from the 
    Connection menu to configure the connection options you will be using.
    Refer to the section "The Connection Setup Dialog Box" in the user's 
    guide or on-line help for further assistance.

    2. Modifications to Your SYSTEM.INI File

    The following changes will be made to your system if you install
    TranXit using all the default conditions during the Setup
    program.

        a.  Additions to SYSTEM.INI in the [386Enh] section:

            device=C:\TRANXIT\PCOMM.386

        b.  Addition to PROGMAN.INI in the [Groups] section:

            Groupn=C:\WINDOWSDIR\TRANXIT.GRP
    

    Note: If you install TranXit on your computer more than once, previous
          instances of PCOMM.386 will be commented out of SYSTEM.INI.  Only
          the most recent installation directory will be reflected in 
          SYSTEM.INI.

    _________________________________________________________________


    II.  Installing TranXit with Remote Install

    To install TranXit on a remote computer that does not have
    a floppy drive, you can use the Remote Install option from
    the Options menu.  The Remote Install menu item may be greyed
    for one of the following reasons:

        a.  You did not select the Remote Install option during
            setup.  You must re-install TranXit and select this
            option.  This will build the components necessary to
            use remote install.

            If you did select the Remote Install option, you will have a
            directory called C:\TRANXIT\RI (if you installed it to C:\TRANXIT), 
            make sure TranXit's SETUP.EXE is in C:\TRANXIT\RI.

        b.  A connection has been made with the remote computer (the New Window 
            button will be available).  In this case, TranXit must be closed 
            on the remote computer.

    When using the Remote Install feature, the remote computer must
    not be running SHARE.EXE.  This may cause transmission failure
    during the install process.  The remote computer must also be
    operating from the DOS prompt.  If you are running Windows(TM), you
    must exit Windows.  A Windows DOS box cannot be used.

    If you experience transmission problems during remote install, the 
    transfer baud rate may be adjusted in TRANXIT.INI. In the [Advanced]
    section modify the following line:

        RemoteInstallBaud=57600

    Valid baud rates are: 2400, 4800, 9600, 19200, 38400, 57600, 115200. Try
    using a slower baud rate when you encounter transmission errors.
    
    _________________________________________________________________


    III.  Trouble Shooting

    1.  Parallel Cable Connection

    If you have configured TranXit to communicate over a parallel cable, 
    and you do not get a New Window button (this is enabled when a 
    connection is established), check the following:

        a.  Make sure the that both the local and remote computers have 
            selected a parallel cable connection in Connection/Setup.

        b.  If the connection is intermittent, make sure the cable is securely
            fastened to the parallel port.

        c.  Verify that there are no conflicts with other hardware devices such
            as sound cards or network adapters.  The default IRQ setting for many 
            sound cards is IRQ 7.  This is also the IRQ that is used for 
            communication over LPT1.  Consult your adapter documentation for 
            changing the default IRQ on these boards.

        d.  If you have selected LPT2, the default IRQ on the I/O communication
            adapter may not be set to IRQ 5.  Try selecting IRQ 7 from the
            Change Connection Settings in the Connection Setup dialog box, or
            consult the I/O adapter documentation for changing the IRQ for
            LPT2 to IRQ 5.  If you have a bus mouse, it may be set to IRQ 5.
            If the mouse freezes after configuring TranXit for LPT2, there is
            an IRQ conflict. Consult your mouse hardware documentation for 
            changing the default IRQ.

        e.  If your computer has more than one parallel port, make sure the 
            cable is attached to the correct port.  Don't laugh, this is 
            a common oversight.

        f.  When connecting to a slower computer, Pentium to 386, you may need
            to start TranXit on the slower computer first.

        g.  The parallel cable must be LapLink(R) compatible and have male 
            DB-25 connectors at both ends. If you are not using a LapLink 
            parallel cable, make sure the cable is configured with the 
            following pin connections:
  
                25 Pin             25 Pin 
                -------            -------
                Pin 2     <--->    Pin 15 
                Pin 3     <--->    Pin 13 
                Pin 4     <--->    Pin 12 
                Pin 5     <--->    Pin 10 
                Pin 6     <--->    Pin 11 
                Pin 15    <--->    Pin 2 
                Pin 13    <--->    Pin 3 
                Pin 12    <--->    Pin 4 
                Pin 10    <--->    Pin 5 
                Pin 11    <--->    Pin 6 
                Pin 25    <--->    Pin 25 (Ground-Ground) 
  

    2.  Serial Cable Connection

    If you have configured TranXit to communicate over a serial cable, and 
    you do not get a New Window button (this is enabled when a connection 
    is established), check the following:

        a.  Make sure the that both the local and remote computers have selected
            the proper serial cable connection in Connection/Setup. The baud 
            rate setting must be the same on both systems.

        b.  If the connection is intermittent, make sure the cable is securely
            fastened to the serial port.

        c.  Verify that there are no conflicts with other serial devices.  
            Conflicts will occur when serial devices are sharing interrupts 
            (IRQ's).  In a standard configuration (if you computer is 
            equipped with 4 serial ports), COM1 and COM3 will share IRQ 4, 
            and COM2 and COM4 share IRQ 3. If your mouse is on COM1 and you're 
            trying to connect TranXit over COM3, there will be an IRQ conflict.  
            In this case, your mouse may freeze and you will not make a 
            connection with the remote computer.

        d.  If your computer has more than one serial port, make sure the cable
            is attached to the correct port.  

        e.  When connecting to a slower computer, Pentium to 386, you may need
            to start TranXit on the slower computer first.

        f.  The serial cable must be LapLink compatible, and can be either a 
            9-pin or a 25-pin female connector on both ends. If you are not 
            using a LapLink serial cable, make sure the cable is configured 
            with the following pin connections:
  
                9 Pin           25 Pin              25 Pin          9 Pin 
                ------          -------             -------         ------
                Pin 5           Pin 7     <--->     Pin 7           Pin 5 
                (Ground-Ground) 
                Pin 3           Pin 2     <--->     Pin 3           Pin 2 
                (Transmit-Receive) 
                Pin 7           Pin 4     <--->     Pin 5           Pin 8 
                (RTS - CTS) 
                Pin 6           Pin 6     <--->     Pin 20          Pin 4 
                (DSR - DTR) 
                Pin 2           Pin 3     <--->     Pin 2           Pin 3 
                (Receive-Transmit) 
                Pin 8           Pin 5     <--->     Pin 4           Pin 7 
                (CTS - RTS) 
                Pin 4           Pin 20    <--->     Pin 6           Pin 6 
                (DTR - DSR) 


    3.  Infrared Connection

    If you have configured TranXit to communicate with an infrared 
    connection, and you do not get a New Window button (this is enabled when 
    a connection is established), check the following:

        a.  Make sure the that both the local and remote computers have selected 
            the proper infrared connection in Connection/Setup. The baud rate 
            setting must be the same on both systems.

        b.  There must be no obstacles blocking the line of sight between
            the infrared adapters.
    
        c.  The adapters should be placed away from any light or 
            electromagnetic source. These can include such items
            as wireless headphones, halogen desk lamps, and even
            computer monitors.

        d.  When connecting to a slower computer, Pentium to 386, you may need
            to start TranXit on the slower computer first.

    _________________________________________________________________


    IV.  Other Issues

    1.  Clipboard Transfer

    When transferring graphics images from one computer's clipboard to 
    another, keep in mind that one of the clipboard formats 
    used is the DDB (Device Dependent Bitmap).  As the name implies this 
    format is dependent on the type of video display being used. 
    Problems may develop when images are transferred from a 16-color 
    display to a 256-color display or vice-versa.  A warning message 
    will appear when the format may not transfer correctly from one 
    computer's clipboard to another.

    _________________________________________________________________


    TranXit is a trademark of Puma Technology, Inc.
    All other product names are trademarks or registered trademarks of 
    their respective holders.

