Virtual Floppy Image Converter Plugin.txt       (C)Copyright 1999-2001 RED

[[ IMPORT Plug-in ]]
  It is Plug-in to take a disk image in the inside of VFIC. 

 [inbkd.vin]
  Plug-in of the image that it is formated with BKDSK of Mr./Ms. nop & TONBO. 
   <Complying with the comment file> 
   <Option>
     - Use Ext. to export filename
       When it is checked, the extension of the input image is reflected
       by a export file name. 
  
 [ind88.vin]
  Plug-in of the image that it is formated with MAKE_HD.EXE of Mr. BURU-. 
  The copyright of this plug-in is reserved by Studio Milmake. 
  
 [indbs.vin]
  Plug-in of the image that it is formated with Enhanced D.B.S. series 
  of Mr. H.Fujino. 
   <Complying with the comment file> 
  
 [indcu.vin]
  Plug-in of the image that it is formated with BCU of Mr./Ms. Camel
  and DCP of Mr./Ms. N.Taniguchi.
  
 [indfc.vin]
  Plug-in of the image that it is formated with DFCNV of Mr./Ms. M.Osanai. 
   <Complying with the comment file> 
   <Note>
    The extension of the input image is reflected by a export file name. 
    The image of the compression type can't be converted.
  
 [indim.vin]
  Plug-in of the image that it is formated with DIFC.X of Mr./Ms. GUN.
   <Complying with the comment file> 
  
 [indip.vin]
  Plug-in of the image that it is formated with DIP of Mr./Ms. K.Mituhasi. 
   <Complying with the comment file> 
  
 [infdd.vin]
  Plug-in of the image that it is formated with Virtual of GADGET. 
   <Complying with the comment file> 
  
 [infdi.vin]
  Plug-in of the image that it is formated with FDI(Anex86) of Mr./Ms. A.N. 
  
 [infim.vin]
  Plug-in of the image that it is formated with FIM of WESTSIDE Ltd. 
   <Complying with the comment file> 
  
 [infim.vin]
  Plug-in of the image that it is formated with FIX of WESTSIDE Ltd. 
   <Complying with the comment file> 
  
 [inmhl.vin]
  Plug-in of the image that it is formated with MAHALITO of Mr./Ms. K.Oikawa. 
  
 [innfd.vin]
  Plug-in of the image that it is formated with NFD(T98-Next)
   of Project T98-Next.
  
 [inprs.vin]
  Plug-in of the image that it is formated with Press1 of Presentech. 
   <Complying with the comment file> 
  
 [inrfd.vin]
  Plug-in to read directly from FD.
   <Note>
    Be sure to give FD which reads it write protection.
    A setup of a DISK OPEN button is necessary with VFIC. 
    A 3mode drive is necessary for reading of FD of 1.23M. 
  
 [inslf.vin]
  Plug-in of the image that it is formated with SLF of Mr./Ms. H.Date. 
   <Complying with the comment file> 
  
 [instd.vin]
  Plug-in of the image that it is formated with STDFILE of TPC ACCESS. 
  
 [invfd.vin]
  Plug-in of the image that it is formated with ERCACHE of Mr. Error15. 
   <Complying with the comment file> 
  
 [invfl.vin]
  Plug-in of the image that it is formated with VFL of Dr.Chin. 
   <Complying with the comment file> 
  
  
  
[[ EXPORT Plug-in ]]
  It is Plug-in which the image take in the inside of VFIC is exported. 
  
 [exbkd.vex]
  The image which can be used with BKDSK of Mr./Ms. nop & TONBO is exported.
  
 [exd88.vex]
  The image which can be used with P88SR of Mr.BURU- & various PC-Emulators
  is exported.
  The copyright of this plug-in is reserved by Studio Milmake. 
  
 [exdcu.vex]
  The image which can be used with DCU of Mr./Ms. Camel
  or DCP of Mr./Ms. N.Taniguchi is exported.
   <Option>
    DCU/DCP You can be set up if it is exported with which format. 
  
 [exdim.vex]
  The image which can be used with DIFC.X of Mr./Ms. GUN is exported.
  
 [exfdd.vex]
  The image which can be used with Virtual of GADGET is exported.
  
 [exfdi.vex]
  The image which can be used with Anex86 of Mr./Ms. A.N. is exported.
   <Option>
    - Execute Dispell to cancel Epson protect
    Dispell is started automatically after a convert is finished. 
    Put Dispell.exe in the same folder with Plug-in to use it. 
  
 [exfil.vex]
  A DOS file in the image is extracted and outputted. 
  
 [exmhl.vex]
  The image which can be used with MAHALITO of Mr./Ms. K.Oikawa is exported.
  
 [exnfd.vex]
  The image which can be used with T98-Next of Project T98-Next is exported.
  
 [extfd.vex]
  The image which can be used with T98 of Mr. YUKI is exported.
   <Option>
    - Execute Dispell to cancel Epson protect
    Dispell is started automatically after a convert is finished. 
    Put Dispell.exe in the same folder with Plug-in to use it. 
  
 [exvfd.vex]
  The image which can be used with ERCACHE of Mr. Error15 is exported.
  
 [exxdf.vex]
  The image which can be used with EX68 of Mr. yamama is exported.
  
  

[[ Caution ]]
  These Plug-ins are being made by the attached materials and
  the individual analysis.
  As for the copyright person of each tool, a developer, the sale cause,
  there is no one related to all in these Plug-ins. 
  Prevent the inquiry about Plug-in from your never doing it. 
  
  It is based on VFIC about the reproduction, the distribution. 
  Refer to readme.txt. 

(C)Copyright 1999-2001 RED
