
          +---------------------------------------------------------+
          |                                                         |
          | PREPARATION FOR VAX/VMS UPGRADE FROM VMS 4.6 TO VMS 4.7 |
          |                                                         |
          +---------------------------------------------------------+



testvax @ s1-ankh [wy1akh] $ cat start
sudo /local/bin/vax8600 testvax.ini
testvax @ s1-ankh [wy1akh] $ ./start

VAX 8600 simulator V4.0-0 Current        git commit id: 114a29bc
Setting CPU and memory
testvax.ini-29> attach rq0 vaxvmsos.ra82
RQ0: creating new file
testvax.ini-32> attach rq1 user_1.ra82
RQ1: creating new file
testvax.ini-35> attach rq2 software_1.ra82
RQ2: creating new file
RQ3: 'vaxvms047a.rd54' Contains ODS2 File system
RQ3: Volume Name: VAXVMS047A   Format: DECFILE11B   Sectors In Volume: 311200
libpcap version 1.8.1 -- Apple version 67.60.2
Eth: opened OS device en0
sim> show config
VAX 8650 simulator configuration

CPU     idle disabled, model=VAX 8650
        256MB, HALT to SIMH
TLB     2 units
  TLB0  8192W
  TLB1  8192W
ABUS
SBIA
UBA     nexus=3, address=20006000, autoconfiguration enabled
MBA0    disabled
MBA1    disabled
TODR
        12B
TMR
TTI     4 units
  TTI0  8b
  TTI1  8b
  TTI2  8b
  TTI3  8b
TTO     4 units
  TTO0  8b
  TTO1  8b
  TTO2  8b
  TTO3  8b
CS
        5242KW, not attached, write enabled
TC      disabled
TDC     disabled
DZ      address=2013E040-2013E05F*, vector=C0-DC*, BR5, lines=32
        not attached, 8b
VH      disabled
CR      disabled
LPT     address=2013FF4C-2013FF4F, vector=80, BR4
        not attached
RP      disabled
RL      disabled
HK      disabled
RK      disabled
RQ      address=2013F468-2013F46B, no vector, BR5, UDA50, 4 units
  RQ0   622MB, attached to vaxvmsos.ra82, write enabled
        RA82, autosize, SIMH format
  RQ1   622MB, attached to user_1.ra82, write enabled
        RA82, autosize, SIMH format
  RQ2   622MB, attached to software_1.ra82, write enabled
        RA82, autosize, SIMH format
  RQ3   159MB, attached to vaxvms047a.rd54, write enabled
        RD54, autosize, SIMH format
RQB     disabled
RQC     disabled
RQD     disabled
RY      disabled
TU      disabled
TS      address=2013F550-2013F553, vector=94, BR5
        not attached, write enabled, SIMH format
        unlimited capacity
TQ      TU81 (180MB), address=2013F940-2013F943, no vector, BR5, 4 units
  TQ0   not attached, write enabled, SIMH format
        capacity=188MB
  TQ1   not attached, write enabled, SIMH format
        capacity=188MB
  TQ2   not attached, write enabled, SIMH format
        capacity=188MB
  TQ3   not attached, write enabled, SIMH format
        capacity=188MB
XU      address=2013F948-2013F94F, vector=50, BR5, MAC=AA:00:04:00:CC:1C
        type=DELUA, throttle=disabled
        attached to en0
XUB     disabled
DMC     disabled

          +--------------------------------------------------+
          |                                                  |
          | 1) INSTALL VAX/VMS 4.6 AS THE BASE SYSTEM        |
          |                                                  |
          +--------------------------------------------------+



sim> boot rq3
Loading boot code from internal vmb.exe


   VAX/VMS Version V4.6  6-Jul-1987 17:00


%BACKUP-I-IDENT, Stand-alone BACKUP V4.6; the date is 20-FEB-2019 07:09:56.41
$ BACKUP/VERIFY DUA3:REQUIRED/SAVE DUA0:
%BACKUP-I-STARTVERIFY, starting verification pass
%BACKUP-I-PROCDONE, Operation completed.  Processing finished at 20-FEB-2019 07:12:22.93
If you do not want to perform another standalone BACKUP operation,
use the console to halt the system.

If you do want to perform another standalone BACKUP operation, 
ensure the standalone application volume is online and ready.
Enter "YES" to continue: <CTRL-E PRESSED TO RETURN TO SIMULATOR>
Simulation stopped, PC: 80008B1F (BRB 80008B1F)
sim> boot rq0
Loading boot code from internal vmb.exe


   VAX/VMS Version  KG  15-Jun-1987 10:00


%%%%%%%%%%%  OPCOM  20-FEB-1987 07:15:08.90  %%%%%%%%%%%
Logfile has been initialized by operator _OPA0:
Logfile is SYS$SYSROOT:[SYSMGR]OPERATOR.LOG;1

Please enter the date and time (DD-MMM-YYYY HH:MM): 20-FEB-2019 07:15

Enter drive holding distribution kit (DDCU): du\ud\DUA3
%MOUNT-I-MOUNTED, VAXVMS047A   mounted on _DUA3:
If this node is part of a cluster, you may want to set up
your system disk to run multiple cluster nodes from a single disk.

Do you want to know more about cluster system disks [N]? y

In a cluster, you can run multiple systems with up to 14 nodes sharing
all files except PAGEFILE.SYS, SWAPFILE.SYS, SYSDUMP.DMP and VAXVMSSYS.PAR.

Do you want to generate a cluster common system disk [N]? Y

In order to successfully boot the system, you must provide a nonzero value
for the SYSGEN parameter SCSSYSTEMID and a nonblank value for the SYSGEN
parameter SCSNODE.  See the Guide to VAXclusters for information on
setting up other SYSGEN parameters after the system is installed. 

Enter this node's SCSSYSTEMID value: 8188
Enter this node's SCSNODE name: TSTVAX

Restoring library saveset.
%BACKUP-I-STARTVERIFY, starting verification pass

Restoring optional saveset.
%BACKUP-I-STARTVERIFY, starting verification pass

Creating [V4COMMON] directory tree.
%DCL-I-SUPERSEDE, previous value of SYS$COMMON has been superseded
%DCL-I-SUPERSEDE, previous value of SYS$SYSROOT has been superseded
%DCL-I-SUPERSEDE, previous value of SYS$COMMON has been superseded

Now we will ask you for new passwords for the following accounts:
        SYSTEM, SYSTEST, FIELD


Enter new password for account SYSTEM: 
Re-enter the password for account SYSTEM for verification: 

%UAF-I-MDFYMSG, user record(s) updated

Enter new password for account SYSTEST: 
Re-enter the password for account SYSTEST for verification: 

%UAF-I-MDFYMSG, user record(s) updated

Enter new password for account FIELD: 
Re-enter the password for account FIELD for verification: 

%UAF-I-MDFYMSG, user record(s) updated

Creating RIGHTS database file, SYS$SYSTEM:RIGHTSLIST.DAT
Ignore any "%SYSTEM-F-DUPIDENT, duplicate identifier" errors.
%UAF-I-RDBCREMSG, RIGHTSLIST.DAT created
%UAF-I-RDBADDMSGU, identifier DEFAULT value: [000200,000200] added to RIGHTSLIST.DAT
%UAF-I-RDBADDMSGU, identifier FIELD value: [000001,000010] added to RIGHTSLIST.DAT
%UAF-I-RDBADDMSGU, identifier SYSTEM value: [000001,000004] added to RIGHTSLIST.DAT
%UAF-I-RDBADDMSGU, identifier SYSTEST value: [000001,000007] added to RIGHTSLIST.DAT
%UAF-E-RDBADDERRU, unable to add SYSTEST_CLIG value: [000001,000007] to RIGHTSLIST.DAT
-SYSTEM-F-DUPIDENT, duplicate identifier
%UAF-I-NOMODS, no modifications made to system authorization file
%UAF-I-RDBDONEMSG, rights database modified

AUTOGEN computes the SYSGEN parameters for your configuration
and then reboots the system with the new parameters.

After the reboot, you may want to do one or more of the following tasks
(consult the Guide to VAX/VMS System Manager's Reference Manual for
detailed information): 

- Delete SYS$SYSTEM:STARTUP.INS

- DECOMPRESS THE SYSTEM LIBRARIES - For space considerations, many of the system
libraries are shipped in a data compressed format.  If you have enough disk
space, you may decompress them for faster access. Use SYS$UPDATE:LIBDECOMP.COM
to data expand the libraries.  If you choose not to decompress these libraries
there will be a negative impact on the performance of the HELP and LINK
commands.

- APPLY THE MANDATORY UPDATE - The mandatory update for VMS V4.6 must be applied
as soon as possible.   You will be unable to install any optional software 
products until this update has been applied.


Running AUTOGEN -- Please wait.

%AUTOGEN-I-BEGIN, GETDATA phase is beginning.
%AUTOGEN-I-NEWFILE, A new version of SYS$SYSTEM:PARAMS.DAT has been created.
        You may wish to purge this file.
%AUTOGEN-I-END, GETDATA phase has successfully completed.
%AUTOGEN-I-BEGIN, GENPARAMS phase is beginning.
%AUTOGEN-I-NEWFILE, A new version of SYS$MANAGER:VMSIMAGES.DAT has been created.
        You may wish to purge this file.
%AUTOGEN-I-NEWFILE, A new version of SYS$SYSTEM:SETPARAMS.DAT has been created.
        You may wish to purge this file.
%AUTOGEN-I-END, GENPARAMS phase has successfully completed.
%AUTOGEN-I-BEGIN, GENFILES phase is beginning.

%AUTOGEN-I-CREATE, DISK$VAXVMSRL4:[SYS0.SYSEXE]PAGEFILE.SYS
        will be modified to hold 529300 blocks.
%SYSGEN-I-EXTENDED, DISK$VAXVMSRL4:[SYS0.SYSEXE]PAGEFILE.SYS;1 extended


%AUTOGEN-I-CREATE, DISK$VAXVMSRL4:[SYS0.SYSEXE]SWAPFILE.SYS
        will be modified to hold 90000 blocks.
%SYSGEN-I-EXTENDED, DISK$VAXVMSRL4:[SYS0.SYSEXE]SWAPFILE.SYS;1 extended


%AUTOGEN-W-DSKSPC, The system disk would be over 95% full
        if the dump file were created with 524292 blocks.
%AUTOGEN-I-NOCHANGE, No dump file modifications will be made.

%AUTOGEN-I-END, GENFILES phase has successfully completed.
%AUTOGEN-I-BEGIN, SETPARAMS phase is beginning.
%SYSGEN-W-SETMAX, value set to maximum for parameter WSMAX
%AUTOGEN-I-END, SETPARAMS phase has successfully completed.
%AUTOGEN-I-BEGIN, REBOOT phase is beginning.

The system is shutting down to allow the system to boot with the
generated site-specific parameters and installed images.

The system will automatically reboot after the shutdown and the
upgrade will be complete.



        SHUTDOWN -- Perform an Orderly System Shutdown


%SHUTDOWN-I-BOOTCHECK, Performing reboot consistency check...
%SHUTDOWN-I-CHECKOK, Basic reboot consistency check completed

%SHUTDOWN-I-OPERATOR, This terminal is now an operator's console.
%SHUTDOWN-I-DISLOGINS, Interactive logins will now be disabled.
%SET-I-INTSET, login interactive limit = 0, current interactive value = 0
%SHUTDOWN-I-STOPQUEMAN, The queue manager will now be stopped.
%JBC-E-JOBQUEDIS, system job queue manager is not running

SHUTDOWN message from user SYSTEM at  Batch   07:18:05
The system will shut down in 0 minutes; back up soon.  Please log off.
Reboot system with AUTOGENerated parameters


%SHUTDOWN-I-SITESHUT, The site-specific shutdown procedure will now be invoked.
%SHUTDOWN-I-STOPUSER, All user processes will now be stopped.
%SHUTDOWN-I-REMOVE, All installed images will now be removed.
Loading boot code from internal vmb.exenow be dismounted.
Rebooting...


   VAX/VMS Version  KG  15-Jun-1987 10:00


%%%%%%%%%%%  OPCOM  20-FEB-2019 07:19:02.07  %%%%%%%%%%%
Logfile has been initialized by operator _TSTVAX$OPA0:
Logfile is SYS$SYSROOT:[SYSMGR]OPERATOR.LOG;1

%UAF-I-RDBADDMSG, identifier SYS$NODE_TSTVAX value: %X80010000 added to RIGHTSLIST.DAT
%SET-I-INTSET, login interactive limit = 64, current interactive value = 0
  SYSTEM       job terminated at 20-FEB-2019 07:19:02.13

Username: SYSTEM
Password: 
        Welcome to VAX/VMS version  KG 
$ SET TERMINAL/INQUIRE/INSERT/LINE/EDIT/WIDTH=132
$ DELETE/LOG SYS$SYSTEM:STARTUP.INS;*
%DELETE-I-FILDEL, SYS$COMMON:[SYSEXE]STARTUP.INS;1 deleted (44 blocks)
$ @SYS$UPDATE:LIBDECOMP
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]HELPLIB.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSLIB]STARLET.OLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSLIB]ERFLIB.TLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]MAILHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]EDTHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]DEBUGHLP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]EXCHNGHLP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]NCPHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]ANLRMSHLP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]DISKQUOTA.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]EDFHLP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]TPUHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]ACLEDT.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]INSTALHLP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]LATCP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]MNRHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]PATCHHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]PHONEHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]SDA.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]SHWCLHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]SYSGEN.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]TECO.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]VMSTLRHLP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSHLP]UAFHELP.HLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSLIB]STARLET.MLB
%UPGRADE-I-EXPANDING, Decompressing library SYS$COMMON:[SYSLIB]LIB.MLB

          +--------------------------------------------------+
          |                                                  |
          | 2) INSTALL VAX/VMS 4.6 MANDATORY UPDATE          |
          |                                                  |
          +--------------------------------------------------+



$ @SYS$UPDATE:VMSINSTAL VMSMUP DUA3:


        VAX/VMS Software Product Installation Procedure  KG     


It is 20-FEB-2019 at 07:32.
Enter a question mark (?) at any time for help.

* Are you satisfied with the backup of your system disk [YES]? 

Please mount the first volume of the set on DUA3:.
* Are you ready? YES
%MOUNT-I-MOUNTED, VAXVMS047A   mounted on _TSTVAX$DUA3:

The following products will be processed:

  VMSMUP V4.6


        Beginning installation of VMSMUP V4.6 at 07:33

%VMSINSTAL-I-RESTORE, Restoring product saveset A...


        This kit contains the mandatory update for Version 4.6 of VAX/VMS.
        It must be applied to the 4.6 base kit.



        1)  Apply all fixes to the system
        2)  Create a file with the descriptions of all fixes
        3)  Both of the above

* What would you like to do [3]: 
%VMSMUP-I-FIXDESC, The fixes are described in SYS$UPDATE:VMSMUP046.TXT
* Do you want to purge files replaced by this installation [YES]? 
%BACKUP-I-STARTVERIFY, starting verification pass
%BACKUP-W-NOFILES, no files selected from DUA3:[000000]VMSMUP046.B;

  1) CTDRIVER (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]CTDRIVER.EXE;1

  2) F11BXQP (new image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]F11BXQP.EXE;2

  3) LATSYM (new image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-NOGBL, some or all global symbols not accessible
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]LATSYM.EXE;2

  4) PEDRIVER (miscellaneous fix)

  5) RMS (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-NOGBL, some or all global symbols not accessible
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]RMS.EXE;1
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]RMS.EXE;1
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]RMS.EXE;1
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]RMS.EXE;1

  6) SYS (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-NOGBL, some or all global symbols not accessible
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]SYS.EXE;1

  7) SYSLOA8NN (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-NOGBL, some or all global symbols not accessible
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]SYSLOA8NN.EXE;1

  8) TUDRIVER (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]TUDRIVER.EXE;1

  9) UETINIT00 (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-NOGBL, some or all global symbols not accessible
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]UETINIT00.EXE;1

 10) VAXCRTL (miscellaneous fix)

 11) VAXCRTL (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]VAXCRTL.EXE;1

 12) VAXCRTLG (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]VAXCRTLG.EXE;1

 13) XQDRIVER (patch image)
%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.VMSMUP046]XQDRIVER.EXE;1

%VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

        Installation of VMSMUP V4.6 completed at 07:33

%VMSINSTAL-I-REBOOT, This product requires that the system be rebooted.


        SHUTDOWN -- Perform an Orderly System Shutdown


%SHUTDOWN-I-BOOTCHECK, Performing reboot consistency check...
%SHUTDOWN-I-CHECKOK, Basic reboot consistency check completed

%SHUTDOWN-I-OPERATOR, This terminal is now an operator's console.
%%%%%%%%%%%  OPCOM  20-FEB-2019 07:33:11.21  %%%%%%%%%%%
Operator status for operator _TSTVAX$OPA0:
CENTRAL, PRINTER, TAPES, DISKS, DEVICES, CARDS, NETWORK, CLUSTER, SECURITY,
OPER1, OPER2, OPER3, OPER4, OPER5, OPER6, OPER7, OPER8, OPER9, OPER10, OPER11,
OPER12

%SHUTDOWN-I-DISLOGINS, Interactive logins will now be disabled.
%SET-I-INTSET, login interactive limit = 0, current interactive value = 1
%SHUTDOWN-I-STOPQUEMAN, The queue manager will now be stopped.
%JBC-E-JOBQUEDIS, system job queue manager is not running

SHUTDOWN message on TSTVAX from user SYSTEM at _TSTVAX$OPA0:   07:33:11
TSTVAX will shut down in 0 minutes; back up soon.  Please log off node TSTVAX.
Reboot after VMSMUP V4.6 installation.

1 terminal has been notified on TSTVAX.

%SHUTDOWN-I-SITESHUT, The site-specific shutdown procedure will now be invoked.
%SHUTDOWN-I-STOPUSER, All user processes will now be stopped.
%SHUTDOWN-I-REMOVE, All installed images will now be removed.
%SHUTDOWN-I-DISMOUNT, All volumes will now be dismounted.
%%%%%%%%%%%  OPCOM  20-FEB-2019 07:33:11.30  %%%%%%%%%%%
Message from user SYSTEM on TSTVAX
_TSTVAX$OPA0:, TSTVAX shutdown was requested by the operator.

%%%%%%%%%%%  OPCOM  20-FEB-2019 07:33:11.31  %%%%%%%%%%%
Logfile was closed by operator _TSTVAX$OPA0:
Logfile was SYS$SYSROOT:[SYSMGR]OPERATOR.LOG;1

%%%%%%%%%%%  OPCOM  20-FEB-2019 07:33:11.31  %%%%%%%%%%%
Operator _TSTVAX$OPA0: has been disabled, username SYSTEM

        SYSTEM SHUTDOWN COMPLETE - USE CONSOLE TO HALT SYSTEM
Infinite loop, PC: 80008D7E (BRB 80008D7E)
sim> boot rq0
Loading boot code from internal vmb.exe


   VAX/VMS Version V4.6  6-Jul-1987 17:00


%%%%%%%%%%%  OPCOM  20-FEB-2019 07:33:59.65  %%%%%%%%%%%
Logfile has been initialized by operator _TSTVAX$OPA0:
Logfile is SYS$SYSROOT:[SYSMGR]OPERATOR.LOG;2

%SET-I-INTSET, login interactive limit = 64, current interactive value = 0
  SYSTEM       job terminated at 20-FEB-2019 07:33:59.72

Username: SYSTEM
Password: 
        Welcome to VAX/VMS version V4.6
    Last interactive login on Wednesday, 20-FEB-2019 07:24
$ SHOW SYSTEM
VAX/VMS V4.6  on node  20-FEB-2019 07:34:29.35   Uptime    0 00:00:41
  Pid    Process Name    State  Pri      I/O       CPU       Page flts Ph.Mem
00000200 NULL            COM      0        0   0 00:00:39.63         0      0   
00000201 SWAPPER         HIB     16        0   0 00:00:00.00         0      0   
00000204 ERRFMT          HIB      9       22   0 00:00:00.00        73    171   
00000205 OPCOM           LEF      9       16   0 00:00:00.01       155    258   
00000206 JOB_CONTROL     HIB      8       14   0 00:00:00.00        86    286   
00000207 SYSTEM          CUR      4       47   0 00:00:00.00       270    618   
$ SHOW DEVICE SYS$SYSDEVICE/FULL

Disk TSTVAX$DUA0:, device type RA82, is online, mounted, file-oriented device,
    shareable, available to cluster, error logging is enabled.

    Error count                    0    Operations completed               1070
    Owner process                 ""    Owner UIC                         [1,1]
    Owner process ID        00000000    Dev Prot    S:RWED,O:RWED,G:RWED,W:RWED
    Reference count                8    Default buffer size                 512
    Total blocks             1216665    Sectors per track                    57
    Total cylinders             1423    Tracks per cylinder                  15

    Volume label         "VAXVMSRL4"    Relative volume number                0
    Cluster size                   2    Transaction count                    67
    Free blocks               552788    Maximum files allowed            202777
    Extend quantity                5    Mount count                           1
    Mount status              System    Cache name      "_TSTVAX$DUA0:XQPCACHE"
    Extent cache size             64    Maximum blocks in extent cache    55278
    File ID cache size            64    Blocks currently in extent cache    116
    Quota cache size               0    Maximum buffers in FCP cache        998

  Volume status:  subject to mount verification, file high-water marking, write-
      through caching enabled.

$ LOGOUT/FULL
  SYSTEM       logged out at 20-FEB-2019 07:52:02.61

  Accounting information:
  Buffered I/O count:          123      Peak working set size:   619
  Direct I/O count:             41      Peak page file size:    1450
  Page faults:                 489      Mounted volumes:           0
  Charged CPU time:  17-NOV-1858 00:00:00.00   Elapsed time:     0 00:17:56.16

Username: SYSTEM
Password: 
        Welcome to VAX/VMS version V4.6
    Last interactive login on Wednesday, 20-FEB-2019 07:34

          +--------------------------------------------------+
          |                                                  |
          | 3) BACKUP/MODIFY MODPARAMS.DAT, CREATE THE EMPTY |
          |    OLDSITEn DATA FILES AND RUN AUTOGEN           |
          |                                                  |
          +--------------------------------------------------+



$ SET TERMINAL/INQUIRE/INSERT/LINE/EDIT/WIDTH=132
$ TYPE SYS$SYSTEM:MODPARAMS.DAT
SCSSYSTEMID=8188                ! System ID for the CI
SCSNODE="TSTVAX"                ! System node name for CI
VAXCLUSTER=0
$ RENAME/LOG SYS$SYSTEM:MODPARAMS.DAT SYS$SYSTEM:MODPARAMS_ORIGINAL.DAT
%RENAME-I-RENAMED, SYS$SYSROOT:[SYSEXE]MODPARAMS.DAT;1 renamed to SYS$SYSROOT:[SYSEXE]MODPARAMS_ORIGINAL.DAT;1
$ CREATE SYS$SYSTEM:MODPARAMS.DAT
SCSSYSTEMID=8188                ! System ID for the CI
SCSNODE="TSTVAX"                ! System node name for CI
VAXCLUSTER=0

TTY_ALTYPAHD=32767
TTY_TYPAHDSZ=32767

min_PQL_MBYTLM=58000
min_gblpages=250000
min_gblsections=650
min_npagedyn=5458432
min_npagevir=28092416
min_sptreq=8500
<CTRL-Z>
$ CREATE SYS$SYSTEM:OLDSITE1.DAT
<CTRL-Z>
$ CREATE SYS$SYSTEM:OLDSITE2.DAT
<CTRL-Z>
$ CREATE SYS$SYSTEM:OLDSITE3.DAT
<CTRL-Z>
$ CREATE SYS$SYSTEM:OLDSITE4.DAT
<CTRL-Z>
$ @SYS$UPDATE:AUTOGEN GETDATA REBOOT
%AUTOGEN-I-BEGIN, GETDATA phase is beginning.
%AUTOGEN-I-NEWFILE, A new version of SYS$SYSTEM:PARAMS.DAT has been created.
        You may wish to purge this file.
%AUTOGEN-I-END, GETDATA phase has successfully completed.
%AUTOGEN-I-BEGIN, GENPARAMS phase is beginning.
%AUTOGEN-I-NEWFILE, A new version of SYS$MANAGER:VMSIMAGES.DAT has been created.
        You may wish to purge this file.
%AUTOGEN-I-NEWFILE, A new version of SYS$SYSTEM:SETPARAMS.DAT has been created.
        You may wish to purge this file.
%AUTOGEN-I-END, GENPARAMS phase has successfully completed.
%AUTOGEN-I-BEGIN, GENFILES phase is beginning.
%AUTOGEN-I-NOCHANGE, No page file modifications will be made.
%AUTOGEN-I-NOCHANGE, No swap file modifications  will be made.

%AUTOGEN-W-DSKSPC, The system disk would be over 95% full
        if the dump file were created with 524292 blocks.
%AUTOGEN-I-NOCHANGE, No dump file modifications will be made.

%AUTOGEN-I-END, GENFILES phase has successfully completed.
%AUTOGEN-I-BEGIN, SETPARAMS phase is beginning.
%SYSGEN-W-SETMAX, value set to maximum for parameter WSMAX
%%%%%%%%%%%  OPCOM  20-FEB-2019 08:46:23.46  %%%%%%%%%%%
Message from user SYSTEM on TSTVAX
%SYSGEN-I-WRITECUR, CURRENT system parameters modified by process ID 00000207 into file SYS$SYSROOT:[SYSEXE]VAXVMSSYS.PAR;1

%AUTOGEN-I-END, SETPARAMS phase has successfully completed.
%AUTOGEN-I-BEGIN, REBOOT phase is beginning.

The system is shutting down to allow the system to boot with the
generated site-specific parameters and installed images.

The system will automatically reboot after the shutdown and the
upgrade will be complete.



        SHUTDOWN -- Perform an Orderly System Shutdown


%SHUTDOWN-I-BOOTCHECK, Performing reboot consistency check...
%SHUTDOWN-I-CHECKOK, Basic reboot consistency check completed

%SHUTDOWN-I-OPERATOR, This terminal is now an operator's console.
%%%%%%%%%%%  OPCOM  20-FEB-2019 08:46:23.87  %%%%%%%%%%%
Operator status for operator _TSTVAX$OPA0:
CENTRAL, PRINTER, TAPES, DISKS, DEVICES, CARDS, NETWORK, CLUSTER, SECURITY,
OPER1, OPER2, OPER3, OPER4, OPER5, OPER6, OPER7, OPER8, OPER9, OPER10, OPER11,
OPER12

%SHUTDOWN-I-DISLOGINS, Interactive logins will now be disabled.
%SET-I-INTSET, login interactive limit = 0, current interactive value = 1
%SHUTDOWN-I-STOPQUEMAN, The queue manager will now be stopped.
%JBC-E-JOBQUEDIS, system job queue manager is not running

SHUTDOWN message on TSTVAX from user SYSTEM at _TSTVAX$OPA0:   08:46:23
TSTVAX will shut down in 0 minutes; back up soon.  Please log off node TSTVAX.
Reboot system with AUTOGENerated parameters

1 terminal has been notified on TSTVAX.

%SHUTDOWN-I-SITESHUT, The site-specific shutdown procedure will now be invoked.
%SHUTDOWN-I-STOPUSER, All user processes will now be stopped.
%SHUTDOWN-I-REMOVE, All installed images will now be removed.
%SHUTDOWN-I-DISMOUNT, All volumes will now be dismounted.
%SHUTDOWN-I-DISMOUNTDEV, Dismounting device _TSTVAX$DUA3:.
%%%%%%%%%%%  OPCOM  20-FEB-2019 08:46:24.16  %%%%%%%%%%%
Message from user SYSTEM on TSTVAX
_TSTVAX$OPA0:, TSTVAX shutdown was requested by the operator.

%%%%%%%%%%%  OPCOM  20-FEB-2019 08:46:24.17  %%%%%%%%%%%
Logfile was closed by operator _TSTVAX$OPA0:
Logfile was SYS$SYSROOT:[SYSMGR]OPERATOR.LOG;4

%%%%%%%%%%%  OPCOM  20-FEB-2019 08:46:24.18  %%%%%%%%%%%
Operator _TSTVAX$OPA0: has been disabled, username SYSTEM
Loading boot code from internal vmb.exe
Rebooting...


   VAX/VMS Version V4.6  6-Jul-1987 17:00


%%%%%%%%%%%  OPCOM  20-FEB-2019 08:46:53.44  %%%%%%%%%%%
Logfile has been initialized by operator _TSTVAX$OPA0:
Logfile is SYS$SYSROOT:[SYSMGR]OPERATOR.LOG;5

%SET-I-INTSET, login interactive limit = 64, current interactive value = 0
  SYSTEM       job terminated at 20-FEB-2019 08:46:53.49

          +---------------------------------------------------------+
          |                                                         |
          | END OF PREPARATION STAGE FOR VAX/VMS UPGRADE FROM       |
          | VMS 4.6 TO VMS 4.7                                      |
          |                                                         |
          +---------------------------------------------------------+
