
          +--------------------------------------------------+
          |                                                  |
          | START OF DECnet Phase IV installation on VMS 4.7 |
          |                                                  |
          +--------------------------------------------------+


Username: SYSTEM
Password: 
        Welcome to VAX/VMS version V4.7
    Last interactive login on Wednesday, 20-FEB-2019 09:30
$ SHOW NET
%SHOW-I-NONET, network unavailable
$ @SYS$UPDATE:VMSINSTAL NETRTG DUA3:[PRODUCTS.DECNET]


        VAX/VMS Software Product Installation Procedure V4.7    


It is 20-FEB-2019 at 09:49.
Enter a question mark (?) at any time for help.

* Are you satisfied with the backup of your system disk [YES]? 

Please mount the first volume of the set on DUA3:.
* Are you ready? YES
%MOUNT-I-MOUNTED, VAXVMS047A   mounted on _TSTVAX$DUA3:

The following products will be processed:

  NETRTG V4.0


        Beginning installation of NETRTG V4.0 at 09:50

%VMSINSTAL-I-RESTORE, Restoring product saveset A...

    DECnet-VAX Full Function Key installation

%PATCH-I-NOLCL, image does not contain local symbols
%PATCH-I-NOGBL, some or all global symbols not accessible
%PATCH-I-WRTFIL, updating image file VMI$ROOT:[SYSUPD.NETRTG040]NETACP.EXE;1
%VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

        Installation of NETRTG V4.0 completed at 09:50



        VMSINSTAL procedure done at 09:50


$ DIR SYS$MANAGER:*CONFIG*

Directory SYS$COMMON:[SYSMGR]

BOOT_CONFIG.COM;1   NETCONFIG.COM;1     SATELLITE_CONFIG.COM;2
SYCONFIG.COM;1      

Total of 4 files.
$ @SYS$MANAGER:NETCONFIG

        DECnet-VAX network configuration procedure

This procedure will help you define the parameters needed to get DECnet 
running on this machine.  You will be shown the changes before they are 
executed, in case you wish to perform them manually.

What do you want your DECnet node name to be?       [TSTVAX]: 
What do you want your DECnet address to be?                 : 7.1020
Do you want to operate as a router?        [NO (nonrouting)]: YES
Do you want a default DECnet account?                  [YES]: NO

        Here are the commands necessary to setup your system.

--------------------------------------------------------------------------
$ RUN SYS$SYSTEM:NCP
    PURGE KNOWN OBJECTS ALL
    PURGE MODULE CONFIGURATOR KNOWN CIRCUITS ALL
$ DEFINE/USER SYS$OUTPUT NL:
$ DEFINE/USER SYS$ERROR NL:
$ RUN SYS$SYSTEM:NCP    ! Remove existing entry, if any
    PURGE NODE 7.1020 ALL
    PURGE NODE TSTVAX ALL
$ RUN SYS$SYSTEM:NCP
    DEFINE EXECUTOR ADDRESS 7.1020 STATE ON
    DEFINE EXECUTOR NAME TSTVAX
    DEFINE EXECUTOR MAXIMUM ADDRESS 1023
    DEFINE EXECUTOR TYPE ROUTING IV
    DEFINE LINE    UNA-0 STATE ON
    DEFINE CIRCUIT UNA-0 STATE ON COST 3
    DEFINE LOGGING MONITOR STATE ON
    DEFINE LOGGING MONITOR EVENTS 0.0-9
    DEFINE LOGGING MONITOR EVENTS 2.0-1
    DEFINE LOGGING MONITOR EVENTS 4.2-13,15-16,18-19
    DEFINE LOGGING MONITOR EVENTS 5.0-18
    DEFINE LOGGING MONITOR EVENTS 128.0-4
--------------------------------------------------------------------------

Do you want to go ahead and do it? [YES]: 
%NCP-I-NMLRSP, listener response - Success 
Logging sink type = monitor
%NML-I-RECADDED, Database entry added

The changes have been made.

If you have not already installed the DECnet-VAX license, then do so now.

After the license has been installed, you should invoke the procedure
SYS$MANAGER:STARTNET.COM to startup DECnet-VAX with these changes.

(If the license is already installed) Do you want DECnet started? [YES]: 
%%%%%%%%%%%  OPCOM  20-FEB-2019 09:52:27.35  %%%%%%%%%%%
Message from user DECNET on TSTVAX
DECnet starting

%RUN-S-PROC_ID, identification of created process is 00000208
%RUN-S-PROC_ID, identification of created process is 0000020A
$ 
%%%%%%%%%%%  OPCOM  20-FEB-2019 09:52:32.37  %%%%%%%%%%%
Message from user DECNET on TSTVAX
DECnet event 4.10, circuit up
From node 7.1020 (TSTVAX), 20-FEB-2019 09:52:28.65
Circuit UNA-0


$ 
%%%%%%%%%%%  OPCOM  20-FEB-2019 09:52:32.37  %%%%%%%%%%%
Message from user DECNET on TSTVAX
DECnet event 4.15, adjacency up
From node 7.1020 (TSTVAX), 20-FEB-2019 09:52:29.52
Circuit UNA-0, Adjacent node = 7.203


%%%%%%%%%%%  OPCOM  20-FEB-2019 09:52:32.37  %%%%%%%%%%%
Message from user DECNET on TSTVAX
DECnet event 4.15, adjacency up
From node 7.1020 (TSTVAX), 20-FEB-2019 09:52:29.84
Circuit UNA-0, Adjacent node = 7.2


$ SHOW SYS
VAX/VMS V4.7  on node TSTVAX 20-FEB-2019 09:52:45.58   Uptime    0 00:09:40
  Pid    Process Name    State  Pri      I/O       CPU       Page flts Ph.Mem
00000200 NULL            COM      0        0   0 00:09:39.11         0      0   
00000201 SWAPPER         HIB     16        0   0 00:00:00.00         0      0   
00000204 ERRFMT          HIB      8       44   0 00:00:00.00        73    171   
00000205 OPCOM           LEF      9       35   0 00:00:00.00       238    203   
00000206 JOB_CONTROL     HIB      8       15   0 00:00:00.00        86    286   
00000207 SYSTEM          CUR      4     1967   0 00:00:00.55      5817    406   
00000208 NETACP          HIB     10       27   0 00:00:00.00       317    285   
00000209 EVL             HIB      4       45   0 00:00:00.01       326    236  N
0000020A REMACP          HIB      8        8   0 00:00:00.00        69    113   
$ SHOW NETWORK
VAX/VMS Network status for local node  7.1020 TSTVAX on 20-FEB-2019 09:57:24.35



        Node          Links  Cost  Hops   Next Hop to Node

     7.1020 TSTVAX       0     0     0     (Local)   ->  7.1020 TSTVAX
     7.2                 0     3     1     UNA-0     ->  7.2    
     7.4                 0     3     1     UNA-0     ->  7.4    
     7.203               0     3     1     UNA-0     ->  7.203  

                Total of 4 nodes.
$ SET HOST 7371


                       WYTV03
                      UICM/33
                     VAX 8650
                    1988-1990
             Wythenshawe, Manchester, UK



Username: *EXIT*

