RIPSAP DEFINITIONS ::= BEGIN

-- This MIB defines the management information for the RIP and SAP
-- protocols running in an IPX enviroment.  It provides information in 
-- addition to that contained in the IPX MIB itself.  All tables in this
-- MIB are linked to an instance of IPX via the system instance
-- identifier as defined in the IPX MIB.


IMPORTS 
   enterprises, Counter
            FROM RFC1155-SMI
   OBJECT-TYPE
            FROM RFC-1212;

novell  OBJECT IDENTIFIER ::= {enterprises 23}
mibDoc  OBJECT IDENTIFIER ::= { novell 2 }
ripsap  OBJECT IDENTIFIER ::= {mibDoc 20}


-- Groups

ripsapSystem  OBJECT IDENTIFIER ::= {ripsap 1}
ripsapCircuit OBJECT IDENTIFIER ::= {ripsap 2}


-- System Group
--   This group contains global information about each instance of
--   RIP/SAP running on one system.

-- RIP System Table
--   This table contains an entry for each instance of RIP
--   running on the system.

ripSysTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF RIPSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The RIP system table."
   ::= {ripsapSystem 1}

ripSysEntry OBJECT-TYPE
   SYNTAX      RIPSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one instance of RIP
                running on the system."
   INDEX       {ripSysInstance}
   ::= {ripSysTable 1}

RIPSysEntry ::= SEQUENCE {
                        ripSysInstance
                           INTEGER,
                        ripSysState
                           INTEGER,
                        ripSysIncorrectPackets
                           Counter
                       }
                           
ripSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of RIP to
                which this row corresponds.  This value links the
                instance of RIP to an instance of IPX running on the
                system  (i.e. the value of ripSysInstance should be the
                same as a value of ipxSysInstance).  This value may be
                written only when creating a new entry in the table."
   ::= {ripSysEntry 1}

ripSysState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        on(2)
                       }
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Indicates the operational state of this instance of RIP."
   ::= {ripSysEntry 2}

ripSysIncorrectPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times that an incorrectly formatted RIP
                packet was received."
   ::= {ripSysEntry 3}


-- SAP System Table
--   This table contains an entry for each instance of SAP
--   running on the system.

sapSysTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF SAPSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The SAP system table."
   ::= {ripsapSystem 2}

sapSysEntry OBJECT-TYPE
   SYNTAX      SAPSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one instance of SAP
                running on the system."
   INDEX       {sapSysInstance}
   ::= {sapSysTable 1}

SAPSysEntry ::= SEQUENCE {
                        sapSysInstance
                           INTEGER,
                        sapSysState
                           INTEGER,
                        sapSysIncorrectPackets
                           Counter
                       }
                           
sapSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of SAP to
                which this row corresponds.  This value links the
                instance of SAP to an instance of IPX running on the
                system  (i.e. the value of SApSysInstance should be the
                same as a value of ipxSysInstance).  This value may be
                written only when creating a new entry in the table."
   ::= {sapSysEntry 1}

sapSysState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        on(2)
                       }
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Indicates the operational state of this instance of SAP."
   ::= {sapSysEntry 2}

sapSysIncorrectPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times that an incorrectly formatted SAP
                packet was received."
   ::= {sapSysEntry 3}


-- Circuit Group
--   This group contains RIP and SAP management information for each
--   circuit known to this system.

-- RIP Circuit Table
--   The RIP Circuit table contains an entry for the RIP information for
--   each circuit known to the system.

ripCircTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF RIPCircEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The RIP Circuit table."
   ::= {ripsapCircuit 1}

ripCircEntry OBJECT-TYPE
   SYNTAX      RIPCircEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one circuit known to the
                system."
   INDEX       {
                ripCircSysInstance,
                ripCircIndex
               }
   ::= {ripCircTable 1}

RIPCircEntry ::= SEQUENCE {
                        ripCircSysInstance
                           INTEGER,
                        ripCircIndex
                           INTEGER,
                        ripCircState
                           INTEGER,
                        ripCircPace
                           INTEGER,
                        ripCircUpdate
                           INTEGER,
                        ripCircAgeMultiplier
                           INTEGER,
                        ripCircPacketSize
                           INTEGER,
                        ripCircOutPackets
                           Counter,
                        ripCircInPackets
                           Counter
                       }

ripCircSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of RIP and IPX
                (via ipxSysInstance) to which this entry corresponds.
                This value may be written only when creating a new entry in
                the table."
   ::= {ripCircEntry 1}

ripCircIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The identifier of this circuit, unique within the
                instance of RIP.  This value corresponds to the circuit
                identifier found in ipxCircIndex.   This value may be
                written only when creating a new entry in the table."
   ::= {ripCircEntry 2}

ripCircState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        on(2),
                        auto-on(3),
                        auto-off(4)
                       }
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Indicates whether RIP information may be sent/received
                over this circuit."
   DEFVAL      { auto-off }
   ::= {ripCircEntry 3}

ripCircPace OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The maximum pace, in packets per second, at which RIP
                packets may be sent on this circuit."
   ::= {ripCircEntry 4}

ripCircUpdate OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The RIP periodic update interval, in seconds."
   DEFVAL      { 60 }
   ::= {ripCircEntry 5}

ripCircAgeMultiplier OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The holding multiplier for information received in RIP
                periodic updates."
   DEFVAL      { 4 }
   ::= {ripCircEntry 6}

ripCircPacketSize OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The RIP packet size used on this circuit."
   ::= {ripCircEntry 7}

ripCircOutPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of RIP packets sent on this circuit."
   ::= {ripCircEntry 8}

ripCircInPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of RIP packets received on this circuit."
   ::= {ripCircEntry 9}


-- SAP Circuit Table
--   The SAP Circuit table contains an entry for the SAP information for
--   each circuit known to the system.

sapCircTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF SAPCircEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The SAP Circuit table."
   ::= {ripsapCircuit 2}

sapCircEntry OBJECT-TYPE
   SYNTAX      SAPCircEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one circuit known to the
                system."
   INDEX       {
                sapCircSysInstance,
                sapCircIndex
               }
   ::= {sapCircTable 1}

SAPCircEntry ::= SEQUENCE {
                        sapCircSysInstance
                           INTEGER,
                        sapCircIndex
                           INTEGER,
                        sapCircState
                           INTEGER,
                        sapCircPace
                           INTEGER,
                        sapCircUpdate
                           INTEGER,
                        sapCircAgeMultiplier
                           INTEGER,
                        sapCircPacketSize
                           INTEGER,
                        sapCircGetNearestServerReply
                           INTEGER,
                        sapCircOutPackets
                           Counter,
                        sapCircInPackets
                           Counter
                       }

sapCircSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of SAP and IPX
                (via ipxSysInstance) to which this entry corresponds.
                This value may be written only when creating a new entry in
                the table."
   ::= {sapCircEntry 1}

sapCircIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The identifier of this circuit, unique within the
                instance of SAP.  This value corresponds to the circuit
                identifier found in ipxCircIndex.   This value may be
                written only when creating a new entry in the table."
   ::= {sapCircEntry 2}

sapCircState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        on(2),
                        auto-on(3),
                        auto-off(4)
                       }
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Indicates whether SAP information may be sent/received
                over this circuit."
   DEFVAL      { auto-off }
   ::= {sapCircEntry 3}

sapCircPace OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The maximum pace, in packets per second, at which SAP
                packets may be sent on this circuit."
   ::= {sapCircEntry 4}

sapCircUpdate OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The SAP periodic update interval, in seconds."
   DEFVAL      { 60 }
   ::= {sapCircEntry 5}

sapCircAgeMultiplier OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The holding multiplier for information received in SAP
                periodic updates."
   DEFVAL      { 4 }
   ::= {sapCircEntry 6}

sapCircPacketSize OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The SAP packet size used on this circuit."
   ::= {sapCircEntry 7}

sapCircGetNearestServerReply OBJECT-TYPE
   SYNTAX      INTEGER {
                        no(1),
                        yes(2)
                       }
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Indicates whether to respond to SAP get nearest server
                requests received on this circuit."
   DEFVAL      { yes }
   ::= {sapCircEntry 8}

sapCircOutPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of SAP packets sent on this circuit."
   ::= {sapCircEntry 9}

sapCircInPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of SAP packets received on this circuit."
   ::= {sapCircEntry 10}

END

