NLSP DEFINITIONS ::= BEGIN

-- This MIB defines the management information for the NLSP protocol
-- running in an IPX enviroment.  It provides information in addition
-- to that contained in the IPX MIB itself.  All tables in this MIB are
-- linked to an instance of IPX via the system instance identifier as
-- defined in the IPX MIB.
--
-- Change History:
--
--  01/11/94
--    The following DEFVAL values were changed to match the NLSP
--    specification:
--
--      nlspSysMinNonBcastLSPTransInt   5 -> 10
--      nlspSysBcastHelloInt           10 -> 20
--      nlspSysNonBcastHelloInt        10 -> 20
--      nlspSysHoldMult                 5 ->  3
--      nlspSysPartSNPInt               5 ->  1
--      nlspCircHelloTimer             10 -> 20
--
--   The units of nlspDestEstDelay, nlspNodeEstDelay, and nlspLinkDelay
--   were changed from milliseconds to microseconds.
--
--  08/09/95
--    Added Aggregated Routes Table to the Forwarding group
--    and Circuit Aggregated Routes table to the Circuit group.
--
--  10/28/96
--    Removed the ranges from the INTEGER types on nlspSysMaxLSPGenInt
--    and nlspSysMaxLSPAge. This allows corect values of seconds to be
--    returned for Long-lived-LSPs.
--

IMPORTS 
   enterprises, Counter
            FROM RFC1155-SMI
   OBJECT-TYPE
            FROM RFC-1212
   PhysAddress
            FROM RFC1213-MIB;

novell  OBJECT IDENTIFIER ::= {enterprises 23}
mibDoc  OBJECT IDENTIFIER ::= { novell 2 }
nlsp    OBJECT IDENTIFIER ::= {mibDoc 19}


-- Groups

nlspSystem        OBJECT IDENTIFIER ::= {nlsp 1}
nlspCircuit       OBJECT IDENTIFIER ::= {nlsp 2}
nlspForwarding    OBJECT IDENTIFIER ::= {nlsp 3}
nlspNeighbors     OBJECT IDENTIFIER ::= {nlsp 4}
nlspTranslation   OBJECT IDENTIFIER ::= {nlsp 5}
nlspGraph         OBJECT IDENTIFIER ::= {nlsp 6}
nlspLSP           OBJECT IDENTIFIER ::= {nlsp 7}


-- Types

SystemID  ::= OCTET STRING (SIZE(6))
NLSPID    ::= OCTET STRING (SIZE(7))
NetNumber ::= OCTET STRING (SIZE(4))


-- System Group
--   This group contains global information about each instance of NLSP
--   running on one system.

-- System Table
--   This table contains an entry for each instance of NLSP running on
--   the system.

nlspSysTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The NLSP system table."
   ::= {nlspSystem 1}

nlspSysEntry OBJECT-TYPE
   SYNTAX      NLSPSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one instance of NLSP running
                on the system."
   INDEX       {nlspSysInstance}
   ::= {nlspSysTable 1}

NLSPSysEntry ::= SEQUENCE {
                     nlspSysInstance
                        INTEGER,
                     nlspSysState
                        INTEGER,
                     nlspSysID
                        SystemID,
                     nlspSysMinNonBcastLSPTransInt
                        INTEGER,
                     nlspSysMinBcastLSPTransInt
                        INTEGER,
                     nlspSysMinLSPGenInt
                        INTEGER,
                     nlspSysMaxLSPGenInt
                        INTEGER,
                     nlspSysMaxLSPAge
                        INTEGER,
                     nlspSysBcastHelloInt
                        INTEGER,
                     nlspSysNonBcastHelloInt
                        INTEGER,
                     nlspSysDRBcastHelloInt
                        INTEGER,
                     nlspSysHoldTimeMultiplier
                        INTEGER,
                     nlspSysCompSNPInt
                        INTEGER,
                     nlspSysPartSNPInt
                        INTEGER,
                     nlspSysWaitTime
                        INTEGER,
                     nlspSysOrigL1LSPBufSize
                        INTEGER,
                     nlspSysVersion
                        INTEGER,
                     nlspSysCorrLSPs
                        Counter,
                     nlspSysL1Overloaded
                        INTEGER,
                     nlspSysL1DbaseOverloads
                        Counter,
                     nlspSysMaxSeqNums
                        Counter,
                     nlspSysSeqNumSkips
                        Counter,
                     nlspSysTransmittedLSPs
                        Counter,
                     nlspSysReceivedLSPs
                        Counter,
                     nlspSysOwnLSPPurges
                        Counter,
                     nlspSysVersionErrors
                        Counter,
                     nlspSysIncorrectPackets
                        Counter,
                     nlspSysNearestL2DefaultExists
                        INTEGER,
                     nlspSysNearestL2DefaultRouter
                        SystemID,
                     nlspSysResourceFailures
                        Counter,
                    }
                           
nlspSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP to which this
                corresponds.  This value links the instance of NLSP to an
                instance of IPX running on the system  (i.e. the value
                of nlspSysInstance should be the same as a value of
                ipxSysInstance).  This value may be written only when
                creating a new entry in the table."
   ::= {nlspSysEntry 1}

nlspSysState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        nlspLevel1Router(2)
                       }
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Indicates the operational state of this instance of NLSP."
   ::= {nlspSysEntry 2}

nlspSysID OBJECT-TYPE
   SYNTAX      SystemID
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The system ID for this instance of NLSP."
   ::= {nlspSysEntry 3}

nlspSysMinNonBcastLSPTransInt OBJECT-TYPE
   SYNTAX      INTEGER (1..30)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The minimum interval, in seconds, between transmission
                of LSPs on a non-broadcast circuit."
   DEFVAL      { 10 }
   ::= {nlspSysEntry 4}

nlspSysMinBcastLSPTransInt OBJECT-TYPE
   SYNTAX      INTEGER (1..30)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The minimum interval, in seconds, between transmission
                of LSPs on a broadcast circuit."
   DEFVAL      { 5 }
   ::= {nlspSysEntry 5}

nlspSysMinLSPGenInt OBJECT-TYPE
   SYNTAX      INTEGER (1..30)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The minimum interval, in seconds, between the generation
                of the same LSP."
   DEFVAL      { 5 }
   ::= {nlspSysEntry 6}

nlspSysMaxLSPGenInt OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The maximum interval, in seconds, between the generation
                of the same LSP."
   DEFVAL      { 7200 }
   ::= {nlspSysEntry 7}

nlspSysMaxLSPAge OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The value, in seconds, placed in the lifetime field of
                LSPs generated by this instance of NLSP."
   DEFVAL      { 7500 }
   ::= {nlspSysEntry 8}

nlspSysBcastHelloInt OBJECT-TYPE
   SYNTAX      INTEGER (1..100)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The interval, in seconds, at which NLSP Hellos will be
                sent on a broadcast circuit, if this system is not the
                designated router."
   DEFVAL      { 20 }
   ::= {nlspSysEntry 9}

nlspSysNonBcastHelloInt OBJECT-TYPE
   SYNTAX      INTEGER (1..100)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The interval, in seconds, at which NLSP Hellos will be
                sent on a non-broadcast circuit."
   DEFVAL      { 20 }
   ::= {nlspSysEntry 10}

nlspSysDRBcastHelloInt OBJECT-TYPE
   SYNTAX      INTEGER (1..100)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The interval, in seconds, at which the designated
                router sends NLSP Hellos on a broadcast circuit."
   DEFVAL      { 3 }
   ::= {nlspSysEntry 11}

nlspSysHoldTimeMultiplier OBJECT-TYPE
   SYNTAX      INTEGER (2..20)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The holding time multiplier used to specify the holding
                time for NLSP neighbor entries as a function of the NLSP
                Hello interval."
   DEFVAL      { 3 }
   ::= {nlspSysEntry 12}

nlspSysCompSNPInt OBJECT-TYPE
   SYNTAX      INTEGER (1..600)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The interval, in seconds, between generation of Complete
                Sequence Number Packets by a designated router on a
                broadcast circuit."
   DEFVAL      { 30 }
   ::= {nlspSysEntry 13}

nlspSysPartSNPInt OBJECT-TYPE
   SYNTAX      INTEGER (1..60)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The minimum interval, in seconds, between transmission of
                Partial Sequence Number Packets."
   DEFVAL      { 1 }
   ::= {nlspSysEntry 14}

nlspSysWaitTime OBJECT-TYPE
   SYNTAX      INTEGER (1..300)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The number of seconds to delay in the waiting state 
                before entering the on state."
   DEFVAL      { 120 }
   ::= {nlspSysEntry 15}

nlspSysOrigL1LSPBufSize OBJECT-TYPE
   SYNTAX      INTEGER (512..4096)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The maximum size of Level 1 LSPs originated by
                this instance of NLSP."
   DEFVAL      { 512 }
   ::= {nlspSysEntry 16}

nlspSysVersion OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The version number of this instance of NLSP."
   ::= {nlspSysEntry 17}

nlspSysCorrLSPs OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of corrupt LSPs detected."
   ::= {nlspSysEntry 18}

nlspSysL1Overloaded OBJECT-TYPE
   SYNTAX      INTEGER {
                        no(1),
                        yes(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "Indicates whether the NLSP Level 1 database is overloaded."
   ::= {nlspSysEntry 19}

nlspSysL1DbaseOloads OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times the NLSP Level 1 LSP database has
                become overloaded."
   ::= {nlspSysEntry 20}

nlspSysMaxSeqNums OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times the router has attempted to exceed
                NLSP's maximum sequence number."
   ::= {nlspSysEntry 21}

nlspSysSeqNumSkips OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times a sequence number skip has occurred."
   ::= {nlspSysEntry 22}

nlspSysTransmittedLSPs OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of LSPs transmitted by this system."
   ::= {nlspSysEntry 23}

nlspSysReceivedLSPs OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of LSPs received by this system."
   ::= {nlspSysEntry 24}

nlspSysOwnLSPPurges OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times a zero-aged copy of the router's own
                LSP has been received from some other node."
   ::= {nlspSysEntry 25}

nlspSysVersionErrors OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times that a received NLSP packet was
                rejected because its version number was invalid."
   ::= {nlspSysEntry 26}

nlspSysIncorrectPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times that an incorrectly formatted NLSP
                packet was received."
   ::= {nlspSysEntry 27}

nlspSysNearestL2DefaultExists OBJECT-TYPE
   SYNTAX      INTEGER {
                        no(1),
                        yes(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "Indicates whether this instance of NLSP knows
                of a NLSP Level 2 router that currently can reach other
                areas using the default metric."
   ::= {nlspSysEntry 28}

nlspSysNearestL2DefaultRouter OBJECT-TYPE
   SYNTAX      SystemID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The system ID of the nearest NLSP Level 2 router that
                currently can reach other areas using the default
                metric.  The value is undefined if the value of
                nlspSysNearestL2DefaultExists is no."
   ::= {nlspSysEntry 29}

nlspSysResourceFailures OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times this instance of the NLSP has been
                unable to obtain needed resources (memory, etc.)"
   ::= {nlspSysEntry 30}


-- System Area Address Table
--   The System Area Address table contains the area addresses configured
--   for NLSP.

nlspSysAreaTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPSysAreaEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The System Area Address table contains the area addresses
                configured for NLSP."
   ::= {nlspSystem 2}

nlspSysAreaEntry OBJECT-TYPE
   SYNTAX      NLSPSysAreaEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry in the table corresponds to one NLSP
                System Area Address."
   INDEX       {
                nlspSysAreaSysInstance,
                nlspSysAreaNet,
                nlspSysAreaMask
               }
   ::= {nlspSysAreaTable 1}

NLSPSysAreaEntry ::= SEQUENCE {
                           nlspSysAreaSysInstance
                              INTEGER,
                           nlspSysAreaNet
                              OCTET STRING,
                           nlspSysAreaMask
                              OCTET STRING
                          }

nlspSysAreaSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspSysAreaEntry 1}

nlspSysAreaNet OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(4))
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The network address portion of the area address."
   ::= {nlspSysAreaEntry 2}

nlspSysAreaMask OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(4))
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The mask portion of the area address."
   ::= {nlspSysAreaEntry 3}


-- Actual Area Address Table
--   The Actual Area Address table contains the area addresses actually
--   used by NLSP.

nlspActAreaTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPActAreaEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The Actual Area Address table contains the area addresses
                actually used by NLSP."
   ::= {nlspSystem 3}

nlspActAreaEntry OBJECT-TYPE
   SYNTAX      NLSPActAreaEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry in the table corresponds to one NLSP
                Actual Area Address."
   INDEX       {
                nlspActAreaSysInstance,
                nlspActAreaNet,
                nlspActAreaMask
               }
   ::= {nlspActAreaTable 1}

NLSPActAreaEntry ::= SEQUENCE {
                           nlspActAreaSysInstance
                              INTEGER,
                           nlspActAreaNet
                              OCTET STRING,
                           nlspActAreaMask
                              OCTET STRING
                          }

nlspActAreaSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspActAreaEntry 1}

nlspActAreaNet OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(4))
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The network address portion of the area address."
   ::= {nlspActAreaEntry 2}

nlspActAreaMask OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(4))
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The mask portion of the area address."
   ::= {nlspActAreaEntry 3}


-- Circuit Group
--   This group contains the NLSP information for each circuit known
--   to this system.

-- Circuit Table
--   The Circuit table contains an entry containing the NLSP information 
--   for each circuit known to the system.

nlspCircTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPCircEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The Circuit table."
   ::= {nlspCircuit 1}

nlspCircEntry OBJECT-TYPE
   SYNTAX      NLSPCircEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one circuit known to the
                system."
   INDEX       {
                nlspCircSysInstance,
                nlspCircIndex
               }
   ::= {nlspCircTable 1}

NLSPCircEntry ::= SEQUENCE {
                        nlspCircSysInstance
                           INTEGER,
                        nlspCircIndex
                           INTEGER,
                        nlspCircState
                           INTEGER,
                        nlspCircPace
                           INTEGER,
                        nlspCircHelloTimer
                           INTEGER,
                        nlspCircL1DefaultCost
                           INTEGER,
                        nlspCircL1DesRouterPriority
                           INTEGER,
                        nlspCircL1CircID
                           OCTET STRING,
                        nlspCircL1DesRouter
                           SystemID,
                        nlspCircLANL1DesRouterChanges
                           Counter,
                        nlspCircNeighChanges
                           Counter,
                        nlspCircRejNeighbors
                           Counter,
                        nlspCircOutPackets
                           Counter,
                        nlspCircInPackets
                           Counter,
                        nlspCircActualMaxPacketSize
                           INTEGER,
                        nlspCircPSNPsSent
                           Counter,
                        nlspCircPSNPsReceived
                           Counter
                       }

nlspCircSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this entry corresponds.
                This value may be written only when creating a new
                entry in the table."
   ::= {nlspCircEntry 1}

nlspCircIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The identifier of this circuit, unique within the
                instance of NLSP.  This value may be written
                only when creating a new entry in the table."
   ::= {nlspCircEntry 2}

nlspCircState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        on(2)
                       }
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Indicates whether NLSP information may be sent/received
                over this circuit."
   DEFVAL      { on }
   ::= {nlspCircEntry 3}

nlspCircPace OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The maximum pace, in packets per second, at which NLSP
                packets may be sent on this circuit."
   ::= {nlspCircEntry 4}

nlspCircHelloTimer OBJECT-TYPE
   SYNTAX      INTEGER (1..100)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The interval, in seconds, between NLSP Hello packets
                sent on this circuit."
   DEFVAL      { 20 }
   ::= {nlspCircEntry 5}

nlspCircL1DefaultCost OBJECT-TYPE
   SYNTAX      INTEGER (1..63)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The NLSP default cost of this circuit for Level 1
                traffic."
   ::= {nlspCircEntry 6}

nlspCircL1DesRouterPriority OBJECT-TYPE
   SYNTAX      INTEGER (1..127)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The priority for becoming the NLSP LAN Level 1
                Designated Router on a broadcast circuit."
   ::= {nlspCircEntry 7}

nlspCircL1CircID OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(7))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID for this circuit."
   ::= {nlspCircEntry 8}

nlspCircL1DesRouter OBJECT-TYPE
   SYNTAX      SystemID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The system ID of the NLSP LAN Level 1 Designated Router
                on this circuit."
   ::= {nlspCircEntry 9}

nlspCircLANL1DesRouterChanges OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times the NLSP LAN Level 1 Designated
                Router has changed on this circuit."
   ::= {nlspCircEntry 10}

nlspCircNeighChanges OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times a NLSP neighbor state change has
                occurred on this circuit."
   ::= {nlspCircEntry 11}

nlspCircRejNeighbors OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times that a NLSP neighbor has been
                rejected on this circuit."
   ::= {nlspCircEntry 12}

nlspCircOutPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of NLSP packets sent on this circuit."
   ::= {nlspCircEntry 13}

nlspCircInPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of NLSP packets received on this circuit."
   ::= {nlspCircEntry 14}

nlspCircActualMaxPacketSize OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The actual maximum packet size (including header),
                in bytes, that has been used on this circuit."
   ::= {nlspCircEntry 15}

nlspCircPSNPsSent OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of PSNPs sent on this circuit."
   ::= {nlspCircEntry 16}

nlspCircPSNPsReceived OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of PSNPs received on this circuit."
   ::= {nlspCircEntry 17}


-- Circuit Aggregated Routes Table
--   The Circuit Aggregated Routes table contains information about the
--   aggregated routes configured on each circuit.

nlspCircAggRouteTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPCircAggRouteEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The Aggregated Route table contains information about the
                aggregated routes configured on a circuit."
   ::= {nlspCircuit 2}

nlspCircAggRouteEntry OBJECT-TYPE
   SYNTAX      NLSPCircAggRouteEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one aggregated route."
   INDEX       {
                nlspCircAggRouteSysInstance,
                nlspCircAggRouteCircIndex,
                nlspCircAggRouteNetNum,
                nlspCircAggRouteMaskLength
               }
   ::= {nlspCircAggRouteTable 1}

NLSPCircAggRouteEntry ::= SEQUENCE {
                                nlspCircAggRouteSysInstance
                                   INTEGER,
                                nlspCircAggRouteCircIndex
                                   INTEGER,
                                nlspCircAggRouteNetNum
                                   NetNumber,
                                nlspCircAggRouteMaskLength
                                   INTEGER,
                                nlspCircAggRouteTicks
                                   INTEGER,
                                nlspCircAggRouteAreaCount
                                   INTEGER,
                                nlspCircAggStatus
                                   INTEGER
                       }

nlspCircAggRouteSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspCircAggRouteEntry 1}

nlspCircAggRouteCircIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The circuit on which the summary is 
                configured."
   ::= {nlspCircAggRouteEntry 2}

nlspCircAggRouteNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The address summary."
   ::= {nlspCircAggRouteEntry 3}

nlspCircAggRouteMaskLength OBJECT-TYPE
   SYNTAX      INTEGER (0..32)
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Length in bits of the address summary."
   ::= {nlspCircAggRouteEntry 4}

nlspCircAggRouteTicks OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The delay in ticks to ???."
   ::= {nlspCircAggRouteEntry 5}

nlspCircAggRouteAreaCount OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "The number of areas into which this aggregated 
                route can be leaked."
   ::= {nlspCircAggRouteEntry 6}

nlspCircAggRouteStatus OBJECT-TYPE
   SYNTAX      INTEGER {
                        unknown(1),
                        current(2),
                        changed(3),
                        read(4),
                        reading(5),
                        write(6),
                        writing(7)
                       }
   ACCESS      read-write
   STATUS      mandatory
   DESCRIPTION "Indicates whether the information about the aggregated
                routes configured on this circuit matches that
                saved in permanent storage (current).  Setting the
                value to write when it had the value changed will write
                the currently in use information to permanent storage, 
                if supported.  Setting the value to read when it had
                the value changed will replace any routes and services
                currently defined for the circuit with those read from
                permanent storage, if supported."
   ::= {nlspCircAggRouteEntry 7}



-- Forwarding Group
--   This group contains NLSP forwarding information in addition to that
--   contained in the IPX forwarding group.

-- Destination Table
--   The Destination table contains additional NLSP forwarding 
--   information about all destinations learned about via NLSP.

nlspDestTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPDestEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The Destination table contains information about all
                known destinations learned about via NLSP."
   ::= {nlspForwarding 1}

nlspDestEntry OBJECT-TYPE
   SYNTAX      NLSPDestEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one destination."
   INDEX       {
                nlspDestSysInstance,
                nlspDestNetNum
               }
   ::= {nlspDestTable 1}

NLSPDestEntry ::= SEQUENCE {
                        nlspDestSysInstance
                           INTEGER,
                        nlspDestNetNum
                           NetNumber,
                        nlspDestID
                           NLSPID,
                        nlspDestEstDelay
                           INTEGER,
                        nlspDestEstThroughput
                           INTEGER,
                        nlspDestNextHopID
                           NLSPID,
                        nlspDestCost
                           INTEGER
                       }

nlspDestSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspDestEntry 1}

nlspDestNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number of the destination."
   ::= {nlspDestEntry 2}

nlspDestID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The destination NLSP ID (6-octet system ID plus 1-octet
                pseudo-node ID)."
   ::= {nlspDestEntry 3}

nlspDestEstDelay OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The estimated delay, in microseconds, to reach the
                destination."
   ::= {nlspDestEntry 4}

nlspDestEstThroughput OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The estimated throughput, in bits per second, to the
                destination."
   ::= {nlspDestEntry 5}

nlspDestNextHopID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID (6-octet system ID plus 1-octet pseudo-node
                ID) of the next hop."
   ::= {nlspDestEntry 6}

nlspDestCost OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The total path default cost to reach this destination."
   ::= {nlspDestEntry 7}


-- Aggregated Routes Table
--   The Aggregated Routes table contains information about the
--   aggregated routes known to this system.

nlspAggRouteTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPAggRouteEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The Aggregated Route table contains information about all
                known aggregated routes."
   ::= {nlspForwarding 2}

nlspAggRouteEntry OBJECT-TYPE
   SYNTAX      NLSPAggRouteEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one aggregated route."
   INDEX       {
                nlspAggRouteSysInstance,
                nlspAggRouteNetNum,
                nlspAggRouteMaskLength,
                nlspAggRouteNextHopCircIndex
               }
   ::= {nlspAggRouteTable 1}

NLSPAggRouteEntry ::= SEQUENCE {
                        nlspAggRouteSysInstance
                           INTEGER,
                        nlspAggRouteNetNum
                           NetNumber,
                        nlspAggRouteMaskLength
                           INTEGER,
                        nlspAggRouteNextHopCircIndex
                           INTEGER,
                        nlspAggRouteTicks
                           INTEGER,
                        nlspAggRouteAreaCount
                           INTEGER,
                        nlspAggRouteNextHopNICAddress
                           PhysAddress,
                        nlspAggRouteNextHopNetNum
                           NetNumber
                       }

nlspAggRouteSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspAggRouteEntry 1}

nlspAggRouteNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The address summary."
   ::= {nlspAggRouteEntry 2}

nlspAggRouteMaskLength OBJECT-TYPE
   SYNTAX      INTEGER (0..32)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "Length in bits of the address summary."
   ::= {nlspAggRouteEntry 3}

nlspAggRouteNextHopCircIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the circuit used to reach 
                the next hop.  When looking at this table on 
                the router configured to advertise the aggregated 
                route, this is the circuit on which the summary is 
                configured."
   ::= {nlspAggRouteEntry 4}

nlspAggRouteTicks OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The delay in ticks to ???."
   ::= {nlspAggRouteEntry 5}

nlspAggRouteAreaCount OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of areas into which this aggregated 
                route can be leaked."
   ::= {nlspAggRouteEntry 6}

nlspAggRouteNextHopNICAddress OBJECT-TYPE
   SYNTAX      PhysAddress
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NIC address of the next hop.  When looking 
                at this table on the router configured to advertise 
                the aggregated route, this value will be 0 when the 
                route is not being summarized."
   ::= {nlspAggRouteEntry 7}

nlspAggRouteNextHopNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number of the next hop.  When 
                looking at this table on the router configured to 
                advertise the aggregated route, this value will be 0 
                when the route is not being summarized."
   ::= {nlspAggRouteEntry 8}

-- NLSP Neighbors Group
--   This group contains management information for each neighboring
--   NLSP router known to the system.

-- NLSP Neighbors Table
--   This table contains an entry for each neighboring NLSP router
--   known to the system.

nlspNeighTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPNeighEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The NLSP Neighbors table."
   ::= {nlspNeighbors 1}

nlspNeighEntry OBJECT-TYPE
   SYNTAX      NLSPNeighEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corressponds to one neighboring NLSP router
                known to the system."
   INDEX       {
                nlspNeighSysInstance,
                nlspNeighCircIndex,
                nlspNeighIndex
               }
   ::= {nlspNeighTable 1}

NLSPNeighEntry ::= SEQUENCE {
                              nlspNeighSysInstance
                                 INTEGER,
                              nlspNeighCircIndex
                                 INTEGER,
                              nlspNeighIndex
                                 INTEGER,
                              nlspNeighState
                                 INTEGER,
                              nlspNeighNICAddress
                                 PhysAddress,
                              nlspNeighSysType
                                 INTEGER,
                              nlspNeighSysID
                                 SystemID,
                              nlspNeighName
                                 OCTET STRING,
                              nlspNeighUsage
                                 INTEGER,
                              nlspNeighHoldTimer
                                 INTEGER,
                              nlspNeighRemainingTime
                                 INTEGER,
                              nlspNeighPriority
                                 INTEGER
                             }

nlspNeighSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspNeighEntry 1}

nlspNeighCircIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The identifier of the parent circuit of this neighbor
                within this instance of the NLSP and IPX."
   ::= {nlspNeighEntry 2}

nlspNeighIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The identifier for this NLSP neighbor entry, unique 
                within the parent circuit."
   ::= {nlspNeighEntry 3}

nlspNeighState OBJECT-TYPE
   SYNTAX      INTEGER {
                        initializing(1),
                        up(2),
                        failed(3),
                        down(4)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The state of the connection to the neighboring NLSP
                router."
   ::= {nlspNeighEntry 4}

nlspNeighNICAddress OBJECT-TYPE
   SYNTAX      PhysAddress
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NIC Address of the neighboring NLSP router."
   ::= {nlspNeighEntry 5}

nlspNeighSysType OBJECT-TYPE
   SYNTAX      INTEGER {
                        unknown(1),
                        nlspLevel1Router(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The type of the neighboring NLSP router."
   ::= {nlspNeighEntry 6}

nlspNeighSysID OBJECT-TYPE
   SYNTAX      SystemID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The neighboring NLSP router's system ID."
   ::= {nlspNeighEntry 7}

nlspNeighName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The readable name for the neighboring NLSP router."
   ::= {nlspNeighEntry 8}

nlspNeighUsage OBJECT-TYPE
   SYNTAX      INTEGER {
                        undefined(1),
                        level1(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The usage of the connection to the neighboring NLSP
                router."
   ::= {nlspNeighEntry 9}

nlspNeighHoldTimer OBJECT-TYPE
   SYNTAX      INTEGER (1..65535)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The initial holding time, in seconds, for this NLSP
                neighbor entry as specified in the NLSP Hello packet."
   ::= {nlspNeighEntry 10}

nlspNeighRemainingTime OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The remaining time to live, in seconds, for this NLSP
                neighbor entry."
   ::= {nlspNeighEntry 11}

nlspNeighPriority OBJECT-TYPE
   SYNTAX      INTEGER (1..127)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The priority of the neighboring NLSP router for
                becoming the LAN Level 1 Designated router if the value
                of nlspNeighSysType is nlspLevel1Router."
   ::= {nlspNeighEntry 12}


-- Translation Group
--   The translation group contains tables providing mappings between
--   network numbers, NLSP system IDs, and router names.

-- NLSP ID Mapping Table
--   This table maps NLSP system IDs to router names and IPX network
--   numbers.

nlspIDMapTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPIDMapEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "This table maps NLSP system IDs to router names and
                IPX network numbers."
   ::= {nlspTranslation 1}

nlspIDMapEntry OBJECT-TYPE
   SYNTAX      NLSPIDMapEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry maps one NLSP system ID to its corresponding
                router name and IPX network number."
   INDEX       {
                nlspIDMapSysInstance,
                nlspIDMapID
               }
   ::= {nlspIDMapTable 1}

NLSPIDMapEntry ::= SEQUENCE {
                              nlspIDMapSysInstance
                                 INTEGER,
                              nlspIDMapID
                                 NLSPID,
                              nlspIDMapServerName
                                 OCTET STRING,
                              nlspIDMapNetNum
                                 NetNumber
                             }

nlspIDMapSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspIDMapEntry 1}

nlspIDMapID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID (6-octet sytem ID plus the pseudo-node ID)."
   ::= {nlspIDMapEntry 2}

nlspIDMapServerName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The readable name corresponding to this NLSP ID."
   ::= {nlspIDMapEntry 3}

nlspIDMapNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number corresponding to this NLSP ID."
   ::= {nlspIDMapEntry 4}


-- IPX Network Number Mapping Table
--   This table maps IPX network numbers to router names and NLSP IDs.

nlspNetMapTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPNetMapEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "This table maps IPX network numbers to router names
                and NLSP IDs."
   ::= {nlspTranslation 2}

nlspNetMapEntry OBJECT-TYPE
   SYNTAX      NLSPNetMapEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry maps one IPX network number to its
                corresponding router name and NLSP ID."
   INDEX       {
                nlspNetMapSysInstance,
                nlspNetMapNetNum
               }
   ::= {nlspNetMapTable 1}

NLSPNetMapEntry ::= SEQUENCE {
                           nlspNetMapSysInstance
                              INTEGER,
                           nlspNetMapNetNum,
                              NetNumber,
                           nlspNetMapServerName
                              OCTET STRING,
                           nlspNetMapID,
                              NLSPID
                          }

nlspNetMapSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspNetMapEntry 1}

nlspNetMapNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number."
   ::= {nlspNetMapEntry 2}

nlspNetMapServerName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The router name corresponding to the IPX network number."
   ::= {nlspNetMapEntry 3}

nlspNetMapID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID corresponding to the IPX network number."
   ::= {nlspNetMapEntry 4}


-- Name Mapping Table
--   This table maps router names to their corresponding IPX network 
--   number and NLSP ID.

nlspNameMapTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPNameMapEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "This table maps router names to the corresponding IPX
                network number and NLSP ID."
   ::= {nlspTranslation 3}

nlspNameMapEntry OBJECT-TYPE
   SYNTAX      NLSPNameMapEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry maps one router name to its corresponding
                IPX network number and NLSP ID."
   INDEX       {
                nlspNameMapSysInstance,
                nlspNameMapServerName
               }
   ::= {nlspNameMapTable 1}

NLSPNameMapEntry ::= SEQUENCE {
                           nlspNameMapSysInstance
                              INTEGER,
                           nlspNameMapServerName
                              OCTET STRING,
                           nlspNameMapNetNum
                              NetNumber,
                           nlspNameMapID
                              NLSPID
                          }

nlspNameMapSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspNameMapEntry 1}

nlspNameMapServerName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The readable name for this system."
   ::= {nlspNameMapEntry 2}

nlspNameMapNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number corresponding to the router name."
   ::= {nlspNameMapEntry 3}

nlspNameMapID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID corresponding to the router name.  This value
                is undefined if the value of nlspSysState is off."
   ::= {nlspNameMapEntry 4}


-- Graph Group
--   The Graph group provides a representation of the network topology.
--   The group is optional.

-- Node Table
--   The node table contains an entry for each node in the graph.

nlspNodeTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPNodeEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The node table contains an entry for each node in the
                graph."
   ::= {nlspGraph 1}

nlspNodeEntry OBJECT-TYPE
   SYNTAX      NLSPNodeEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one graph node."
   INDEX       {
                nlspNodeSysInstance,
                nlspNodeID
               }
   ::= {nlspNodeTable 1}

NLSPNodeEntry ::= SEQUENCE {
                        nlspNodeSysInstance
                           INTEGER,
                        nlspNodeID
                           NLSPID,
                        nlspNodeNetNum
                           NetNumber,
                        nlspNodeType
                           INTEGER,
                        nlspNodeEstDelay
                           INTEGER,
                        nlspNodeEstThroughput
                           INTEGER,
                        nlspNodeMaxPacketSize
                           INTEGER,
                        nlspNodeCost
                           INTEGER,
                        nlspNodeOverload
                           INTEGER,
                        nlspNodeReachable
                           INTEGER
                       }

nlspNodeSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspNodeEntry 1}

nlspNodeID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID for this node."
   ::= {nlspNodeEntry 2}

nlspNodeNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number of this node."
   ::= {nlspNodeEntry 3}

nlspNodeType OBJECT-TYPE
   SYNTAX      INTEGER {
                        unknown(1),
                        nlspLevel1Router(2),
                        nlspLevel2Router(3),
                        router(4),
                        network(5)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The type of system the node represents."
   ::= {nlspNodeEntry 4}

nlspNodeEstDelay OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The estimated delay, in microseconds, to reach the
                destination represented by this node."
   ::= {nlspNodeEntry 5}

nlspNodeEstThroughput OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The estimated throughput, in bits per second, to the
                destination represented by this node."
   ::= {nlspNodeEntry 6}

nlspNodeMaxPacketSize OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The maximum packet size, in bytes, that can be sent to
                the destination represented by this node."
   ::= {nlspNodeEntry 7}

nlspNodeCost OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The cost to reach this node."
   ::= {nlspNodeEntry 8}

nlspNodeOverload OBJECT-TYPE
   SYNTAX      INTEGER {
                        no(1),
                        yes(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "Indicates whether this node is overloaded."
   ::= {nlspNodeEntry 9}

nlspNodeReachable OBJECT-TYPE
   SYNTAX      INTEGER {
                        no(1),
                        yes(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "Indicates whether the destination represented by this
                node is reachable."
   ::= {nlspNodeEntry 10}


-- Link Table
--   This table contains the entries for all of the links in the graph.

nlspLinkTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPLinkEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The Link table contains entries for all of the links in
                the graph."
   ::= {nlspGraph 2}

nlspLinkEntry OBJECT-TYPE
   SYNTAX      NLSPLinkEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one link."
   INDEX       {
                nlspLinkSysInstance,
                nlspLinkNLSPID,
                nlspLinkIndex
               }
   ::= {nlspLinkTable 1}

NLSPLinkEntry ::= SEQUENCE {
                        nlspLinkSysInstance
                           INTEGER,
                        nlspLinkNLSPID
                           NLSPID,
                        nlspLinkIndex
                           INTEGER,
                        nlspLinkNeighNLSPID
                           NLSPID,
                        nlspLinkFromNeighCost
                           INTEGER,
                        nlspLinkMaxPacketSize
                           INTEGER,
                        nlspLinkThroughput
                           INTEGER,
                        nlspLinkDelay
                           INTEGER,
                        nlspLinkMediaType
                           OCTET STRING,
                        nlspLinkToNeighCost
                           INTEGER
                       }

nlspLinkSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspLinkEntry 1}

nlspLinkNLSPID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID (6-byte system ID plus 1-octet pseudo-node
                ID) of the node to which this link belongs."
   ::= {nlspLinkEntry 2}

nlspLinkIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique value identifying the link within the node."
   ::= {nlspLinkEntry 3}

nlspLinkNeighNLSPID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID (6-byte system ID plus 1-octet pseudo-node
                ID) of the neighboring node."
   ::= {nlspLinkEntry 4}

nlspLinkFromNeighCost OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The cost to use this link to reach this node from
                the neighboring node."
   ::= {nlspLinkEntry 5}

nlspLinkMaxPacketSize OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The maximum size, in bytes, of a packet that may be sent
                over this link."
   ::= {nlspLinkEntry 6}

nlspLinkThroughput OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The link's maximum throughput, in bits per second."
   ::= {nlspLinkEntry 7}

nlspLinkDelay OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The delay, in microseconds, on this link."
   ::= {nlspLinkEntry 8}

nlspLinkMediaType OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(2))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The media type of this link."
   ::= {nlspLinkEntry 9}

nlspLinkToNeighCost OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The cost to use this link to reach the neighbor from
                this node."
   ::= {nlspLinkEntry 10}


-- Path Table
--    This table allows the path(s) that a packet may take to reach a 
--    destination to be reconstructed.  The entries in this table 
--    represent those links that are one hop closer to the source and
--    would be used for the minimum cost path(s) to reach the 
--    destination.

nlspPathTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPPathEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The path table."
   ::= {nlspGraph 3}

nlspPathEntry OBJECT-TYPE
   SYNTAX      NLSPPathEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each row in this table represents a link to a node that
                is one hop closer to the source and would be used for
                the minimum cost path(s) to reach the destination."
   INDEX       {
                nlspPathSysInstance,
                nlspPathDestNLSPID,
                nlspPathLinkIndex
               }
   ::= {nlspPathTable 1}

NLSPPathEntry ::= SEQUENCE {
                        nlspPathSysInstance
                           INTEGER,
                        nlspPathDestNLSPID
                           NLSPID,
                        nlspPathLinkIndex
                           INTEGER
                       }

nlspPathSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this row corresponds."
   ::= {nlspPathEntry 1}

nlspPathDestNLSPID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID (6-octet system ID plus 1-octet pseudo-node
                ID) of this destination."
   ::= {nlspPathEntry 2}

nlspPathLinkIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique value identifying this link within the
                destination node."
   ::= {nlspPathEntry 3}


-- Graph XRoutes Table
--   This table contains information about all of the XRoutes provided by
--   a node in the graph.

nlspGraphXRouteTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPGraphXRouteEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "This table contains the information about the XRoutes
                associated with a node in the graph."
   ::= {nlspGraph 4}

nlspGraphXRouteEntry OBJECT-TYPE
   SYNTAX      NLSPGraphXRouteEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry in the table contains the information for one
                XRoute associated with the node."
   INDEX       {
                nlspGraphXRouteSysInstance,
                nlspGraphXRouteNLSPID,
                nlspGraphXRouteNetNum
               }
   ::= {nlspGraphXRouteTable 1}

NLSPGraphXRouteEntry ::= SEQUENCE {
                        nlspGraphXRouteSysInstance
                           INTEGER,
                        nlspGraphXRouteNLSPID
                           NLSPID,
                        nlspGraphXRouteNetNum
                           NetNumber,
                        nlspGraphXRouteCost
                           INTEGER,
                        nlspGraphXRouteHopCount
                           INTEGER
                       }
               
nlspGraphXRouteSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this entry corresponds."
   ::= {nlspGraphXRouteEntry 1}

nlspGraphXRouteNLSPID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID of the node."
   ::= {nlspGraphXRouteEntry 2}

nlspGraphXRouteNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number of the XRoute's destination."
   ::= {nlspGraphXRouteEntry 3}

nlspGraphXRouteCost OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The cost to reach the XRoute's destination."
   ::= {nlspGraphXRouteEntry 4}

nlspGraphXRouteHopCount OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of hops necessary to reach the XRoute's
                destination."
   ::= {nlspGraphXRouteEntry 5}


-- Graph Services Table
--   This table contains information about all of the services provided by
--   a node in the graph.

nlspGraphServTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPGraphServEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "This table contains the information about the services
                associated with a node in the graph."
   ::= {nlspGraph 5}

nlspGraphServEntry OBJECT-TYPE
   SYNTAX      NLSPGraphServEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry in the table contains the information for one
                service associated with the node."
   INDEX       {
                nlspGraphServSysInstance,
                nlspGraphServNLSPID,
                nlspGraphServName,
                nlspGraphServTypeValue
               }
   ::= {nlspGraphServTable 1}

NLSPGraphServEntry ::= SEQUENCE {
                        nlspGraphServSysInstance
                           INTEGER,
                        nlspGraphServNLSPID
                           NLSPID,
                        nlspGraphServName
                           OCTET STRING,
                        nlspGraphServTypeValue
                           OCTET STRING,
                        nlspGraphServType
                           INTEGER,
                        nlspGraphServNetNum
                           NetNumber,
                        nlspGraphServNode
                           OCTET STRING,
                        nlspGraphServSocket
                           OCTET STRING
                       }
               
nlspGraphServSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this entry corresponds."
   ::= {nlspGraphServEntry 1}

nlspGraphServNLSPID OBJECT-TYPE
   SYNTAX      NLSPID
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NLSP ID of the node."
   ::= {nlspGraphServEntry 2}

nlspGraphServName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(1..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The service name."
   ::= {nlspGraphServEntry 3}

nlspGraphServTypeValue OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(2))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The service type's hexadecimal value."
   ::= {nlspGraphServEntry 4}

nlspGraphServType OBJECT-TYPE
   SYNTAX      INTEGER {
                        unknown(1)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The service type."
   ::= {nlspGraphServEntry 5}

nlspGraphServNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number portion of the IPX address of
                the service."
   ::= {nlspGraphServEntry 6}

nlspGraphServNode OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(6))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The node portion of the IPX address of the service."
   ::= {nlspGraphServEntry 7}

nlspGraphServSocket OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(2))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The socket portion of the IPX address of the service."
   ::= {nlspGraphServEntry 8}


-- LSP Group
--   The LSP group provides a representation of NLSP's LSP database.  This
--   group is optional.

-- LSP Header Table
--    The LSP header table contains summary information about each LSP 
--    in the database as well as an OCTET STRING containing the entire
--    LSP header.

nlspLSPTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPLSPEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The LSP header table."
   ::= {nlspLSP 1}

nlspLSPEntry OBJECT-TYPE
   SYNTAX      NLSPLSPEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one LSP's header."
   INDEX       {
                nlspLSPSysInstance,
                nlspLSPID
               }
   ::= {nlspLSPTable 1}

NLSPLSPEntry ::= SEQUENCE {
                        nlspLSPSysInstance
                           INTEGER,
                        nlspLSPID
                           OCTET STRING,
                        nlspLSPLifetime
                           INTEGER,
                        nlspLSPSeqNum
                           INTEGER,
                        nlspLSPChecksum
                           INTEGER,
                        nlspLSPRouterType
                           INTEGER,
                        nlspLSPOverload
                           INTEGER,
                        nlspLSPHeader
                           OCTET STRING
                       }

nlspLSPSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier for the instance of NLSP and IPX
                (via ipxSysInstance) to which this entry corresponds."
   ::= {nlspLSPEntry 1}

nlspLSPID OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(8))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The value that uniquely identifies this LSP."
   ::= {nlspLSPEntry 2}

nlspLSPLifetime OBJECT-TYPE
   SYNTAX      INTEGER (0..65535)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of seconds prior to the expiration of the
                LSP."
   ::= {nlspLSPEntry 3}

nlspLSPSeqNum OBJECT-TYPE
   SYNTAX      INTEGER (0..255)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The sequence number of the LSP."
   ::= {nlspLSPEntry 4}

nlspLSPChecksum OBJECT-TYPE
   SYNTAX      INTEGER (0..65535)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The checksum value of the LSP."
   ::= {nlspLSPEntry 5}

nlspLSPRouterType OBJECT-TYPE
   SYNTAX      INTEGER {
                        unknown(1),
                        nlspLevel1Router(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The type of the router that sent the LSP."
   ::= {nlspLSPEntry 6}

nlspLSPOverload OBJECT-TYPE
   SYNTAX      INTEGER {
                        no(1),
                        yes(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "Indicates whether the sending router's LSP database is
                overloaded."
   ::= {nlspLSPEntry 7}

nlspLSPHeader OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(27))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The complete LSP header."
   ::= {nlspLSPEntry 8}


-- LSP Options Table
--    The LSP options table is used to obtain each option contained in 
--    an LSP.

nlspLSPOptTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF NLSPLSPOptEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The LSP Options table."
   ::= {nlspLSP 2}

nlspLSPOptEntry OBJECT-TYPE
   SYNTAX      NLSPLSPOptEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one option from an LSP."
   INDEX       {
                nlspLSPOptSysInstance,
                nlspLSPOptLSPID,
                nlspLSPOptIndex
               }
   ::= {nlspLSPOptTable 1}

NLSPLSPOptEntry ::= SEQUENCE {
                           nlspLSPOptSysInstance
                              INTEGER,
                           nlspLSPOptLSPID
                              OCTET STRING,
                           nlspLSPOptIndex
                              INTEGER,
                           nlspLSPOptCode
                              INTEGER,
                           nlspLSPOptLength
                              INTEGER,
                           nlspLSPOptValue
                              OCTET STRING
                          }

nlspLSPOptSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of NLSP and IPX
                (via ipxSysInstance) to which this entry corresponds."
   ::= {nlspLSPOptEntry 1}

nlspLSPOptLSPID OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(8))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The value that uniquely identifies the LSP."
   ::= {nlspLSPOptEntry 2}

nlspLSPOptIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The value that uniquely identifies this option within the
                LSP."
   ::= {nlspLSPOptEntry 3}

nlspLSPOptCode OBJECT-TYPE
   SYNTAX      INTEGER (0..255)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The code that identifies the type of the option."
   ::= {nlspLSPOptEntry 4}

nlspLSPOptLength OBJECT-TYPE
   SYNTAX      INTEGER (0..255)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The length of the option's value field."
   ::= {nlspLSPOptEntry 5}

nlspLSPOptValue OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..255))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The option's value field."
   ::= {nlspLSPOptEntry 6}

END

