;This ADF file is compatable only with the programmed I/O version
; of the NE/2 which is the production version

AdapterID 07154h

AdapterName  "NetWare NE/2 NIC"

NumBytes 1


nameditem
        Prompt  "I/O, EPROM"


;Selections with boot ROM enabled

     Choice "1000H-102FH, 0C8000H-0C9FFFH"

          pos[0]=XXX0001Xb
          io 1000h-102fh
          mem 0C8000H-0C9FFFH
          
     Choice "2020H-204FH, 0CA000H-0CBFFFH"

          pos[0]=XXX0010Xb
          io 2020H-204FH
          mem 0CA000H-0CBFFFH

     Choice "8020H-804FH, 0CC000H-0CDFFFH"

          pos[0]=XXX0011Xb
          io 8020H-804FH 
          mem 0CC000H-0CDFFFH

     Choice "0A0A0H-0A0CFh, 0CE000H-0CFFFFH"

          pos[0]=XXX0100Xb
          io 0A0A0h-0A0CFh
          mem 0CE000H-0CFFFFH

     Choice "0B0B0H-0B0DFh, 0D0000H-0D1FFFH"

          pos[0]=XXX0101Xb
          io 0B0B0H-0B0DFh
          mem 0D0000H-0D1FFFH


     Choice "0C0C0H-0C0EFh, 0D2000H-0D3FFFH"

          pos[0]=XXX0110Xb
          io 0C0C0h-0C0EFh
          mem 0D2000H-0D3FFFH

     Choice "0C3D0H-0C3FFh, 0D4000H-0D5FFFH"

          pos[0]=XXX0111Xb
          io 0C3D0h-0C3FFh
          mem 0D4000H-0D5FFFH




;Selections with boot ROM disabled

     Choice "1000H-102FH, DISABLED"

          pos[0]=XXX1001Xb
          io 1000h-102fh
          
     Choice "2020H-204FH, DISABLED"

          pos[0]=XXX1010Xb
          io 2020H-204FH

     Choice "8020H-804FH, DISABLED"

          pos[0]=XXX1011Xb
          io 8020H-804FH 

     Choice "0A0A0H-0A0CFh, DISABLED"

          pos[0]=XXX1100Xb
          io 0A0A0h-0A0CFh

     Choice "0B0B0H-0B0DFh, DISABLED"

          pos[0]=XXX1101Xb
          io 0B0B0H-0B0DFh

     Choice "0C0C0H-0C0EFh, DISABLED"

          pos[0]=XXX1110Xb
          io 0C0C0h-0C0EFh

     Choice "0C3D0H-0C3FFh, DISABLED"

          pos[0]=XXX1111Xb
          io 0C3D0h-0C3FFh


Help

"The I/O address range shown are the addresses at which the adapter
will decode for the adapter's control and data i/o.  

The EPROM address block is decoded for the use of a remote
boot EPROM.  This optionn may be disabled."




nameditem
        Prompt  "Interrupt level"

     Choice "IRQ 3"

     pos[0]=X00XXXXXb
     int 3

     Choice "IRQ 4"
     pos[0]=X01XXXXXb
     int 4

     Choice "IRQ 5"
     pos[0]=X10XXXXXb
     int 5

     Choice "IRQ 9"
     pos[0]=X11XXXXXb
     int 9


Help

"The IRQ selection assigns which interrupt
request line the lan adapter will use to
signal the microprocessor via the interrupt
controller."



