;ADF file for the NE/2-32 lan adapter
;written by Carleton E. Watkins 17-MAR-89


AdapterID 07151h

AdapterName  "NE/2-32"

NumBytes 1


nameditem
        Prompt  "I/O, RAM (in HEX)"


     Choice "3000-302F, 000C0000-000C7FFF"

          pos[0]=XXXX001Xb
          io 3000H-302FH
          mem 000C0000H-000C7FFFH
          
     Choice "4000-402F, 000D0000-000D7FFF"

          pos[0]=XXXX010Xb
          io 4000H-402FH
          mem 000D0000H-000D7FFFH

     Choice "5000-502F, FFF90000-FFF97FFF"

          pos[0]=XXXX011Xb
          io 5000H-502FH
          mem 0FFF90000H-0FFF97FFFH

     Choice "6000-602F, FFFA0000-FFFA7FFF"

          pos[0]=XXXX100Xb
          io 6000H-602FH
          mem 0FFFA0000H-0FFFA7FFFH

     Choice "7000-702F, FFFB0000-FFFB7FFF"

          pos[0]=XXXX101Xb
          io 7000H-702FH
          mem 0FFFB0000H-0FFFB7FFFH


     Choice "9000-902F, FFFC0000-FFFC7FFF"

          pos[0]=XXXX110Xb
          io 9000H-902FH
          mem 0FFFC0000H-0FFFC7FFFH

     Choice "D000-D02F, FFFD0000-FFFD7FFF"

          pos[0]=XXXX111Xb
          io 0D000H-0D02FH
          mem 0FFFD0000H-0FFFD7FFFH



Help

"The I/O address ranges shown are the 
addresses at which the adapter
will decode for control and use of the
network controller, reset function,
and Ethernet ID address PROM.  

The RAM address will determine where 
the adapter's packet buffer RAM will 
appear in host system's memory map."


nameditem
        Prompt  "Interrupt Request Level"

     Choice "IRQ 3"

     pos[0]=X000XXXXb
     int 3

     Choice "IRQ 4"
     pos[0]=X001XXXXb
     int 4

     Choice "IRQ 5"
     pos[0]=X010XXXXb
     int 5

     Choice "IRQ 9"
     pos[0]=X011XXXXb
     int 9

     Choice "IRQ 10"
     pos[0]=X100XXXXb
     int 10

     Choice "IRQ 11"
     pos[0]=X101XXXXb
     int 11



Help

"The IRQ selection assigns which interrupt
request line the lan adapter will use to
signal the microprocessor via the interrupt
controller."



nameditem
        Prompt  "Connector Selection"


     Choice "Thin Wire"

     pos[0]=1XXXXXXXb

     Choice "Thick Wire"
     pos[0]=0XXXXXXXb

Help

"This selection allows the user to choose
either the thick or thin connector available
on the board."


