<        Installation instructions for OS/2 Device Driver FixPak XR_D003















        

        
        



        August 16, 2002

        
        Build level 10.070
        
        
        
        This FixPak applies to:
        
        XR_4000 Warp v4
        XR_4010 WSOD Rel 2
        XR_4500 WSeB UNI and SMP
        XR_4501 CP1, WSeB and Warp 4
        XR_4502 CP2, WSeB and Warp 4
        
        Requires Corrective Service Facility release F.144 or later
        
        OS/2 Fix Distribution
        Software Group
        Austin, Tx
        
        
        (c) Copyright International Business Machines Corporation, 1981, 2002.
        All rights Reserved.

        August 16, 2002 - Device Driver FixPak XR_D003




                 August 16, 2002 - Device Driver FixPak XR_D003

   CONTENTS


     1.0 Terms and Conditions  . . . . . . . . . . . . . . . . . . . . . . 1

     2.0 Do not use your system  . . . . . . . . . . . . . . . . . . . . . 2

     3.0 Installation Notes  . . . . . . . . . . . . . . . . . . . . . . . 3
       3.0.1 Installation on a Japanese system   . . . . . . . . . . . . . 3
       3.0.2 New SYSLEVEL.BDD  . . . . . . . . . . . . . . . . . . . . . . 3
       3.0.3 Relocated OS/2 file support   . . . . . . . . . . . . . . . . 3
       3.0.4 Please use Fixtool f.144 or later   . . . . . . . . . . . . . 4
       3.0.5 IBM1S506 Device Driver useage   . . . . . . . . . . . . . . . 4
       3.0.6 Updated Corrective Service Facility (CSF)   . . . . . . . . . 5
       3.0.7 CSF0208 No products were found  . . . . . . . . . . . . . . . 5
       3.0.8 CSF0248 Archive path is shared between mismatched   . . . . . 5
       3.0.9 CSF0249 Error opening or creating archive file.   . . . . . . 6
       3.0.10 Configuration Installation Distribution ( CID )  . . . . . . 6
       3.0.11 Read-Only files  . . . . . . . . . . . . . . . . . . . . . . 6

     4.0 Post Installation Notes   . . . . . . . . . . . . . . . . . . . . 7
       4.0.1 Slow mouse acceleration   . . . . . . . . . . . . . . . . . . 7
       4.0.2 New version of IBM1S506.ADD   . . . . . . . . . . . . . . . . 7
       4.0.3 Setting IRQ9 processing in config.sys for VPIC.SYS  . . . . . 7
       4.0.4 Intermittent pause with IBM Thinkpad 760E/ED/ELD/EL   . . . . 8
       4.0.5 APM users   . . . . . . . . . . . . . . . . . . . . . . . . . 8
       4.0.6 Fixed IDE Hard Drive and Removable Media Support  . . . . . . 8

     5.0 New Function   . . . . . . . . . . . . . . . . . . . . . . . . . 10

     6.0 Corrective Service Facility  . . . . . . . . . . . . . . . . . . 11
       6.0.1 Required CSF level   . . . . . . . . . . . . . . . . . . . . 11
       6.0.2 Where you can find CSF code  . . . . . . . . . . . . . . . . 11
       6.0.3 Creating FixPak diskettes  . . . . . . . . . . . . . . . . . 11

     7.0 Installation Process   . . . . . . . . . . . . . . . . . . . . . 13
     7.1 Before installation  . . . . . . . . . . . . . . . . . . . . . . 13
     7.2 Method 1: Install from booted OS/2 partition.    . . . . . . . . 13
     7.3 Method 2: Boot from Corrective Service Disk 1.   . . . . . . . . 15
     7.4 Additional Corrective Service Facility information   . . . . . . 15

     8.0 CSD level of SYSLEVEL.OS2  . . . . . . . . . . . . . . . . . . . 16

     9.0 Latest device drivers  . . . . . . . . . . . . . . . . . . . . . 17

     10.0 FixPak Corrective Service levels and disk layouts   . . . . . . 18

     11.0 Space Utilization   . . . . . . . . . . . . . . . . . . . . . . 27

     12.0 Recovering FixPak ARCHIVE and BACKUP space  . . . . . . . . . . 28


   
                                                                Contents  ii


                 August 16, 2002 - Device Driver FixPak XR_D003

     13.0 TRADEMARKS  . . . . . . . . . . . . . . . . . . . . . . . . . . 29



















































   
                                                               Contents  iii


                 August 16, 2002 - Device Driver FixPak XR_D003

   1.0 TERMS AND CONDITIONS

   Important - please read the following terms and conditions.

   Downloading the Service Fixes included in FixPak XR_D003 for OS/2 Warp 3
   indicates your acceptance of the following terms and conditions:

   1. You must be, and agree that you are, a current licensee of one of the
      following:

      þ  OS/2 Warp 4

      þ  OS/2 Work Space on Demand Release 2

      þ  Warp Server for e-business

      þ  Convenience Pack 1 Warp Server for e-business

      þ  Convenience Pack 1 OS/2 Warp 4

      þ  Convenience Pack 2 Warp Server for e-business

      þ  Convenience Pack 2 OS/2 Warp 4

   2. You may make copies of this Fixpak equal to the number of licensed
      copies of one of the above OS\2 versions covered by Passport Advantage
      Software Maintenance or Software Choice Subscription.
   3. You may only use the Service Fixes included with FixPak XR_D003 for
      maintenance purposes.
   4. All other terms and conditions of your OS/2 license agreements apply
      to the Service Fixes; however, this does not extend any warranty
      and/or services, including but not limited to the "Initial
      Installation" period, outlined in such agreements.



















   
                                                     Terms and Conditions  1


                 August 16, 2002 - Device Driver FixPak XR_D003

   2.0 DO NOT USE YOUR SYSTEM

   Once you begin a FixPak installation, do not try to use your system for
   any other purpose. Doing so may yield unexpected problems which can cause
   the FixPak installation to fail.















































   
                                                   Do not use your system  2


                 August 16, 2002 - Device Driver FixPak XR_D003

   3.0 INSTALLATION NOTES



   3.0.1 INSTALLATION ON A JAPANESE SYSTEM

   When installing this Fixpak on a Japanese system, you may receive a popup
   for KBDBASE.SYS and VKBD.SYS stating that the file on the system is newer
   than the file in the Fixpak and asking if you want to replace it or not.
   You must reply "Yes" to both of these prompts or your keyboard will not
   function correctly.

   The reason this occurs is the US version of these files have both a newer
   date/time stamp and build level string.

   Again, You must reply "Yes" to both of these prompts or your keyboard
   will not function correctly.

   If you replied "No" to either of the prompts and are having problems with
   your keyboard, just reapply the Fixpak and reply "Yes" when prompted as
   described above.


   3.0.2 NEW SYSLEVEL.BDD

   This Fixpak requires a SYSLEVEL.BDD file to be located in the
   \OS2\INSTALL directory of any drive that is to be serviced.  A new
   Fixtool exit called FIXTPREP.EXE is included with this Fixpak. It will
   create a new SYSLEVEL.BDD file in each OS/2 bootable drive if the
   following requirements are met:

   1. \OS2\INSTALL\SYSLEVEL.BDD does not exist
   2. \OS2\INSTALL\SYSLEVEL.FPK exists
   3. \OS2\INSTALL\SYSLEVEL.OS2 is at the following level:
      þ  Fixpak 13 or later for Warp 4
      þ  Fixpak 13 or later for WSOD release 1
      þ  Any level of WSOD release 2

   If yes, then a \OS2\INSTALL\SYSLEVEL.BDD is created which will allow this
   Fixpak to install on this drive.


   3.0.3 RELOCATED OS/2 FILE SUPPORT

   This FixPak will service directories based on the location of supported
   SYSLEVEL.BDD.  Please check your system to make sure extra copies of
   these files are not located in directories other than:

     \OS2\INSTALL\SYSLEVEL.OS2 on the boot drive of your OS/2 partition(s)



   
                                                       Installation Notes  3


                 August 16, 2002 - Device Driver FixPak XR_D003

   If additional copies of these files are found in other locations on your
   hard disk then CSF will try to service files as follows:

   For SYSLEVEL.OS2

     ..\..\   all files in a directory two levels above (toward the root).
              This should be the root directory of your boot drive.
     ..\*     all files in a directory one level above (toward the root) and
              all subdirectories below. This should be the OS2 directory and
              subdirectories.


   If you have moved OS/2 files or directories, do the following
   in order to have them serviced:

   1. Create a file named USERDIRS.BDD in the \OS2\INSTALL directory of the
      OS\2 Warp partition to be serviced.


      In this file, place the full path to the directory you want to be
      serviced. Examples would be:

        C:\JSI\*
        D:\JSI\SH\*



      Be sure to include the trailing * (asterisk) after the last backslash.

   Note: Leave this file for any future OS/2 Device Driver FixPaks you
   might apply.


   3.0.4 PLEASE USE FIXTOOL F.144 OR LATER


   Use Corrective Service Facility (FIXTOOL) build F.144 or later for this
   Device Driver Fixpak and all future Device Driver Fixpaks.


   3.0.5 IBM1S506 DEVICE DRIVER USEAGE


   It is important to use IBMIDECD.FLT with the IBM1S506.ADD driver.
   If you are using the /BM or !BM parameters to enable or disable busmaster;
   you MUST specify the adapter with /A:x. You can also specify the unit on
   that adapter with /U:z.
   For example:




   
                                                       Installation Notes  4


                 August 16, 2002 - Device Driver FixPak XR_D003

       BASEDEV=IBM1S506.ADD /A:0 /U:0 /!BM or /A:0 /!BM to disable BUS Master DMA
       BASEDEV=IBM1S506.ADD /A:0 /U:0 /BM or /A:0 /BM to enable



   Use the /V parameter to view what mode the drives are set to. For example:

       BASEDEV=IBM1S506.ADD /V /A:0 /U:0 /!BM




   3.0.6 UPDATED CORRECTIVE SERVICE FACILITY (CSF)


   Use CSF level f.144 or later for all Fixpaks.  It is contained in CS_144.EXE.
   This is a self-extracting ZIP file.  It is not and does not contain bootable
   disks.


   See the READ.ME file for instructions on how to boot with diskettes along
   with a lot of other useful information.


   3.0.7 CSF0208 NO PRODUCTS WERE FOUND


   This means no SYSLEVEL files was found that had a CSD Level, COMPID, Version and Type that matched
   any of the SYSLEVEL files supported by this FixPak. Run the SYSLEVEL command and record the output
   for SYSLEVEL.OS2 in the OS2/INSTALL directory on your boot drive. Compare this data with the data
   contained in the README.1ST file on FixPak disk 1.


   To recover from this, rename the existing SYSLEVEL.OS2 file to SYSL.OS2 and copy SYSLEVEL.OS2 from
   your Warp 4 installation DISK 1.


   3.0.8 CSF0248 ARCHIVE PATH IS SHARED BETWEEN MISMATCHED

   1. The Archive path you specified (or was previously specified) contains
      files from a different release of OS/2. You need to specify a different
      Archive path.
   2. You have a bad SYSLEVEL.OS2 or SYSLEVEL.MPM file. Both must have the same
      Current CSD Level, Version, Type and Component ID if you point both FixPak
      Archives to the same location.


      Check \OS2\INSTALL\SYSLEVEL.OS2 and \MMOS2\INSTALL\SYSLEVEL.MPM. If either is
      wrong, place the last FixPak disk in A: and run
      FIXSYSL.CMD to correct SYSLEVEL.OS2
      problems or SYSZMPM.CMD to fix SYSLEVEL.MPM problems.

   
                                                       Installation Notes  5


                 August 16, 2002 - Device Driver FixPak XR_D003

   3.0.9 CSF0249 ERROR OPENING OR CREATING ARCHIVE FILE.


   Typically this means the FixPak Archive directory has been deleted but the
   files that point to it still exist. You need to delete the LOGF000.BDD and
   LOGSTART.BDD files from your OS2/INSTALL directory.  LOGSTART.BDD has the
   R/O attribute set and it needs to be reset before the file can be deleted.
   There may also be a LOGARCH.OS2 file that needs to be deleted.


   This can also occur for Multi Media Presentation Manager/2 (MMPM). You would
   then need to delete the LOGF0000.MPM and LOGSTART.MPM files from the
   \MMOS2\INSTALL directory and possibly LOGARCH.MPM if it exists.


   3.0.10 CONFIGURATION INSTALLATION DISTRIBUTION ( CID )

   Read the README.CID on Disk # 1 for an example of how to set up
   a response file to do a CID install.


   3.0.11 READ-ONLY FILES


   If you installed OS/2 from a CD-ROM, some files being updated
   may have the Read-Only attribute set. This will cause the update
   program to ask you if you want the files replaced. Answer OK.

























   
                                                       Installation Notes  6


                 August 16, 2002 - Device Driver FixPak XR_D003

   4.0 POST INSTALLATION NOTES



   4.0.1 SLOW MOUSE ACCELERATION


   Some systems may experience a slow mouse acceleration after this FixPak
   has been installed. If you experience this problem, restore MOUSE.SYS,
   VMOUSE.SYS, and POINTDD.SYS from your BACKUP directory.


   4.0.2 NEW VERSION OF IBM1S506.ADD


   This FixPak contains a new version of IBM1S506.ADD. This version has special
   features for flushing the buffers when shutting down OS/2. There was a new,
   undocumented parameter added on the IBM1S506.ADD BASEDEV line in CONFIG.SYS.

    /!SHUTDOWN  - Disable spin down of drives

   This parameter disables the new feature that has been determined to cause some
   disk drives not to respond when the system is rebooted from any state but a
   physical power on (use of the CTRL-ALT-DEL keys either before or after the
   SHUTDOWN icon is used).
   If your system is experiencing such a problem, please add the /!SHUTDOWN
   parameter to your CONFIG.SYS.

   In the next release of IBM1S506.ADD, /!SHUTDOWN will be the default behavior,
   and a /SHUTDOWN will be added to enable the feature.


   4.0.3 SETTING IRQ9 PROCESSING IN CONFIG.SYS FOR VPIC.SYS


   Some applications like PCAS (and some terminal emulators) have problems
   sharing IRQ9 in a VDM.  Since the DOS Virtual Device drivers are not loaded
   out of CONFIG.SYS, a new device driver VPICPARM.SYS has been added starting
   with Warp 4 FixPak 8.

   To prevent sharing of IRQ9 in a VDM, add the following statement in
   config.sys:

      device=x:\os2\mdos\vpicparm.sys irq9_off
      (x: is your OS/2 boot drive)



   Next, in the settings for the program that requires exclusive access to IRQ9,
   set the DOS setting HW_SHARE_IRQ9 to ON.


   
                                                  Post Installation Notes  7


                 August 16, 2002 - Device Driver FixPak XR_D003


   When you next boot your system, VDMs will not share IRQ9.


   4.0.4 INTERMITTENT PAUSE WITH IBM THINKPAD 760E/ED/ELD/EL


   If you have an IBM Thinkpad 760E/ED/ELD/EL that exhibits sluggish harddisk behavior
   (pausing intermittently with hard drive light on) after this FixPak has been applied,
   add the /!BM parameter to the BASEDEV=IBM1S506.ADD statement (if present) in  your
   CONFIG.SYS.  This will disable the Bus Mastering function whose default has been changed
   from OFF to ON.


   If your CONFIG.SYS has the statement

   BASEDEV=PIIXIDE.ADD



   you must remark out the statement by inserting REM as the first characters on the line
   as shown below.

   REM BASEDEV=PIIXIDE.ADD
   BASEDEV=IBM1S506.ADD /A:0 /!BM /U:1 /ATAPI /FORCE




   4.0.5 APM USERS


   APM users will need to add the following statement after the
   DEVICE=\OS2\BOOT\APM.SYS statement in their CONFIG.SYS:

      RUN=\OS2\BOOT\APMDAEMN.EXE



   This will complete the fix for APAR JR09869.


   4.0.6 FIXED IDE HARD DRIVE AND REMOVABLE MEDIA SUPPORT


   FixPak 6 (FP6) for Warp 4 extended support for fixed Enhanced IDE drives to
   sizes up to 8.4GB and added new caching HPFS and FAT file system support for
   removable media drives such as SCSI Syquest Syjet 1.5GB portable hard drive
   and the Iomega jaz 1GB and 2GB personal hard drives.



   
                                                  Post Installation Notes  8


                 August 16, 2002 - Device Driver FixPak XR_D003


   See the README.RMS file on the first FixPak diskette for complete information
   on large IDE Hard Drive and Removable Media Support.

















































   
                                                  Post Installation Notes  9


                 August 16, 2002 - Device Driver FixPak XR_D003

   5.0 NEW FUNCTION


   It is our policy not to include new function in FixPaks. However, as with
   any policy there
   may be exceptions. If any exception occurs in the future,
   we will communicate them to you in this section of the README.1ST.













































   
                                                            New Function  10


                 August 16, 2002 - Device Driver FixPak XR_D003

   6.0 CORRECTIVE SERVICE FACILITY



   6.0.1 REQUIRED CSF LEVEL


   You must use release level F.144 or later of the OS/2 Corrective Service
   Facility to install this FixPak.
   Check the BUILD.LVL file for the level you are using.
   If it does not have a BUILD.LVL file then it is old and
   cannot be used.


   6.0.2 WHERE YOU CAN FIND CSF CODE


   The latest Corrective Service Facility code is available
   from:


   ftp://service.boulder.ibm.com/ps/products/os2/fixtool/


   Select the required language then the latest fixtool release (CS?143 at the
   time this Fixpak was released).


   The .TXT file has instructions.  The .EXE is a self-extracting ZIP file that
   contains the CSF code.  See the READ.ME file contained in .EXE for
   information on how to use the new CSF.


   6.0.3 CREATING FIXPAK DISKETTES


   Use LOADDSKF.EXE to create the diskettes. For each disk image, place
   a 2MB HD (1.44MB formatted) diskette in A:.

   Warning: DO NOT use a 1MB (720KB formatted) diskette because you might have problems
   trying to install this FixPak.


   For each diskette image in the FixPak, do the following:


   Enter LOADDSKF XR_D003.?DK A: /F  (? can be 1 through 9, A through Z).


   Label the diskette as


   
                                             Corrective Service Facility  11


                 August 16, 2002 - Device Driver FixPak XR_D003

         FixPak XR_D003
   Corrective Service Diskette ?
          (CSF DISK ?)

















































   
                                             Corrective Service Facility  12


                 August 16, 2002 - Device Driver FixPak XR_D003

   7.0 INSTALLATION PROCESS



   7.1 BEFORE INSTALLATION


   Before installing any FixPak, run CHKDSK /F against
   all drives on your system to correct any file system errors that might be
   present. You cannot do this while OS/2 is active. You must shut down and
   run CHKDSK by one of the following methods:

   þ  Boot from your Installation and DISK 1 diskettes
      you used to install OS/2 with.
      If your file system is HPFS, then put the diskette with CHKDSK and
      UHPFS.DLL on it in your A: drive before issuing the CHKDSK command.
   þ  Boot from the Utilities disk you created via the "Create Utility
      Diskettes" icon in the System Setup folder.
   þ  Boot from a different OS/2 partition.



   7.2 METHOD 1: INSTALL FROM BOOTED OS/2 PARTITION.

   This method allows you to select the products (partitions) to be serviced.


   This is the method you should use if you have more than one OS/2 partition
   and want to control which one is serviced.

   Note: You can use a diskette drive other than A: with this method. If your
   3.5" diskette drive is B:, use B: where A: is mentioned in the following steps.
   (this method only).

   1. Insert CSF DISK Diskette 1 in drive A.
   2. Open an OS/2 window or full-screen session.
   3. Type A:\SERVICE and press the Enter key.

      Note: You could also use the "Drives" object for A: and double click on the
      "SERVICE.EXE" Icon to start the install.
   4. Follow the displayed instructions. When prompted to insert Corrective
      Service Diskette 1 (not CSF DISK Diskette 1), place FixPak XR_D003
      Corrective Service Diskette 1 in drive A. Repeat for the rest of the FixPak
      disks when requested to do so.

      Note: It can take a considerable length of time for the Corrective Service
      Facility to scan your hard disk for serviceable files. In some cases, it has
      taken as long as 40 minutes. Please be patient and allow this process to
      complete.
   5. If this is the first OS/2 Warp FixPak you have applied to
      this system, then enter the path to the ARCHIVE directory

   
                                                    Installation Process  13


                 August 16, 2002 - Device Driver FixPak XR_D003

      where a copy of replaced files
      will be stored (for example, D:\ARCHIVE).

      Note: This ARCHIVE directory is not related to the ARCHIVES directory
      built into OS/2. Please specify a different path.
      You must specify a different ARCHIVE directory for each product to
      be serviced.


      If this is not the first OS/2 FixPak, then enter the path
      to the BACKUP directory
      where a copy of replaced files will be stored (for example,
      D:\BACKUP).

      Note: You must specify a different BACKUP directory for each product to
      be serviced.


      For either case, make sure there is sufficient space available on the
      drive you specify. Even though these files are kept in compressed
      (PACK2) format, they require between 7 and 12 MB of disk space.
   6. Click on "OK".
   7. You will see an "Application in use" dialog box showing a list of
      locked files that cannot be serviced while the system is running.
      You are given two choices - to Continue or Reboot. Select
      Continue.
   8. During the installation process you might see messages about Archiving,
      Updating and Deferring service.
      þ  Archiving saves a compressed copy of the original file in the
         ARCHIVE or BACKUP path you specified.
      þ  Updating means the original files are replaced with the new
         ones from this FixPak.
      þ  Deferring service means the file to be updated is currently in use
         by the system and cannot be updated. The new files from the FixPak
         are placed in unpacked format
         in the \IBMCSFLK\FIX directory on the drive with the most free space.
         They are processed by the locked file device
         driver during reboot after you shut down the system.
   9. Select NO for a redisplay of the "Product List" after
      the first part of the FixPak application process has completed if this
      message is displayed.
   10.Click Cancel and Exit to close the Corrective Service Facility window
      if necessary.
   11.Shut down and reboot your system.

      You will see the following during reboot of the system
      if you applied service to the
      OS/2 partition you were booted from.




   
                                                    Installation Process  14


                 August 16, 2002 - Device Driver FixPak XR_D003

      The locked file driver is loaded.

             Processing locked files

             Processing complete



      The system will do one automatic reboot after the Locked File Device Driver
      has completed.



   7.3 METHOD 2: BOOT FROM CORRECTIVE SERVICE DISK 1.


   This method does not prompt the user for any information. No interaction with
   the user takes place other than requests to put the next diskette in drive A.
   All serviceable partitions on your system will be updated automatically. Be
   especially careful of extra SYSLEVEL.OS2 or SYSLEVEL.MPM files when using
   this method because they can cause CSF to apply service to directories you do
   not want serviced.

   1. Shut down your OS/2 system.
   2. Insert CSF DISK Diskette 1 in drive A.
   3. Press Ctrl+Alt+Del to boot the disk in drive A.


   Service will be applied to ALL partitions that contain a version of OS/2
   that is supported by this FixPak. See the section "FixPak Corrective
   Service Notes" for the CSD levels this FixPak applies to.

   Note: It can take a considerable length of time for the Corrective Service
   Facility to scan your hard disk for serviceable files. In some cases it has
   taken as long as 40 minutes. Please be patient and allow this process to
   complete.


   7.4 ADDITIONAL CORRECTIVE SERVICE FACILITY INFORMATION


   Additional information on the Corrective Service Facility is available
   from the README.INF file on the first Corrective Service
   Facility disk. To view this file, place CSF disk 1 in drive A and enter
   VIEW A:\README.INF.







   
                                                    Installation Process  15


                 August 16, 2002 - Device Driver FixPak XR_D003

   8.0 CSD LEVEL OF SYSLEVEL.OS2


   The Current CSD level for the "IBM OS/2 Base Operating System" will
   not be changed by installation of this FixPak even though the
   SERVICE.LOG file indicates it will. This FixPak is not a Service Level
   change. It upgrades the existing service level, therefore
   the SYSLEVEL is not changed.


   All fix information is recorded in SERVICE.LOG. Look at the file

      \OS2\INSTALL\SERVICE.LOG



   on your boot drive for information relating to the installation of
   FixPaks on your system.


   The first page of this document has a line that looks like:

   Build Level: n.nnn



   That is the number you should see when you run the BLDLEVEL command against
   device drivers contained in this Fixpak that have a build level string.
   Note that some do driver have the string and some don't.























   
                                               CSD level of SYSLEVEL.OS2  16


                 August 16, 2002 - Device Driver FixPak XR_D003

   9.0 LATEST DEVICE DRIVERS

   You can find the latest device drivers as well as other files in the
   OS/2 Device Driver Pak Online site (DD-Pak Online) at:

      http://www7.software.ibm.com/2bcprod.nsf



   Some of the selections will require you to have a Software Choice
   Subscription, others will be free.









































   
                                                   Latest device drivers  17


                 August 16, 2002 - Device Driver FixPak XR_D003

   10.0 FIXPAK CORRECTIVE SERVICE LEVELS AND DISK LAYOUTS

   Build Level: 10.070

   Product location on CSD:  A:\FIX\BDD.1
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.00
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4000_
   System Id:  1000
   Component Id:  5639A6100
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.01
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4010_
   System Id:  1000
   Component Id:  5639A6120
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.50
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4500_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.50
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4500_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.51
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4501_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.51
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4501_
   System Id:  1000
   Component Id:  5639A6150

   
                       FixPak Corrective Service levels and disk layouts  18


                 August 16, 2002 - Device Driver FixPak XR_D003

   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.51
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4501_
   System Id:  1000
   Component Id:  5639A6101
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4502_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4502_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4502_
   System Id:  1000
   Component Id:  5639A6101
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4503_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4503_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"

   
                       FixPak Corrective Service levels and disk layouts  19


                 August 16, 2002 - Device Driver FixPak XR_D003

   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4503_
   System Id:  1000
   Component Id:  5639A6101
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\*
           ..\..\VT
           ..\..\VT\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*
   Will create the following directories
      ..\..\OS2\BOOT   Stub File:  @BOOTDIR

      ..\..\OS2\MDOS   Stub File:  @MDOSDIR

      ..\..\OS2   Stub File:  @OS2DIR

      ..\..\OS2\DLL   Stub File:  @DLLDIR

      ..\..\OS2\SYSTEM   Stub File:  @SYSTDIR

      ..\..\OS2\SYSTEM\TRACE   Stub File:  @TRACDIR


   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   152XPRES.EXE  152XPRES.EX_    2    05/21/2002  15:48     3125  C0BA9152
   154XPRES.EXE  154XPRES.EX_    2    05/21/2002  15:47     3245  DFA9A16F
   164XPRES.EXE  164XPRES.EX_    2    05/21/2002  15:48     2773  766E9BB7
   174XPRES.EXE  174XPRES.EX_    2    05/21/2002  15:48     2933  F6AD6C4E
   7770PRES.EXE  7770PRES.EX_    2    05/21/2002  15:49     3141  1AFDEABF
   7870PRES.EXE  7870PRES.EX_    2    01/18/2002  12:44     6822  168E183C
   AHA152X.ADD   AHA152X.AD_     1    05/21/2002  15:48    44224  CE3262C5
   AHA154X.ADD   AHA154X.AD_     2    05/21/2002  15:47    20646  FD60A229
   AHA164X.ADD   AHA164X.AD_     2    05/21/2002  15:47    20038  84CD128C
   AHA174X.ADD   AHA174X.AD_     2    05/21/2002  15:48    18030  AD1DEEF3
   AHA6360.SNP   AHA6360.SN_     1    05/21/2002  16:21    27383  8BEC1E68
   AIC7770.ADD   AIC7770.AD_     1    05/21/2002  15:49    42574  55ACDC2E
   AIC7870.ADD   AIC7870.AD_     1    04/24/2002  14:30   154140  F90C5FAD
   AIC7870.SNP   AIC7870.SN_     2    05/21/2002  16:22     9104  D02E943C
   AIC78U2.ADD   AIC78U2.AD_     1    01/18/2002  12:45   156412  C580A7AF

   
                       FixPak Corrective Service levels and disk layouts  20


                 August 16, 2002 - Device Driver FixPak XR_D003

   APM.SYS       APM.SY_         2    05/21/2002  15:37    12751  C438695B
   APMDAEMN.EXE  APMDAEMN.EX_    2    04/03/2002  15:52     2733  E7A844BD
   AUDMPIO.DRV   AUDMPIO.DR_     2    01/18/2002  13:34     7264  50D12669
   BSAUDIO.SNP   BSAUDIO.SN_     2    04/03/2002  15:30     5752  3D5CA1DB
   BSAUDRES.DLL  BSAUDRES.DL_    2    01/18/2002  13:33     1380  0C784492
   BTKPRES.EXE   BTKPRES.EX_     2    05/21/2002  15:51     2941  06739008
   BTSCSI.ADD    BTSCSI.AD_      1    05/21/2002  15:51    26567  CCD1F1FF
   BUSAUDIO.SYS  BUSAUDIO.SY_    1    05/21/2002  16:26    31965  D2B04932
   CD_BOOT.FLT   CD_BOOT.FL_     2    05/21/2002  15:54     5658  CDDCBE70
   CMD640X.ADD   CMD640X.AD_     1    05/21/2002  15:52    36038  A9B286D5
   CMPXCHG8.SYS  CMPXCHG8.SY_    2    04/25/2002  14:51     2650  46FA9E29
   COM.SYS       COM.SY_         1    08/13/2002  13:47    25335  02CC6C0D
   CS31BA11.DRV  CS31BA11.DR_    1    01/18/2002  13:58   104208  086DAEF8
   DELIVERY.SYS  DELIVERY.SY_    2    05/21/2002  15:46     3806  FAE48809
   DELIVPRC.EXE  DELIVPRC.EX_    2    05/21/2002  15:46     2733  AAF6F467
   DETNE2.SYS    DETNE2.SY_      2    04/03/2002  14:32     5666  04130B4F
   DPT20XX.ADD   DPT20XX.AD_     1    05/21/2002  15:50    24700  3719E304
   DPTPRES.EXE   DPTPRES.EX_     2    05/21/2002  15:51     3463  D412024A
   ES688DD.SYS   ES688DD.SY_     1    01/18/2002  13:34    40448  A467D13B
   ES688WIN.386  ES688WIN.38_    2    01/18/2002  13:34    14197  61986F47
   ES688WIN.DRV  ES688WIN.DR_    1    01/18/2002  13:34    64336  6BD4EDB2
   ESSVSD88.DLL  ESSVSD88.DL_    2    01/18/2002  14:20     1140  6137BA00
   EXTDSKDD.SYS  EXTDSKDD.SY_    2    05/21/2002  16:14     1682  3AD8C748
   FD16-700.ADD  FD16-700.AD_    1    05/21/2002  15:49    34146  C715A28D
   FD16-700.EXE  FD16-700.EX_    2    05/21/2002  15:49     3725  AA163D5E
   FD7000EX.ADD  FD7000EX.AD_    2    05/21/2002  15:49    20762  2910B44F
   FD7000EX.EXE  FD7000EX.EX_    2    05/21/2002  15:50     2801  AF406944
   FD8XX.ADD     FD8XX.AD_       1    05/21/2002  15:50    29944  80ABA468
   FD8XX.EXE     FD8XX.EX_       2    05/21/2002  15:50     3263  69F8B284
   FLASHPT.ADD   FLASHPT.AD_     1    05/21/2002  15:51    57125  18EB0E61
   FLASHPT.SNP   FLASHPT.SN_     2    05/21/2002  16:19     4161  2A759FF1
   I2OXPORT.SYS  I2OXPORT.SY_    2    05/21/2002  15:54    11132  5B60612D
   IBM16AFS.EXE  IBM16AFS.EX_    2    05/21/2002  15:50     3177  AF72CF09
   IBM1FLPY.ADD  IBM1FLPY.AD_    1    05/21/2002  15:45    35418  F768431C
   IBM1S506.ADD  IBM1S506.AD_    1    05/21/2002  15:57    62730  235026B0
   IBM2ADSK.ADD  IBM2ADSK.AD_    2    05/21/2002  15:45     9936  616114F2
   IBM2AMB1.SYS  IBM2AMB1.SY_    2    05/21/2002  16:07    12453  4E716B63
   IBM2CAD1.SYS  IBM2CAD1.SY_    2    05/21/2002  16:08    12495  07BBEA52
   IBM2CMQ1.SYS  IBM2CMQ1.SY_    2    05/21/2002  16:07    10101  A7BA7BC6
   IBM2FLPY.ADD  IBM2FLPY.AD_    2    05/21/2002  15:45    14424  18D09BA0
   IBM2MAT1.SYS  IBM2MAT1.SY_    2    05/21/2002  16:08    10083  6E6D456A
   IBM2NCR1.SYS  IBM2NCR1.SY_    2    05/21/2002  16:08    10063  30C981EE
   IBM2NEC1.SYS  IBM2NEC1.SY_    2    05/21/2002  16:08    10063  17586A02
   IBM2SCPR.EXE  IBM2SCPR.EX_    2    05/21/2002  15:46     3051  593219F3
   IBM2SCSI.ADD  IBM2SCSI.AD_    1    05/21/2002  15:46    33115  70CDFEC6
   IBM2SS02.SYS  IBM2SS02.SY_    2    05/21/2002  16:37    22835  5F75D24B
   IBM2ZEN1.SYS  IBM2ZEN1.SY_    2    04/03/2002  15:09    10047  25F2316E
   IBM2ZOS1.SYS  IBM2ZOS1.SY_    2    05/21/2002  16:08    10079  17313DE7
   IBMATAPI.FLT  IBMATAPI.FL_    1    05/21/2002  16:40    31172  3719FC52
   IBMIDECD.FLT  IBMIDECD.FL_    1    05/21/2002  15:57    24616  7CB36AC4
   IBMINT13.I13  IBMINT13.I1_    2    05/21/2002  15:46    11522  89AE2DFE

   
                       FixPak Corrective Service levels and disk layouts  21


                 August 16, 2002 - Device Driver FixPak XR_D003

   IBMKBD.SYS    IBMKBD.SY_      2    05/21/2002  16:03     8714  CD6A612C
   ICMEMCDD.SYS  ICMEMCDD.SY_    2    04/03/2002  15:13    13932  68CEB1EB
   ICMEMFMT.EXE  ICMEMFMT.EX_    1    04/03/2002  15:13    50932  01C46628
   ICMEMMTD.SYS  ICMEMMTD.SY_    2    04/03/2002  15:13     7788  F069A669
   IPSRAID.ADD   IPSRAID.AD_     2    04/24/2002  18:47    22310  AACDFBC4
   JAZZDD.SYS    JAZZDD.SY_      1    05/21/2002  16:27    44522  2C9BF210
   KBDBASE.SYS   KBDBASE.SY_     1    05/21/2002  16:05    24989  BCCBE3F4
   LMS205.ADD    LMS205.AD_      1    05/21/2002  15:57    36386  A2B36E9C
   LMS206.ADD    LMS206.AD_      1    05/21/2002  15:58    38744  98735A13
   MITFX001.ADD  MITFX001.AD_    2    05/21/2002  15:56    20506  82D7CAD1
   MMMIXER.DLL   MMMIXER.DL_     2    01/18/2002  14:03    22800  9244C67E
   MOUSE.SYS     MOUSE.SY_       1    05/21/2002  16:02    30819  22CC268E
   MSBUS01.SYS   MSBUS01.SY_     2    05/21/2002  16:01     1294  4261BBCD
   MSINP01.SYS   MSINP01.SY_     2    05/21/2002  16:01     1411  5FEC8DCB
   MSSER01.SYS   MSSER01.SY_     2    05/21/2002  16:01     1761  1CAD73F8
   MSSER02.SYS   MSSER02.SY_     2    05/21/2002  16:00     2198  13655725
   MVPROAUD.DRV  MVPROAUD.DR_    2    01/18/2002  14:04    24608  5A6230F0
   MVPRODD.SYS   MVPRODD.SY_     1    05/21/2002  16:27    52444  47011C06
   OPL3.DRV      OPL3.DR_        1    01/18/2002  14:11    56384  3F702A0C
   OS2ASPI.DMD   OS2ASPI.DM_     2    05/21/2002  16:33    11234  F96EB82E
   OS2CDROM.DMD  OS2CDROM.DM_    1    05/21/2002  15:54    39528  9375B3BF
   OS2SCSI.DMD   OS2SCSI.DM_     2    05/21/2002  16:33    11606  461AD894
   PCIBUS.SNP    PCIBUS.SN_      2    04/03/2002  15:23     2496  40610DEE
   PCLOGIC.SYS   PCLOGIC.SY_     2    05/21/2002  16:02     3692  1E91EDEB
   PCMOU02.SYS   PCMOU02.SY_     2    05/21/2002  15:59     2306  67807469
   PDIMOU01.SYS  PDIMOU01.SY_    2    05/21/2002  16:00     1388  4C13AF4B
   PDIMOU02.SYS  PDIMOU02.SY_    2    05/21/2002  15:59     2018  D8E0CCF0
   PDITOU01.SYS  PDITOU01.SY_    2    05/21/2002  16:13    13642  7A678DAB
   PDITOU02.SYS  PDITOU02.SY_    2    05/21/2002  16:13    13234  1372C375
   POINTDD.SYS   POINTDD.SY_     2    05/21/2002  16:10     3846  8C3B4B6C
   PRINT01.SYS   PRINT01.SY_     2    05/21/2002  16:11    16894  19E03242
   PRINT02.SYS   PRINT02.SY_     2    05/21/2002  16:11    12134  8FB67A8C
   RESERVE.SYS   RESERVE.SY_     2    05/21/2002  15:37     5704  8D6D43D0
   RESOURCE.SYS  RESOURCE.SY_    1    05/21/2002  15:36    55402  1FD05C95
   RMAUDIO.SYS   RMAUDIO.SY_     2    05/21/2002  16:26    26273  9D34925E
   RMINFO.DLL    RMINFO.DL_      1    04/03/2002  14:31    22847  96EAE8DF
   RMVIEW.EXE    RMVIEW.EX_      1    05/21/2002  15:36    32885  C103FFF3
   SB16D2.SYS    SB16D2.SY_      1    01/18/2002  13:43    64424  7A436B63
   SBAWE32.DRV   SBAWE32.DR_     1    01/18/2002  14:06    48640  DE2980A1
   SBAWED2.SYS   SBAWED2.SY_     1    01/18/2002  13:43   101700  A1E8AE4A
   SBCD2.ADD     SBCD2.AD_       2    05/21/2002  15:56    18828  229DA2D8
   SBD2.SYS      SBD2.SY_        1    04/03/2002  15:37    41388  7C84F9DA
   SBP2D2.SYS    SBP2D2.SY_      1    04/03/2002  15:37    46508  DFCAF6C0
   SBPD2.SYS     SBPD2.SY_       1    04/03/2002  15:37    43948  8650F0C5
   SGAUDVDD.SYS  SGAUDVDD.SY_    2    01/18/2002  13:46     6144  1C17BFC3
   SONY31A.ADD   SONY31A.AD_     1    05/21/2002  15:56    32734  20369B40
   SONY535.ADD   SONY535.AD_     2    05/21/2002  15:56    19538  BA78B61F
   SYM8XX.ADD    SYM8XX.AD_      1    01/18/2002  12:59    63580  82E88D8D
   SYM8XXPC.EXE  SYM8XXPC.EX_    2    01/18/2002  12:59     9185  FD36534F
   SYM_HI.ADD    SYM_HI.AD_      1    01/18/2002  12:59    67140  2B253BF5
   SYM_HIPC.EXE  SYM_HIPC.EX_    2    01/18/2002  12:59     9177  63D8DFCB

   
                       FixPak Corrective Service levels and disk layouts  22


                 August 16, 2002 - Device Driver FixPak XR_D003

   TESTCFG.SYS   TESTCFG.SY_     2    05/21/2002  16:11     9808  4880A13D
   TMV1PRES.EXE  TMV1PRES.EX_    2    05/21/2002  15:43     3017  F64795FD
   TMV1SCSI.ADD  TMV1SCSI.AD_    2    05/21/2002  16:34    21660  E27AF070
   TOUCH.SYS     TOUCH.SY_       2    05/21/2002  16:12    20090  664DC9E5
   U160PRES.EXE  U160PRES.EX_    2    01/18/2002  12:47     6822  8337CCAD
   USBAUDIO.HLP  USBAUDIO.HL_    2    01/18/2002  16:02     1067  B6B0901E
   USBAUDIO.ICO  USBAUDIO.IC_    2    01/18/2002  16:02      874  DEB26F26
   USBAUDIO.SCR  USBAUDIO.SC_    2    01/18/2002  16:02     3092  DDD8FDAA
   USBAUDIO.SYS  USBAUDIO.SY_    1    05/21/2002  16:41    35884  D5B76B78
   USBCDROM.ADD  USBCDROM.AD_    2    05/21/2002  16:41     5278  11EE3DDA
   USBCOM.SYS    USBCOM.SY_      2    05/21/2002  16:41    19943  083FF221
   USBD.SYS      USBD.SY_        1    05/21/2002  16:40    21634  22D7F3F4
   USBETHR.NIF   USBETHR.NI_     2    04/24/2002  17:08     1114  63CA7D98
   USBETHR.OS2   USBETHR.OS_     2    05/21/2002  16:41    19446  E2F51F16
   USBHID.SYS    USBHID.SY_      2    05/21/2002  16:41    13310  7B8505DB
   USBKBD.SYS    USBKBD.SY_      1    05/21/2002  16:41    12804  9E21B464
   USBMOUSE.SYS  USBMOUSE.SY_    2    05/21/2002  16:41    12338  A7E04046
   USBMSD.ADD    USBMSD.AD_      1    05/21/2002  16:41    31394  C9291399
   USBOHCD.SYS   USBOHCD.SY_     1    05/21/2002  16:41    30292  DC52346B
   USBUHCD.SYS   USBUHCD.SY_     1    05/21/2002  16:40    25840  A35EEA8A
   VAPM.SYS      VAPM.SY_        2    04/03/2002  15:30     1120  D5E01A22
   VASPI.SYS     VASPI.SY_       2    04/03/2002  15:17     8992  1B01544E
   VCDROM.SYS    VCDROM.SY_      2    04/03/2002  15:30     6880  48DF9AE8
   VCOM.SYS      VCOM.SY_        2    04/03/2002  15:31    12384  8170D9C1
   VDISK.SYS     VDISK.SY_       2    05/21/2002  16:13     2920  49BE559B
   VDSK.SYS      VDSK.SY_        2    04/03/2002  15:31    10384  64028653
   VFLPY.SYS     VFLPY.SY_       2    04/03/2002  15:32     6064  8428B9F3
   VIDRMS.SYS    VIDRMS.SY_      2    05/21/2002  16:26    29073  38E7AC24
   VIDVBC.SYS    VIDVBC.SY_      2    05/21/2002  16:29    28501  96E03800
   VISION02.SYS  VISION02.SY_    2    05/21/2002  15:59     2294  20D59D0A
   VKBD.SYS      VKBD.SY_        1    05/21/2002  16:24    25655  21A7B759
   VLPT.SYS      VLPT.SY_        2    04/03/2002  15:32    10081  0E3ACAFF
   VMOUSE.SYS    VMOUSE.SY_      2    04/03/2002  15:33    18704  02A968D4
   VSNDSYS.386   VSNDSYS.38_     1    01/18/2002  14:11    64026  D9AE3A28
   VTOUCH.SYS    VTOUCH.SY_      2    04/03/2002  15:34    13660  0EA85767

   ************************************************************************
   Product location on CSD:  A:\FIX\BDD.2
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.00
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4000_
   System Id:  1000
   Component Id:  5639A6100
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.01
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4010_
   System Id:  1000

   
                       FixPak Corrective Service levels and disk layouts  23


                 August 16, 2002 - Device Driver FixPak XR_D003

   Component Id:  5639A6120
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.50
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4500_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.50
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4500_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.51
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4501_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.51
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4501_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.51
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4501_
   System Id:  1000
   Component Id:  5639A6101
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4502_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________

   
                       FixPak Corrective Service levels and disk layouts  24


                 August 16, 2002 - Device Driver FixPak XR_D003

   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4502_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4502_
   System Id:  1000
   Component Id:  5639A6101
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4503_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4503_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.52
   Fixpak name:   XR_D003_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4503_
   System Id:  1000
   Component Id:  5639A6101
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\..\..\..\IBMLAN\RPL\BB10.JP\OS2
           ..\..\..\..\..\IBMLAN\RPL\BB20.JP\OS2

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   106BASE.SYS   KBD-106X.SY_    2    09/21/2001  23:49    30765  89179796

   
                       FixPak Corrective Service levels and disk layouts  25


                 August 16, 2002 - Device Driver FixPak XR_D003

   AXBASE.SYS    KBD-AXX.SY_     2    09/21/2001  23:50    28205  BFE6333B
   KBDBASE.SYS   KBD-AX.SY_      2    09/21/2001  23:50    28205  89D73ADA
   KBDBASE.SYS   KBD-106.SY_     2    09/21/2001  23:49    30765  75179797
   KBDBASE.SYS   KBD-101.SY_     2    09/21/2001  23:47    31501  31B89B3C
   POINTDD.SYS   POINTDD.SY_     2    05/21/2002  16:10     3846  8C39F76C
   POINVGA2.SYS  POINTDDX.SY_    2    05/21/2002  16:10     3846  A5D79863
   USBASE.SYS    KBD-101X.SY_    2    09/21/2001  23:47    31501  39B934C2
   VKBD.SYS      VKBD101.SY_     2    04/15/2002  17:59    54523  250204A6
   VKBD.SYS      VKBD106.SY_     2    04/15/2002  17:59    54334  211D8980
   VKBD106.SYS   VKBD106X.SY_    2    04/15/2002  17:59    54334  B865D16D
   VKBDUS.SYS    VKBD101X.SY_    2    04/15/2002  17:59    54523  2E909843









































   
                       FixPak Corrective Service levels and disk layouts  26


                 August 16, 2002 - Device Driver FixPak XR_D003

   11.0 SPACE UTILIZATION


   The FixPak installation process requires free space on the following drives:

   Space needed
                  Drive

   Up to 2MB
                  C:

   Up to 2MB
                  Boot drive (4MB if boot is C:)

   Up to 22MB
                  Drive with most free space, holds deferred files if A:SERVICE method
                  used.

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4000

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4010

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4500

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4501

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4502

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4503

   Note: The lines labeled "FixPak Archive/Backup for product with CSD level of"
   will be on the drive you specify and will occupy up to the size indicated for
   the Archive and for the Backup directories. If, for example, the indicated
   size is 30MB then the space actually occupied on the drive can be up to 60MB.












   
                                                       Space Utilization  27


                 August 16, 2002 - Device Driver FixPak XR_D003

   12.0 RECOVERING FIXPAK ARCHIVE AND BACKUP SPACE

   Warning: Make sure you read and understand the following before
   removing the Archive and Backup files and directories.


   You can recover the space used for FixPak Archive and Backup files as
   long as you understand that doing this prevents you from being able to
   backout to the previous Backup or Archive level. If it becomes
   necessary at a later time to backout a FixPak, the only way you can do
   this is to reinstall Warp.


   Do the following to delete the FixPak Backup and Archive files and
   remove the files used by CSF to keep track of what service has been
   applied to your system.

   1.  Delete every instance of the following files on your system
       (search every drive and every directory they contain).
       þ   LOGF0000.*   (can be OS2 or MPM)
       þ   LOGSTART.*   (can be OS2 or MPM)
       þ   LOGARCH.*    (can be OS2 or MPM)
       þ   CSF_*.*
       þ   FIXSTART
   2.  Delete the files in the FixPak Archive and Backup directories on
       your harddisk.
   3.  Remove the FixPak Archive and Backup directories with the RMDIR
       command.
























   
                              Recovering FixPak ARCHIVE and BACKUP space  28


                 August 16, 2002 - Device Driver FixPak XR_D003

   13.0 TRADEMARKS


   The following terms are trademarks of the International Business
   Machines Corporation in the United States or other countries or both:

   þ  IBM
   þ  OS/2



   Other company, product, and service names may be trademarks or service
   marks of others.


   THE INFORMATION PROVIDED IN THIS README IS PROVIDED "AS IS" WITHOUT
   WARRANTY OF ANY KIND.  IBM DISCLAIMS ALL WARRANTIES, WHETHER
   EXPRESSED OR IMPLIED, INCLUDING WITHOUT LIMITATION, THE IMPLIED
   WARRANTIES OF FITNESS FOR A PARTICULAR PURPOSE AND MERCHANTABILITY
   WITH RESPECT TO THE INFORMATION IN THIS DOCUMENT. BY FURNISHING
   THIS DOCUMENT, IBM GRANTS NO LICENSES TO ANY PATENTS OR COPYRIGHTS.


   (C) Copyright IBM Corporation, 2002. All rights reserved.
   U.S. Government Users Restricted Rights -- Use, duplication or
   disclosure restricted by GSA ADP Schedule Contract with IBM Corp.


























   
                                                              TRADEMARKS  29
