00000093
®U 2 6 FA drv_menu_text¯ Install OS/2 Version 2.1    
 Install OS/2 Warp           
 Uninstall OS/2 2.1 drivers  
 Uninstall OS/2 Warp drivers 
 Read Installation Notes     
®U 7 10 FA pmdir_text¯    About to install the Presentation Manager Driver.  
    Please enter the OS/2 boot drive on which the      
    Presentation Manager driver will be installed:     
                                                       
®U 11 20 FA pmundir_text¯                Presentation Manager Driver Uninstall                
 About to remove the PM driver.  The directories containing the PM   
 driver will be removed, and the files CONFIG.SYS and SYSTEM.INI     
 (located in WINOS2) will be modified to remove the driver.          
 
 Backups of the above files will be saved with the extension .BAK    
 in the same directories.                                            
 
 Please enter the OS/2 boot drive on which the PM driver is located: 
                                                                     
®U 21 23 FA windir_text¯ Please enter the full path to                
 the Windows directory :                      
                                              
®U 24 25 FA windowdir_text¯ Please enter the full path of Windows driver directory 
                                                        
®U 26 31 FA wife_check_text¯ Simplified  Chinese  OS/2 
 Traditional Chinese  OS/2 
 Japanese OS/2             
 Korean   OS/2             
 Thai     OS/2             
 English  OS/2             
®U 32 34 FA NotInstalledmsg_text¯ Cannot find the drivers with 32 bit seamless 
 Windows support.  Probably they have been    
 removed already or have never been installed.
®U 35 36 FA ActiveDrivermsg_text¯ Unable to uninstall an active display driver.      
 Please use DSPINSTL to install a VGA driver first. 
®U 37 38 FA WarpActivemsg_text¯ Unable to uninstall an active display driver. Please 
 use SELECTIVE INSTALL to install a VGA driver first. 
®U 39 41 FA OldDrivermsg_text¯ An old 16 bit version of the display driver is  
 currently active.  Please upgrade to the 32 bit 
 driver first. 
®U 42 43 FA NotOS2Bootmsg_text¯ The specified drive is not an OS/2 boot 
 drive.  Please choose another drive.    
®U 44 44 FA copy_problem_text¯ Problem Copying File 
®U 45 45 FA directory_failure_text¯ Could not locate directory; Installation aborted 
®U 46 46 FA UninstallFailure_text¯ Unable to complete uninstall of drivers. 
®U 47 48 FA need_OS2_text¯ To uninstall, you must run from a DOS 
 full screen session from within OS/2  
®U 49 49 FA no_readme_file_text¯ Unable to display the Installation Notes 
®U 50 57 FA pm_done_text¯ Your PM drivers have been successfully copied. 
 Now you need to exit from this program, and    
 run DSPINSTL from within an OS/2 Window.       
 
 When DSPINSTL asks you for the location of the 
 driver files, specify the following directory: 
 
 
®U 58 60 FA unpm_done_text¯ The OS/2 display drivers have been successfully 
 uninstalled.  The backup files CONFIG.BAK and   
 SYSTEM.BAK (if necessary) have been created. 
®U 61 64 FA missing_files_text¯ Files missing:                 
 Please run Install from Disk 1 
 of the ORIGINAL diskettes that 
 accompany the Video Adapter.   
®U 65 65 FA win_inst_msg_text¯ Do you have Windows installed in your system? (Y/N) 
®U 66 66 NP copying_msg¯Copying %s to %s 
®M 67 67 0 0 drv_menu¯    Install OS/2 Drivers     
®M 68 68 0 0 pmdir¯ 
®M 69 69 0 0 pmundir¯ 
®M 70 70 0 0 windir¯ 
®M 71 71 0 0 windowdir¯ 
®M 72 72 0 0 wife_check¯  OS/2  Far East Editions  
®G 73 73 0 0 NotInstalledmsg¯ 
®G 74 74 0 0 ActiveDrivermsg¯ 
®G 75 75 0 0 WarpActivemsg¯ 
®G 76 76 0 0 OldDrivermsg¯ 
®G 77 77 0 0 NotOS2Bootmsg¯ 
®G 78 78 0 0 copy_problem¯ 
®G 79 79 0 0 directory_failure¯ 
®G 80 80 0 0 UninstallFailure¯ 
®G 81 81 0 0 need_OS2¯ 
®G 82 82 0 0 no_readme_file¯ 
®G 83 83 0 0 pm_done¯ 
®G 84 84 0 0 unpm_done¯ 
®G 85 85 0 0 missing_files¯ 
®G 86 86 0 0 win_inst_msg¯ 
®G 87 87 0 0 msg_base¯mb
®U 88 88 NP run_only_from_install¯This program can not be executed from the command line
®U 89 89 NP pm_drvr_not_instld¯PM Driver not Installed
®U 90 94 FA OS2_warning_msg_text¯ These drivers require the OS/2 Video FixPack to    
 function properly under OS/2 2.1x. If you have     
 not already installed the OS/2 Video Fixpack,      
 please contact your local IBM representative for   
 the latest upgrade. Do you want to continue (Y/N)? 
