; Citrix modem definitions
;
; WARNING:  Individual modem sections (names) cannot exceed 33 characters
; including the brackets.
;
;--------------------------------
[Apex Data PCMCIA Data/Fax - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=57600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT W1 X4 &K3<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[AT&T Comsphere 3800 Serie - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT \\X1 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[AT&T DataPort 14.4/FAX Mo - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT &C1 \\X1 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[ATI 14400 ETC-Express PCM - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=57600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F0<cr>
COMMAND_INIT=AT S0=0 &C1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[ATI 14400 ETC-I/E Fax-Mod - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F2<cr>
COMMAND_INIT=AT S0=0 &C1<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[ATI 2400etc/e - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=ATE1 &F2 V1 X6 S0=0 S38=5 &B1&C1&K3<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Black Box 325 Modem/Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1 %B6%C1 \\G\\J\\Q3<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Boca Research M1440 14.4K - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATE1V1X4 S0=0 &C1&D1&K3&S1<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Boca Research V.FAST 28.8 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATE1V1X4 S0=0 &C1&D1&K3&S1<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Bullet E9696m V.32 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X1 &C1 $C1$E1$F4$L3$S1$X5 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Cardinal 9600 V.42bis Ext - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&K3&R0 %C1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Cardinal MVPV34XF Ext - CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=138
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Cardinal MVPV34I Int - CTX]
ALIAS=Cardinal MVPV34XF Ext - CTX

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

;--------------------------------
[Cardinal MVPV34ILC Int - CTX]
ALIAS=Cardinal MVPV34XF Ext - CTX

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

;--------------------------------
[Crdnl MVPV34ISP Int Voice - CTX]
ALIAS=Cardinal MVPV34XF Ext - CTX

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

;--------------------------------
[Crdnl MVPV34XSP Ext Voice - CTX]
ALIAS=Cardinal MVPV34XF Ext - CTX

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

;--------------------------------
[Cardinal MVPV34PC PCMCIA - CTX]
ALIAS=Cardinal MVPV34XF Ext - CTX

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

;--------------------------------
[Cardnl MVPV34IV Int Voice - CTX]
ALIAS=Cardinal MVPV34XF Ext - CTX

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

;--------------------------------
[Cardnl MVPV34XV Ext Voice - CTX]
ALIAS=Cardinal MVPV34XF Ext - CTX

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

;--------------------------------
[Compaq 14.4 PCMCIA Data + - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Compaq Enhanced 9600 Data - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=ATE1 &C1 V1 X1 W1 S95=32 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Compaq PCMCIA 14.4 Data+F - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=57600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Compaq PCMCIA SPEEDPAQ 14 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=57600
MAXCONNECTBPS=57600

COMMAND_INIT=ATE1 V1 X4 S0=0 &D2&S1 \\G0\\J0\\N3\\Q3\\X1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Compaq SPEEDPAQ 144/P PCM - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &D2&S1 \\G0\\J0\\N3\\Q3\\X1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Compaq SPEEDPAQ 192 PCMCI - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &D2&S1 \\G0\\J0\\N3\\Q3\\X1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Dallas Fax Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATE1V1X4 &C1&D1&K3&Q9&S1 \\G0\\N3 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Encore 1200 HB Integral M - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=1200
MAXCONNECTBPS=1200

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Entre 2400X - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Evercom 96 Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&D1&S1 %C1%E1 \\A3\\G0\\J0\\N3\\Q3<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Generic 2400 Baud Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Generic 9600 Baud Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[GVC 14400bps V.42 Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&D2 \\N6\\Q3\\J\\V1 %C1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[GVC 28800bps V.42 Fax Mod - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATS0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[GVC 9600bps V.42 Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&D2 \\N6\\Q3\\V1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes ACCURA 144 + FAX144 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATW1 &C1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes ACCURA 288 V.FC + F - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATW1 &C1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Accura 33600 v7.x - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=%C0"H0
<compression_on>=%C1"H3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 DT

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=33600

COMMAND_INIT=AT&F&C1&D2 V1 W1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Accura336 IntData/Fx -CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=138
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=33600

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Accura336 IntFxVoice -CTX]
ALIAS=Hayes Accura336 IntData/Fx -CTX
;--------------------------------
[Hayes Accura336 ExtFxVoice -CTX]
ALIAS=Hayes Accura336 IntData/Fx -CTX

;--------------------------------
[Hayes Accura336 IntFx/DSVD -CTX]
ALIAS=Hayes Accura336 IntData/Fx -CTX

;--------------------------------
[Hayes Accura336 ExtFx/DSVD -CTX]
ALIAS=Hayes Accura336 IntData/Fx -CTX

;--------------------------------
[Hayes Accura56K ExtDataFax -CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=138
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=56000
MAXCONNECTBPS=57600

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=56000

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
;--------------------------------
[Hayes Accura56K IntDataFax -CTX]
ALIAS=Hayes Accura56K ExtDataFax -CTX

;--------------------------------
[Hayes Accura56K ExtFxVoice -CTX]
ALIAS=Hayes Accura56K ExtDataFax -CTX

;--------------------------------
[Hayes Accura56K IntFxVoice -CTX]
ALIAS=Hayes Accura56K ExtDataFax -CTX

;--------------------------------
[Hayes Accura 56K PCMCIA - CTX]
ALIAS=Hayes Accura56K ExtDataFax -CTX

;--------------------------------
[Hayes Century 336 - CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=33600

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Century 2 336 - CTX]
ALIAS=Hayes Century 336 - CTX

;--------------------------------
[Hayes Optima 33600 PCMCIA - CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Optima 336 Business - CTX]
ALIAS=Hayes Century 336 - CTX

;--------------------------------
[Hayes Optima 56K Business - CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=56000
MAXCONNECTBPS=57600

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=56000

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Optima 336R LineCard -CTX]
ALIAS=Hayes Century 336 - CTX

;--------------------------------
[Hayes Smartmodem 1200 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=1200
MAXCONNECTBPS=1200

COMMAND_INIT=ATE1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Smartmodem 2400 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Smartmodem OPTIMA 2 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT W1 &C1&Q9&S2 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes Smartmodem OPTIMA 9 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 N4 W1 &C1&K3&Q9&S2 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes V-series Smartmodem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=ATE1 V1 X1 S0=0S37=9N1Q0&Q5&K3&C1&S2<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Hayes V-Series ULTRA Smar - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATW1 &C1&D2&S2 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[IBM High Speed Internal/P - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATQ0W1X4 &C1&D2&K3 \\G0\\N3 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Intel 14.4ex Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &D2&S1 \\G0\\J0\\N3\\Q3\\X1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Intel PCMCIA Faxmodem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=ATE1 V1 X4 S0=0 &D2&S1 \\G0\\J0\\N3\\Q3\\X1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Maxwell Modem 2400V from  - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Megahertz 14.4 PCMCIA Dat - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT X4 W1 S0=0 &K3 %C3<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Megahertz 14.4/14.4 FAX/M - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1V1X4 S0=0 \\Q3\\J0\\N3\\X1\\V1 %C1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Megahertz XJACK 28.8 PCMC - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=ATE1 V1 X4 S0=0 &D2&S1 \\G0\\J0\\N3\\Q3\\X1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Microcom DeskPort FAST 28 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F S0=0 &C1&D0 %C3 \\G0\\N3\\Q3<cr>
COMMAND_INIT=AT %B28800<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Microcom DeskPort FAST ES - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F S0=0 &C1&D0 %C3 \\G0\\N3<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Microcom QX/4232hs Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&D1 %C3 \\G0\\J0\\N6\\Q4<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Microcom TravelCard FAST  - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F S0=0 &C1&D0 %C3 \\G0\\N3\\Q3<cr>
COMMAND_INIT=AT %B28800<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Microdyne Access Modem (N - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 &F \\Q3 &C1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Motorola Codex 3220 Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 &F&Y0<cr>
COMMAND_INIT=AT &C1&S1 *FL3 S0=0 &W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Motorola Codex 326X Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 &C1&S1 *FL3 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Motorola Life Style V.34  - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT &C1 \\Q3 \\V4 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Motorola VoiceSURFR 33.6 - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Copyright (c) 1995 SSC,

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1  \\N0 %C0 S0=0 S2=128 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAP-M<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAP-M<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>

;--------------------------------
[Motorola VoiceSURFR 56k - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=56000
MAXCONNECTBPS=115200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=Motorola ModemSURFR 56K Internal
DETECT_RESPONSE=Motorola ModemSURFR 56K External
DETECT_RESPONSE=Motorola VoiceSURFR 56K Internal
DETECT_RESPONSE=Motorola VoiceSURFR 56K External

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1  \\N0 %C0 S0=0 S2=128 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/MNP<cr><lf>

;--------------------------------
[Motorola Power Series V.3 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT &C1 \\Q3 \\V4 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Motorola Premier 33.6 - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=Motorola Premier 33.6 Desktop
DETECT_RESPONSE=Motorola Premier 33.6 Internal

COMMAND_INIT=AT&F1<cr>
COMMAND_INIT=AT&C1&D2 \\V1  \\N0 %C0 S0=0 S2=128 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/MNP<cr><lf>

;--------------------------------
[Motorola UDS CELLect PCMC - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=57600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F<cr>
COMMAND_INIT= AT S0=0 &D2&S1 \\Q3<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Motorola UTA220 V120 64K - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=64000
MAXCONNECTBPS=57600
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<autodial_on>=ATD
<autodial_off>=ATD

DETECT_STRING=ATi<cr>
DETECT_RESPONSE=960
			      
COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 W0 S0=0 %A2=2 %A4=0 %A96=1<cr>
COMMAND_INIT=AT<hwflowcontrol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps><cr><lf>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Motorola UTA220 V120 56K - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=64000
MAXCONNECTBPS=57600
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<autodial_on>=ATD
<autodial_off>=ATD

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=960
			      
COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 W0 S0=0 %A2=2 %A4=1 %A96=1<cr>
COMMAND_INIT=AT<hwflowcontrol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps><cr><lf>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultTech ComPlte MT5634HD8 -CTX]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=&Q5
<protocol_off>=&Q6
<autodial_on>=ATX1D
<autodial_off>=ATX1D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=56000
MAXCONNECTBPS=115200

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=MT5634HD8
COMMAND_INIT=AT &F E1<cr>
COMMAND_INIT=AT &S0<cr>
COMMAND_INIT=AT S0=1 <cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;--------------------------------
[MultTech ComPlte MT3334HD8 -CTX]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=&Q5
<protocol_off>=&Q6
<autodial_on>=ATX1D
<autodial_off>=ATX1D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=MT5634HD8
COMMAND_INIT=AT &F E1<cr>
COMMAND_INIT=AT &S0<cr>
COMMAND_INIT=AT S0=1 <cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;--------------------------------
[MultiTech LT PCMCIA MT143 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0 &E7&E13<cr>
COMMAND_INIT=AT $BA0$MB14400$SB38400$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech LT PCMCIA MT283 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0 &E7&E13<cr>
COMMAND_INIT=AT $BA0$MB28800$SB115200$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech MT1432BR/MT932B - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0 &C1&D0&E1&E4&E13&E15&Q0&S1<cr>
COMMAND_INIT=AT $BA0$MB14400$SB19200$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech MT1432MR/MRI/MR - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0 &C1&D0&E1&E4&E13&E15&Q0&S1<cr>
COMMAND_INIT=AT $BA0$MB14400$SB19200$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech MT1432MU - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0 &E7&E13<cr>
COMMAND_INIT=AT $BA0$MB14400$SB19200$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech MT1932BL/ZDX - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0 &E7&E13<cr>
COMMAND_INIT=AT $BA0$MB19200$SB19200$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech MT2834BA - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT X4 S0=0 &E7&E13<cr>
COMMAND_INIT=AT $BA0$MB28800$SB115200$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech MT2834ZDX 28.8  - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT X4 S0=0 &E7&E13<cr>
COMMAND_INIT=AT $BA0$MB28800$SB115200$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech MultiModem224 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultiTech MultiModemV32 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1V1X1S0=0 &E1&E4&E13&E15 $BA0$MB9600$SB19200$R1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[MultTech MultiModem MT2834 -CTX]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&E4
<hwflowcontrol_off>=&E3
<compression_on>=&E15
<compression_off>=&E14
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=57600
MAXCONNECTBPS=57600

DETECT_STRING=ATI2<cr>
DETECT_RESPONSE=MT2834BA

COMMAND_INIT=AT &F E1<CR>
COMMAND_INIT=AT &SF1 &S0 S36=1 S37=2<cr>
COMMAND_INIT=AT R0 &E6 &E8 &E10 &E13 $E0 $BA0<cr>
COMMAND_INIT=AT &C1 &D2 V1 Q0 X4 &Q0 S0=0 S7=55 S2=128 S13=128<cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;--------------------------------
[MultTech MultiMdm MT2834MR -CTX]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&E4
<hwflowcontrol_off>=&E3
<compression_on>=&E15
<compression_off>=&E14
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200

DETECT_STRING=ATI2<cr>
DETECT_RESPONSE=MT2834MR

COMMAND_INIT=AT &F E1<CR>
COMMAND_INIT=AT &SF1 &S0 S36=4 S37=5 $SB115200<cr>
COMMAND_INIT=AT $R1 &E6 &E8 &E10 &E13 $E0 $BA0<cr>
COMMAND_INIT=AT &C1 &D2 V1 Q0 X4 &Q0 S0=0 S7=55 S13=0<cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;--------------------------------
[MultTech MultMdm MT5600ZDX -CTX]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=&E15
<compression_off>=&E14
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=56000
MAXCONNECTBPS=115200

DETECT_STRING=ATI2<cr>
DETECT_RESPONSE=MT56000ZDX
COMMAND_INIT=AT &F E1<cr>
COMMAND_INIT=AT &SF1 &S0<cr>
COMMAND_INIT=AT &C1 V1 &D2 &Q0 X4 &S0 S0=0 <cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;--------------------------------
[Octocom OSI 8596 and 8596 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&E1&I1&K2&R0 %H3%I1%S0 *E1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Okidata Okitel 2400 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0 &T5<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[PIICEON PCMCIA Dispatcher - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=57600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT W1 &C1&K3&R1 %C3 \\N3<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Practical Modem 2400 SA - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 &C1&D1 V1 X1 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Practical Peripherals 144 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&K1&Q9&S2<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Practical Peripherals 960 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&K3&Q9&S1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Practical P 336B Data/Fax - CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=138
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Practical P 33600 PCMCIA - CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Pract P 56K ExtVoice w/Key -CTX]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=138
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=56000
MAXCONNECTBPS=57600

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=56000

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=12<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Practical P 56K ExtDataFax -CTX]
alias= Pract P 56K ExtVoice w/Key -CTX

;--------------------------------
[Practical P 56K IntDataFax -CTX]
alias= Pract P 56K ExtVoice w/Key -CTX

;--------------------------------
[Practical P 56K Int Voice - CTX]
alias= Pract P 56K ExtVoice w/Key -CTX

;--------------------------------
[Practical P PC336LCD - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=0
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 DT

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PC33600LCD

COMMAND_INIT=AT&F&C1&D2 V1 W1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Practical P PM336MT v7.x - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=%C0"H0
<compression_on>=%C1"H3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 DT

;DETECT_STRING=ATI3<cr>
;DETECT_RESPONSE=PM336MT

COMMAND_INIT=AT&F&C1&D2 V1 W1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Prctical P PM56KMT V10.2.3 -CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=57333
MAXCONNECTBPS=57600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H1&R2
<hwflowcontrol_off>=&H0&R1
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=5600

COMMAND_INIT=AT&F1&C1&D2&A1 V1 E1 L1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker>&B1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;--------------------------------
[Practical PractiCARD 144 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT W1 &C1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[QuikKomm Modem 2400 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 &C1 V1 X1 S0=0 &T5<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Racal-Datacom ALM 3223 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT \\Q1\\X0 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Racal-Datacom ALM 3226 Ce - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT W1 S0=0 &C1<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Racal-Datacom ALM 3239 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT \\Q1\\X0 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Racal-Datacom RMD 3232 Mo - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT &C1 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Scout PCMCIA V.32 14,400  - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0 <cr>
COMMAND_INIT=AT<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Scout ScoutPlus V.32bis 1 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT S0=0 &B2 *F3*M2*S1<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Spartan 9600 MNP5/V.42 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X1 S0=0 \\Q3 \\N6<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Supra 14.4 Data/Fax Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F2<cr>
COMMAND_INIT=AT &C1 W1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Supra 28.8 Data/Fax Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F2<cr>
COMMAND_INIT=AT &C1 W1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Telebit QBlazer Plus - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT X4 S0=0 S58=2 S68=255 S180=2 S190=1<cr>
COMMAND_INIT=AT S255=0 &W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Telebit T1600 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 &F9 S0=0 S51=5<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Telebit T2000 and TrailBl - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 S0=0 S7=40 S50=254 S51=5 S52=1 S58=2 S66=1 S67=0 S68=2 S94=1 S95=2 S96=1 S131=1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Telenetics TC 1442L/1442  - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATW1 S0=0 &C1&K1&R0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Toshiba Noteworthy T144NW - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATW1 S0=0 &C1&R0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[TWINCOM 144/DF Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&K3&Q9 \\N3 %C1%E1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[UDS Fast Talk V.32/42B - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1V1X4S0=0 &C1&S1 %B9600%C1 \\D1\\G\\J\\M1\\N7\\Q3\\R1\\T\\V\\X<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[UDS FasTalk II  14.4 V.32 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F2<cr>
COMMAND_INIT=AT S0=0 &C1&D2 \\Q3\\V1\\X1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[UDS FastTalk 32bx - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATH3 S0=0 &C1&D2&S1 \\Q3\\X1<cr>
COMMAND_INIT=AT&W<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[UDS V.3229/V.3229L Modem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT &C1 \\Q3 \\V1 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Universal Data Systems V. - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=ATE1 V1 X4 S0=0 &C1&R&S1<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USRobotics COURIER 2400 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1 V1 X1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USRobotics COURIER Dual S - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 S15=8 B0 &A3&B1&C1&H1&M4&N0&R2<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USRobotics COURIER HST - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=ATE1 V1 X4 S0=0 &B1&H1&I0&R2<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USRobotics COURIER HST Du - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 S15=8 B0 &A3&B1&C1&H1&M4&N0&R2<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USR Courier V.Everything - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&R2&H1
<hwflowcontrol_off>=&R1&H0
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4 
<protocol_off>=&M0 
<autodial_on>=ATDT
<autodial_off>=ATD


DETECT_STRING=ATI3<cr><cr>
DETECT_RESPONSE=Courier V.Everything
DETECT_RESPONSE=00:00:00
DETECT_STRING=ATI4<cr><cr>
DETECT_RESPONSE=Courier V.Everything
DETECT_STRING=ATI6<cr><cr>
DETECT_RESPONSE=Courier V.Everything
DETECT_STRING=ATI7<cr><cr>
DETECT_RESPONSE=Courier V.Everything
DETECT_RESPONSE=Options                V32bis,Terbo,V.FC,V.34<cr>
DETECT_RESPONSE=Options                HST,V32bis,Terbo,V.FC,V.34<cr>
DETECT_RESPONSE=Options                HST,V32bis,Terbo,VFC,V.34+<cr>

COMMAND_INIT=AT&FX4B0E1V1Q0S0=0<cr>
COMMAND_INIT=AT&A1&B1S2=128S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;--------------------------------
[USR Courier V.Every PCMCIA -CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&R2&H1
<hwflowcontrol_off>=&R1&H0
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4 
<protocol_off>=&M0 
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr><cr>
DETECT_RESPONSE=Courier V.Everything PCMCIA
DETECT_RESPONSE=Courier 28800
DETECT_RESPONSE=00:00:00
DETECT_STRING=ATI4<cr><cr>
DETECT_RESPONSE=Courier V.Everything PCMCIA
DETECT_RESPONSE=Courier PCMCIA V.34
DETECT_STRING=ATI6<cr><cr>
DETECT_RESPONSE=Courier V.Everything PCMCIA
DETECT_RESPONSE=Courier PCMCIA V.34
DETECT_STRING=ATI7<cr><cr>
DETECT_RESPONSE=Courier V.Everything PCMCIA
DETECT_RESPONSE=Courier PCMCIA V.34
DETECT_RESPONSE=Options                V32bis,Terbo,V.FC,V.34<cr>
DETECT_RESPONSE=Options                HST,V32bis,Terbo,V.FC,V.34<cr>
DETECT_RESPONSE=Options                HST,V32bis,Terbo,VFC,V.34+<cr>
DETECT_RESPONSE=Product type           US/Canada PCMCIA 

COMMAND_INIT=AT&FX4B0E1V1Q0S0=0<cr>
COMMAND_INIT=AT&A1&B1S2=128S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;--------------------------------
[USRobotics Dual Analog Mo - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 &B1&H1&I0&R2<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USRobotics Sportster 14.4 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F &A3&B1&H1&K3&R2 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USRobotics Sportster 28.8 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=ATE1 V1 X4 S0=0 S15=8 B0 &A3&B1&C1&H1&M4&N0&R2<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USRobotics Sportster 9600 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F &A3&B1&H1&K3&R2 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[USRobotics Sportster 33600 -CTX]
ALIAS=USRobotics Sportster V.34 - CTX
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=USRobotics Sportster 33600 Fax
DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=USRobotics Sportster 33600 Fax
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=USRobotics Sportster 33600 Fax

;--------------------------------
[USRobotics Sportster V.34 - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H1&R2
<hwflowcontrol_off>=&H0&R1
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Sportster 28800
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=Sportster 28800 V.34 
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=Sportster 28800 V.34
DETECT_STRING=ATI7<cr>
DETECT_RESPONSE=Sportster 28800 V.34

COMMAND_INIT=AT&FX4B0E1V1Q0S0=0<cr>
COMMAND_INIT=AT&A1&B1S2=128S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker>&B1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;--------------------------------
[USR Sportster V.34 PCMCIA - CTX]
ALIAS=USRobotics Sportster V.34 - CTX
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Sportster 28800
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=Sportster PCMCIA V.34 
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=Sportster PCMCIA V.34
DETECT_STRING=ATI7<cr>
DETECT_RESPONSE=Sportster PCMCIA V.34
DETECT_RESPONSE=Product type           US/Canada PCMCIA 

;--------------------------------
[USR Sprtster Vi 33600 DSVD -CTX]
ALIAS=USR Sprtster Vi 28800 DSVD -CTX
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=Sportster Vi 33600 DSVD FAX
DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=Sportster Vi 33600 DSVD FAX
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=Sportster Vi 33600 DSVD FAX

;--------------------------------
[USR Sprtster Vi 28800 DSVD -CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=57600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H1&R2
<hwflowcontrol_off>=&H0&R1
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Sportster Vi 28800 DSVD FAX
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=Sportster Vi 28800 DSVD FAX
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=Sportster Vi 28800 DSVD FAX
DETECT_STRING=ATI7<cr>
DETECT_RESPONSE=Sportster Vi 28800 DSVD FAX

COMMAND_INIT=AT&FX4B0E1V1Q0S0=0<cr>
COMMAND_INIT=AT&A1&B1S2=128S7=55-SSE=1<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker>&B1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;--------------------------------
[USR Sportster Vi 33600 - CTX]
ALIAS=USRobotics Sportster V.34 - CTX
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=USRobotics Sportster Vi 33600 Fax
DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=USRobotics Sportster Vi 33600 Fax
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=USRobotics Sportster Vi 33600 Fax

;--------------------------------
[USR Total Control MP V.34 - CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&R2&H1
<hwflowcontrol_off>=&R1&H0
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4 
<protocol_off>=&M0 
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI7<cr><cr>
DETECT_RESPONSE=Options                V32bis,Terbo,V.FC,V.34<cr>
DETECT_RESPONSE=Options                HST,V32bis,Terbo,V.FC,V.34<cr>

COMMAND_INIT=AT&FX4B0E1V1Q0S0=0<cr>
COMMAND_INIT=AT&A1&B1S2=128S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;--------------------------------
[USR Ttl Contrl NetSrvr V34 -CTX]
ALIAS=USR Total Control MP V.34 - CTX
DETECT_STRING=ATI7<cr><cr>

;--------------------------------
[USR Total Contrl Quad V.34 -CTX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=33600
MAXCONNECTBPS=115200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&R2&H1
<hwflowcontrol_off>=&R1&H0
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4 
<protocol_off>=&M0 
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr><cr>
DETECT_RESPONSE=00:00:00
DETECT_STRING=ATI4<cr><cr>
DETECT_RESPONSE=USRobotics Analog/Digital Quad V.32bis V.34+
DETECT_STRING=ATI6<cr><cr>
DETECT_RESPONSE=USRobotics Analog/Digital Quad V.32bis V.34+
DETECT_STRING=ATI7<cr><cr>
DETECT_RESPONSE=Options                V32bis,Terbo,V.FC,V.34+<cr>
DETECT_RESPONSE=Options                V32bis,Terbo,V.FC,V.34<cr>

COMMAND_INIT=AT&FX4B0E1V1Q0S0=0<cr>
COMMAND_INIT=AT&A1&B1S2=128S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;--------------------------------
[USRobotics WorldPort 14.4 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT X7 S0=0 &B1&H1&R2<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[ViVa Modem 24 - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATE1V1X1 &C1&S1 S0=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[ZOOM 14400 V.32bis FaxMod - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATW1 &C1&D2 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[ZOOM 28800 V.34X FaxModem - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATW1 &C1&D2 S0=0<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Zypcom Z32b-SX Series Dat - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F1<cr>
COMMAND_INIT=AT S0=0 &C1<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Zypcom Z32t-SX Series Dat - CTX]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F1<cr>
COMMAND_INIT=AT S0=0 &C1<cr>
COMMAND_INIT=AT&W0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Zoltrix288 RC288Dpi Rev 04BC]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F&C1&D2W2S46=136%C0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Pract Per PC288LCD V.34]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=0
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 DT

COMMAND_INIT=AT&f3 V1 W1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------
[Pract Perf PM288MT II V.34]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=0
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 DT

COMMAND_INIT=AT&C1&D1&K3 V1 W1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

