    ©Copyright 2003-2004 Marvell®.
    All rights reserved

    SetupYukonWin.htm created 16-Apr-2004

    Readme File for SETUPYUKONWIN.exe v6.36
    Marvell Yukon Gigabit Ethernet Adapter Family

# This file contains

1 Overview
2 Required Files
3 Installation Instructions
4 Silent Installation
5 Troubleshooting

## 1 Overview

    The Miniport Driver installation package contains the Marvell 32-bit
    Miniport driver for the Marvell Yukon Gigabit Ethernet Adapter Family.

    This README file explains how to install the Miniport Driver Package on a
    machine running Windows 98 SE, Windows ME, Windows NT 4.0, Windows 2000,
    Windows XP and Windows Server 2003.

## 2 Required Files

    To install the Miniport Driver, the following file is required:

        SetupYukonWin.exe

## 3 Installation Instructions

    With PCI adapters, due to the plug & play facility of PCI, Windows is
    able to find, identify and configure the adapter automatically. Cancel
    all the operating system attempts to install the drive automatically.

    NOTE:
       To install the driver make sure that you are logged in as a user with
    administrative rights.

    To install the Miniport Driver, proceed as follows:

    1. Execute the setup file SetupYukonWin.exe .

    2. Follow the instructions of the installation procedure.

## 4 Silent Installation

    In order to install the driver silently following commands line should be
    executed:

    - for installation:

    SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    REBOOT=ReallySuppress/qn"

    - for driver removal:

    SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log REMOVE=ALL
    REBOOT=ReallySuppress /qn"

    - for driver repair:

    SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    REINSTALLMODE=vomus REINSTALL=ALL REBOOT=ReallySuppress /qn"

    On Windows 98 SE/ME it is recommended to use "REBOOT=Force" instead of
    "REBOOT=ReallySupress" because each drive installation is completed after
    reboot.

    By default destination directory is %PROGRAMFILES%\Marvell\Miniport
    Driver.

    This can be changed by setting INSTALLDIR variable .

    For example :

    SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    INSTALLDIR=C:\MyDir REBOOT=ReallySuppress/qn"

    The installation status is logged in the file %WINDIR%\YukonInstall.log .

    The log file path can be changed replacing %WINDIR%\YukonInstall.log with
    the preferred file path.

    NOTE:
      Silent installation is not supported for Windows NT4.

## 5 Troubleshooting

    If you should encounter any problems with your Miniport Driver Package,
    please re-read the instructions above and the documentation supplied with
    the operating system carefully.
    Additionally refer to your system event log file (using the Event Viewer)
    and check it for entries from Marvell Miniport Driver.

    If your particular problem is not listed or the error persists, please
    send your system event log file or at least the event id number and the
    logging data (as WORDs) of the entries made by Marvell Miniport Driver to our
    technical support.

    For further information please contact support.
    *** End of Readme File ***