; yukonw9x.inf created 17-Mar-2004
;
; Marvell Yukon Gigabit Ethernet Adapter
;
; (C)Copyright 2002-2004 Marvell(R).
; 
; All rights reserved
;
; INF File for NDIS5 Miniport Driver for Windows ME and 98SE YUKONW9X.sys v6.36

[Version]
Signature	= "$Chicago$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %Marvell%
DriverVer=03/17/2004, 6.36.0.0

[Manufacturer]
%Marvell%	= Marvell


[ControlFlags]

ExcludeFromSelect	= *

[Marvell]

%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_012111AB
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_032111AB
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_102111AB
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_952111AB
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_502111AB

%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_811A1043
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_173C1043
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_80011019
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0F381019
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_004715D4
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1406147B
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_E0001458
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_90251695
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0C19105B
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1C0317F2
%Yukon.DeviceDesc% = SingleV2Copper.ndi, PCI\VEN_11AB&DEV_4320






;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Version 2.0 Copper>

[SingleV2Copper.ndi]
AddReg		= yukonw9x.reg, yukonw9x.params, yukonw9x.Copper.params, yukonw9x.V2.Copper.params 
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yukonw9x.CopyFiles

[SingleV2Copper.ndi.Services]
AddService	= yukonw9x, 2, yukonw9x.Service, common.EventLog






;-------------------------------------------------------------------------------
; General Driver Parameters
;
[yukonw9x.params]
HKR, Ndi\Params\NetworkAddress,	Flag, 1,20,0,0,0
HKR, Ndi\Params\MaxFrameSize,	Flag, 1,20,0,0,0
HKR, Ndi\Params\Moderate,	Flag, 1,20,0,0,0
HKR, Ndi\Params\FixedIntMod,	Flag, 1,20,0,0,0
HKR, Ndi\Params\MaxReceives,	Flag, 1,20,0,0,0
HKR, Ndi\Params\MaxTransmits,	Flag, 1,20,0,0,0

HKR, Ndi\Params\NetworkAddress,	ParamDesc,,	%NetAddress%
HKR, Ndi\Params\NetworkAddress,	Type,,		"edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,,	"18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,,	"1"
HKR, Ndi\Params\NetworkAddress,	Default,,	""
HKR, Ndi\Params\NetworkAddress,	Optional,,	"1"

HKR, Ndi\Params\MaxFrameSize,	ParamDesc,,	%MaxFrSize%
HKR, Ndi\Params\MaxFrameSize,	Type,,		"int"
HKR, Ndi\Params\MaxFrameSize,	Base,,		"10"
HKR, Ndi\Params\MaxFrameSize,	Min,,		"12"
HKR, Ndi\Params\MaxFrameSize,	Max,,		"9014"
HKR, Ndi\Params\MaxFrameSize,	Step,,		"1"
HKR, Ndi\Params\MaxFrameSize,	Default,,	"1514"


HKR, Ndi\Params\Moderate,	ParamDesc,,	%IntMod%
HKR, Ndi\Params\Moderate,	Type,,		"enum"
HKR, Ndi\Params\Moderate\enum,1,,		%On%
HKR, Ndi\Params\Moderate\enum,0,,		%Off%
HKR, Ndi\Params\Moderate,	Default,,	"1"

HKR, Ndi\Params\FixedIntMod,	ParamDesc,,	%MaxIrq%
HKR, Ndi\Params\FixedIntMod,	Type,,		"int"
HKR, Ndi\Params\FixedIntMod,	Base,,		"10"
HKR, Ndi\Params\FixedIntMod,	Min,,		"1000"
HKR, Ndi\Params\FixedIntMod,	Max,,		"30000"
HKR, Ndi\Params\FixedIntMod,	Step,,		"1"
HKR, Ndi\Params\FixedIntMod,	Default,,	"5000"


HKR, Ndi\Params\MaxReceives,	ParamDesc,,	%NumRcv%
HKR, Ndi\Params\MaxReceives,	Type,,		"int"
HKR, Ndi\Params\MaxReceives,	Base,,		"10"
HKR, Ndi\Params\MaxReceives,	Min,,		"3"
HKR, Ndi\Params\MaxReceives,	Max,,		"500"
HKR, Ndi\Params\MaxReceives,	Step,,		"1"
HKR, Ndi\Params\MaxReceives,	Default,,	"50"

HKR, Ndi\Params\MaxTransmits,	ParamDesc,,	%NumTx%
HKR, Ndi\Params\MaxTransmits,	Type,,		"int"
HKR, Ndi\Params\MaxTransmits,	Base,,		"10"
HKR, Ndi\Params\MaxTransmits,	Min,,		"4"
HKR, Ndi\Params\MaxTransmits,	Max,,		"200"
HKR, Ndi\Params\MaxTransmits,	Step,,		"1"
HKR, Ndi\Params\MaxTransmits,	Default,,	"50"




;No QoS Support under W9X

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"

HKR,, MessageLog,,           "4"

;-------------------------------------------------------------------------------
; Additional Driver Parameters for Single Link Copper Adapters
;
 [yukonw9x.Copper.params]
;
; Configurable Parameters
;


;-------------------------------------------------------------------------------
; Additional Driver Parameters for Version 2.0 Copper Adapters
;
[yukonw9x.V2.Copper.params]
;
; Configurable Parameters
;
HKR, Ndi\Params\WakeUpModeCap_A,	Flag, 1,20,0,0,0
HKR, Ndi\Params\Speed_A,	        Flag, 1,20,0,0,0
HKR,Ndi\Params\ConnectionType_A,        Flag, 1,20,00,00,00

HKR, Ndi\Params\WakeUpModeCap_A,       ParamDesc,,	%WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,       type,,		"enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  0,,		"None"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  15,,		"OS Controlled"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  25,,		"Magic Packet"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  26,,		"Pattern Match"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  27,,		"Magic Packet and Pattern Match"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  28,,		"Link Change"
HKR, Ndi\Params\WakeUpModeCap_A, Default,,		"27"

HKR,Ndi\Params\ConnectionType_A,      ParamDesc,  0, %MediaType%
HKR,Ndi\Params\ConnectionType_A,      Type,       0, "enum"
HKR,Ndi\Params\ConnectionType_A,      Default,    0, "0"
HKR,Ndi\Params\ConnectionType_A\enum, "0",        0, %Autosense%
HKR,Ndi\Params\ConnectionType_A\enum, "1",        0, %10MHD%
HKR,Ndi\Params\ConnectionType_A\enum, "2",        0, %10MFD%
HKR,Ndi\Params\ConnectionType_A\enum, "3",        0, %100MHD%
HKR,Ndi\Params\ConnectionType_A\enum, "4",        0, %100MFD%

HKR,, WaitForRxResources,, "0"




;-------------------------------------------------------------------------------
; General Registry Entries
;
[yukonw9x.reg]
HKR, Ndi, HelpText,, %HelpText%
HKR, Ndi\Interfaces, DefUpper,, "ndis5,ndis4,ndis3"
HKR, Ndi\Interfaces, UpperRange,, "ndis5,ndis4,ndis3"
HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "yukonw9x"
HKR,Ndi,DeviceID,,"PCI\VEN_1148&DEV_4300"
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,yukonw9x.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR, NDIS,LogDriverName,,"yukonw9x"
HKR, NDIS,MajorNdisVersion,1,05
HKR, NDIS,MinorNdisVersion,1,00

[yukonw9x.Service]
DisplayName	= %yukonw9x.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\yukonw9x.sys
LoadOrderGroup = NDIS

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\yukonw9x.sys"
HKR,, TypesSupported,	0x00010001, 7

;-------------------------------------------------------------------------------
; Source Files
;
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
yukonw9x.sys	= 1,,

[yukonw9x.CopyFiles]
yukonw9x.sys,,,2



;-------------------------------------------------------------------------------
; Destination Directories
;
[DestinationDirs]

DefaultDestDir = 11
yukonw9x.CopyFiles	= 11


;-------------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
Marvell = "Marvell"
NetAddress              = "Network Address"
MaxFrSize               = "Maximum Frame Size"
WakeUpCaps              = "Wake Up Capabilities"
Speed	                = "LinkSpeed"
IntMod                  = "Interrupt Moderation"
MaxIrq                  = "Max IRQ per Sec"
NumRcv                  = "Number of Receive Buffers"
NumTx                   = "Number of Transmit Buffers"
RlmtPrio		= "Change RLMT Broadcast Priority"
RLMT                    = "RLMT Mode"
Link                    = "CLS"             
OtherPort               = "CLP"                  
Segment                 = "CLPSS" 
Preferred               = "Preferred Port"
Sense			= "Auto-Sense"
On                      = "On"
Off                     = "Off"
Non                     = "None"
Err                     = "Errors"
Wrn                     = "Warnings"
Sta                     = "Status Messages"
All                     = "All Messages"
A                       = "A"
B                       = "B"
QoSSupA                 = "802.1p Support Port A"
QoSSupB                 = "802.1p Support Port B"
AutonegA		= "Autonegotiation Port A"
AutonegB		= "Autonegotiation Port B"
DupCapA			= "DuplexCapabilities Port A"
DupCapB			= "DuplexCapabilities Port B"
RoleA			= "Role on Port A"
RoleB			= "Role on Port B"
Slave			= "Slave"
Master			= "Master"
Auto			= "Auto"
both			= "Half and Full Duplex"
full			= "Full Duplex"
half			= "Half Duplex"
FlowCtrlA		= "FlowControl Port A"
FlowCtrlB		= "FlowControl Port B"
bothFC			= "Asymmetrical and Symmetrical Flow Control"
sym			= "Symmetrical Flow Control"
asym			= "Asymmetrical Flow Control"
noFc			= "No Flow Control"
MediaType		= "MediaType"
Autosense		= "AutoSense"
10MHD               	= "10Mbps Half Duplex"
10MFD               	= "10Mbps Full Duplex"
100MHD              	= "100Mbps Half Duplex"
100MFD              	= "100Mbps Full Duplex"



Yukon.DeviceDesc = "Marvell Yukon Gigabit Ethernet 10/100/1000Base-T Adapter, Copper RJ-45"
    


yukonw9x.DriverDesc	= "NDIS5 Miniport Driver for Marvell Yukon Gigabit Ethernet Adapter"

DriverDisk		= "Marvell Yukon Gigabit Ethernet Adapter Installation Disk"

HelpText		= "This Marvell network adapter connects you to the network."


