       -------------------- P R O J . 4 --------------------

    This is Release 4.9.3 of cartographic projection software.

    PLEASE read the following information as well as READMEs in the src
    and nad directories.

    For more information on PROJ.4 maintenance please see the web page at:

      http://www.remotesensing.org/proj
                    or
      http://proj.maptools.org/

       ---------------------------------------------------

    Installation:
    -------------

    FSF's configuration procedure is used to ease installation of the
    PROJ.4 system.

    The default destination path prefix for installed files is /usr/local.
    Results from the installation script will be placed into subdirectories
    bin, include, lib, man/man1 and man/man3.  If this default path prefix
    is proper, then execute:

    	./configure

    If another path prefix is required, then execute:

    	./configure --prefix=/my/path

    In either case, the directory of the prefix path must exist and be
    writable by the installer.

    After executing configure, execute:

    	make
            make install

    The install target will create, if necessary, all required sub-directories.

    Windows Build
    -------------

    PROJ.4 can be built with Microsoft Visual C/C++ using the makefile.vc
    in the PROJ directory.  First edit the PROJ\nmake.opt and modify
    the INSTDIR value at the top to point to the directory where
    the PROJ tree shall be installed. If you want to install into
    C:\PROJ, it can remain unchanged.
    Then use the makefile.vc to build the software:

    eg.
    C:\> cd proj
    C:\PROJ> nmake /f makefile.vc
    C:\PROJ> nmake /f makefile.vc install-all

    Note that you have to have the VC++ environment variables, and path
    setup properly.  This may involve running the VCVARS32.BAT script out
    of the Visual C++ tree.

    The makefile.vc builds proj.exe, proj.dll and proj.lib.

    It should also be possible to build using the Unix instructions
    and Cygwin32, but this hasn't been tested recently.

       ---------------------------------------------------

    Distribution files and format.
    ------------------------------

    Sources are distributed in one or more files.  The principle elements
    of the system are in a compress tar file named `PROJ.4.x.tar.gz' where
    "x" will indicate level.sub-level of the release.  For U.S. users
    interested in NADCON datum shifting procedures, additional files
    containing conversion matricies are distributed with the name
    `PROJ.4.x.y.tar' where y is an uppercase letter starting with "A."
    These supplementary files will contain compressed files and thus
    the tar file is not compressed.

    Interim reports on Rel. 4 proj are available in PostScript form as
    *.ps.gz .  New and old users are strongly recommended to carefully read
    these manuals.  They are supplements and NOT a replacement for the full
    manual OF 90-284 (which new users should also obtain).

       ---------------------------------------------------

    Principle new aspects of system:
    --------------------------------

    ANSI X3.159-1989 C code.  Site must have ANSI C compiler and header files.

    Several method of determining radius from specified ellipsoid.

    Use of initialization files through +init=file:key.  Default projection
    specifications also may be defined in an ASCII file.

    +inv option REMOVED and -I may be used in its place.  Use of invproj
    alias of proj still functions as per Rel.3.

    +ellps=list and +proj=list REMOVED.  Use respective -le and -lp.

    +units= to specify cartesian coordinate system units.  To get list
    use -lu.

    -v added to dump final cartographic parameters employed.

    Addition of computing scale factors and angular distortion added through
    -S option.  Valuable for designing new projection parameter details.

    -V option which verbosely lists projected point characteristics.

    Programmers may use projection library with calls to pj_init,
    pj_fwd, pj_inv and pj_transform.

    Program nad2nad for conversion of data to and from NAD27 and NAD83
    datums.

    Program cs2cs for converting between coordinate systems, with optional
    datum translation.

    -------------------------------------------------------------

    Things currently left undone:
    ----------------------------

    proj_def.dat NOT fully in place.  Needs additional settings for
    many of the projections.  Probably will not be completed until main
    manual rewritten.