Red Hat Linux 7.2: The Official Red Hat Linux Alpha Installation Guide
Prev | Chapter 3. Installing Red Hat Linux | Next

# Firewall Configuration

Red Hat Linux offers firewall protection for enhanced system security. A firewall exists between your computer and the network, and determines which resources on your computer remote users on the network can access. A properly configured firewall can greatly increase the security of your system.

Choose the appropriate security level for your system.

Figure 3-12. Firewall Configuration

High

  If you choose High, your system will not accept connections (other than the default settings) that are not explicitly defined by you. By default, only the following connections are allowed:

  - DNS replies

  - DHCP — so any network interfaces that use DHCP can be properly configured

  If you choose High, your firewall will not allow the following:

  - Active mode FTP (passive mode FTP, used by default in most clients, should still work)

  - IRC DCC file transfers

  - RealAudioTM

  - Remote X Window System clients

  If you are connecting your system to the Internet, but do not plan to run a server, this is the safest choice. If additional services are needed, you can choose Customize to allow specific services through the firewall.

Medium

  If you choose Medium, your firewall will not allow remote machines to have access to certain resources on your system. By default, access to the following resources are not allowed:

  - Ports lower than 1023 — the standard reserved ports, used by most system services, such as FTP, SSH, telnet, and HTTP

  - The NFS server port (2049)

  - The local X Window System display for remote X clients

  - The X Font server port (by default, xfs does not listen on the network, it is disabled in the font server)

  If you want to allow resources such as RealAudioTM, while still blocking access to normal system services, choose Medium. Select Customize to allow specific services through the firewall.

No Firewall

  No firewall provides complete access to your system and does no security checking. Security checking is the disabling of access to certain services. This should only be selected if you are running on a trusted network (not the Internet) or plan to do more firewall configuration later.

Choose Customize to add trusted devices or to allow additional incoming services.

Trusted Devices

  Selecting any of the Trusted Devices allows access to your system for all traffic from that device; it is excluded from the firewall rules. For example, if you are running a local network, but are connected to the Internet via a PPP dialup, you can check eth0 and any traffic coming from your local network will be allowed. Selecting eth0 as trusted means all traffic over the Ethernet is allowed, put the ppp0 interface is still firewalled. If you want to restrict traffic on an interface, leave it unchecked.

  It is not recommended that you make any device that is connected to public networks, such as the Internet, a Trusted Device.

Allow Incoming

  Enabling these options allow the specified services to pass through the firewall. Note, during a workstation installation, the majority of these services are not installed on the system.

  DHCP

    If you allow incoming DHCP queries and replies, you allow any network interface that uses DHCP to determine its IP address. DHCP is normally enabled. If DHCP is not enabled, your computer can no longer get an IP address.

  SSH

    Secure SHell (SSH) is a suite of tools for logging into and executing commands on a remote machine. If you plan to use SSH tools to access your machine through a firewall, enable this option. You need to have the `openssh-server` package installed in order to access your machine remotely, using SSH tools.

  Telnet

    Telnet is a protocol for logging into remote machines. Telnet communications are unencrypted, and provide no security from network snooping. Allowing incoming Telnet access is not recommended. If you do want to allow inbound Telnet access, you will need to install the `telnet-server` package.

  WWW (HTTP)

    The HTTP protocol is used by Apache (and by other Web servers) to serve Web pages. If you plan on making your Web server publicly available, enable this option. This option is not required for viewing pages locally or for developing Web pages. You will need to install the `apache` package if you want to serve Web pages.

  Mail (SMTP)

    If you want to allow incoming mail delivery through your firewall, so that remote hosts can connect directly to your machine to deliver mail, enable this option. You do not need to enable this if you collect your mail from your ISP's server using POP3 or IMAP, or if you use a tool such as fetchmail. Note that an improperly configured SMTP server can allow remote machines to use your server to send spam.

  FTP

    The FTP protocol is used to transfer files between machines on a network. If you plan on making your FTP server publicly available, enable this option. You need to install the `wu-ftpd` (and possibly the `anonftp`) package for this option to be useful.

  Other ports

    You can allow access to ports which are not listed here, by listing them in Other ports field. Use the following format: `port:protocol`. For example, if you want to allow IMAP access through your firewall, you can specify `imap:tcp`. You can also explicitly specify numeric ports; to allow UDP packets on port 1234 through the firewall, enter `1234:udp`. To specify multiple ports, separate them with commas.

Prev | Home | Next
Network Configuration | Up | Language Support Selection