Red Hat Linux 7.2: The Official Red Hat Linux Alpha Installation Guide
Prev |  | Next

# Appendix F. Driver Disks

# Why Do I Need a Driver Disk?

While the Red Hat Linux installation program is loading, you may see a screen that asks you for a driver disk. The driver disk screen is most often seen in three scenarios:

- If you run the installation program in `expert mode`

- If you run the installation program by entering `linux dd` at the `boot:` prompt

- If you run the installation program on a computer which does not have any PCI devices

## So What Is a Driver Disk Anyway?

A driver disk adds support for hardware that is not otherwise supported by the installation program. The driver disk could be produced by Red Hat, it could be a disk you make yourself from drivers found on the Internet, or it could be a disk that a hardware vendor includes with a piece of hardware.

There is no need to use a driver disk unless you need a particular device in order to install Red Hat Linux. Driver disks are most often used for non-standard or very new CD-ROM drives, SCSI adapters, or NICs. These are the only devices used during the installation that might require drivers not included on the Red Hat Linux CD-ROMs (or boot disk, if you created an installation boot disk to begin the install process).

| Note
| If an unsupported device is not needed to install Red Hat Linux on your system, continue with the installation and add support for the new piece of hardware once the installation is complete.

## How Do I Obtain a Driver Disk?

The Red Hat Linux CD-ROM 1 includes a driver disk image (`images/drivers.img`) containing many rarely used drivers. If you suspect that your system may require one of these drivers, you should create the driver disk before beginning your Red Hat Linux installation.

Another option for finding specialized driver disk information is on Red Hat's website at http://www.redhat.com/support/errata under the section called Bug Fixes. Occasionally, popular hardware may be made available after a release of Red Hat Linux that will not work with drivers already in the installation program or included on the driver disk image on the Red Hat Linux CD-ROM 1. In such cases, the Red Hat website may contain a link to a driver disk image.

### Creating a Driver Disk from an Image File

If you have a driver disk image that you need to write to a floppy disk, this can be done from within DOS or Red Hat Linux.

To create a driver disk from a driver disk image using Red Hat Linux:

1. Insert a blank, formatted floppy disk into the first floppy drive.

2. From the same directory containing the driver disk image, such as ``dd.img``, type `dd if=`dd.img` of=/dev/fd0` as root.

To create a driver disk from a driver disk image using DOS:

1. Insert a blank, formatted floppy disk into the a: drive.

2. From the same directory containing the driver disk image, such as ``dd.img``, type `rawrite `dd.img` a:` at the command line.

## Using a Driver Disk During Installation

Having a driver disk is not enough; you must specifically tell the Red Hat Linux installation program to load that driver disk and use it during the installation process.

| Note
| A driver disk is different than a boot disk. If you require a boot disk to begin the Red Hat Linux installation, you will still need to create that floppy and boot from it before using the driver disk. If you do not already have an installation boot disk and your system does not support booting from the CD-ROM, you should create an installation boot disk. For instructions on how make a boot disk, see the section called Making Installation Diskettes in Chapter 1.

Once you have created your driver disk, begin the installation process by booting from the Red Hat Linux CD-ROM 1 (or the installation boot disk). At the `boot:` prompt, enter either `linux expert` or `linux dd`. Refer to the section called Booting the Installation Program in Chapter 3 for details on booting the installation program.

The Red Hat Linux installation program will ask you to insert the driver disk. Once the driver disk is read by the installer, it can apply those drivers to hardware discovered on your system later in the installation process.

Prev | Home | Next
An Introduction to Disk Partitions |  | Additional Resources About Alphas and Linux