  System Time Synchronization? 
 The Question is:
 
I have several vaxes that are not running TCP/IP software.  How can I
 sychronize their time?  These vaxes are running DECnet.
 
 
 The Answer is :
 
  Most commonly, using IP NTP or using DECnet-Plus DTSS.  Most OpenVMS
  systems have a NET-APP-SUP* or UCX license, thus permitting TCP/IP
  Services to be installed and configured.
 
  But at its simplest, DCL task-to-task can be used.  See topic (159)
  for an example.
 
  Please also see the OpenVMS FAQ section on keeping the OpenVMS system
  time synchronized for suggestions, alternatives, and pointers.
 
 Answer written or last revised on  21-OCT-2002 
