  Problems getting DECwindows to start? 
 The Question is:
 
I have a new 4100 running OpenVMS 7.2. I can't get DECWindows running on the
console.  DECWindows does run fine on this system using other Xterms.  In
SRM Ive set the ostype to OpenVMS, the tta0_type to vidio and console to
graphics. The AlphaBIOS routine
s paint the screen with MSwindows, so I'm sure the S3 graphics card is
working fine, but when VMS is booted, the console stays in roll screen mode
and DECWindows doesn't start. Am I missing a device driver? Did I miss
something in the install?
 
----------------------------------- ----------- ------------
PRODUCT                             KIT TYPE    STATE
----------------------------------- ----------- ------------
BRISTOL AXPVMS WINDU42 V4.2         Full LP     Installed
DEC AXPVMS AMDS V7.2                Full LP     Installed
DEC AXPVMS DCE V1.5                 Full LP     Installed
DEC AXPVMS DCOM V1.0                Full LP     Installed
DEC AXPVMS DECNET_PHASE_IV V7.2     Full LP     Installed
DEC AXPVMS DWMOTIF V1.2-5           Full LP     Installed
DEC AXPVMS MACRO64 V1.2             Full LP     Installed
DEC AXPVMS OPENVMS V7.2             Platform    Installed
DEC AXPVMS TCPIP V5.0-9             Full LP     Installed
DEC AXPVMS VMS V7.2                 Oper System Installed
DEC VMS APPDEV V1.0                 Full LP     Installed
DEC VMS NS_NAV_EXPORT V3.3          Full LP     Installed
----------------------------------- ----------- ------------
 
 The Answer is:
 
  Is the available ECO for DECwindows V1.2-5 applied?
 
  Is the WINDOW_SYSTEM system parameter set to 1?   (Set in MODPARAMS.DAT,
  and a subsequent pass of AUTOGEN with FEEDBACK has then been run?)
 
  If so, please contact the Compaq Customer Support Center.
