  PCL Printing? LN17 Landscape, Portrait? 
 The Question is:
 
How do I configure a LN17 to print in landscape?
 
 
 The Answer is:
 
  With the OpenVMS DCPS package installed for Postscript printing (and
  with supported Postscript printers), you can use PRINT qualifiers such
  as: /PARAMETER=(PAGE_ORIENTATION=LANDSCAPE).  This assumes this LN17
  is the Postscript variant.
 
  With a PCL-compatible printing device, the sequences used to control
  portrait and landscape orientation are organized as follows:
 
    Esc &amp; l Ps O
 
  Where Esc is the ASCII escape character, the ampersand character, a
  lowercase l, the selector, and an uppercase O character.  Ps is the
  selector; Ps is the character 0 for Portrait and 1 for Landscape.
  There are no space characters in this sequence.  As with various
  similar mechanisms, these sequences are often case-sensitive.
 
  This sequence assumes a PCL printer, and various LN17 printers use PCL.
 
  For information on printer device control libraries, please see topics
  such as (1020), and see the related referenced topics.
 
  A PCL command reference follows:
 
	--
 
 
 
                                                          PCL Command Summary
 
 
 
 
 
         Table 1:  Commands listed by function
          Command strings are shown separated by spaces for ease in reading.
        _____________________________________________________________________
          Duplex and Tray Selection
        _____________________________________________________________________
          &lt;esc&gt;&amp; l Ps S   Simplex/duplex mode
                            Ps = 0 Simplex
                            Ps = 1 Duplex, long edge binding
                            Ps = 2 Duplex, short edge binding
          &lt;esc&gt;&amp; a Ps G   Duplex Page Side Selection
                            Ps = 0 Select the next side
                            Ps = 1 Select the front side
                            Ps = 2 Select the back side
          &lt;esc&gt;&amp; l Ps H   Paper Source
                            Ps = 0 Print the current page
                            Ps = 1 Upper tray
                            Ps = 2 Manual Input paper
                            Ps = 3 Manual input envelope
                            Ps = 4 Lower tray
        _____________________________________________________________________
          Sheet size and margins
        _____________________________________________________________________
          &lt;esc&gt;&amp; l Ps A   Page Size
                            Ps = 1  Executive 7.25 x 10.5 inches
                            Ps = 2  Letter 8.5 x 11 inches
                            Ps = 3  Legal 8.5 x 14 inches
                            Ps = 26 A4 210mm x 297mm
                            Ps = 80 Monarch Envelope 3 7/8 x 7 1/2 inches
                            Ps = 81 Commercial Size 10/ 4 1/8 x 9 1/2 inches
                            Ps = 90 International DL 110mm x 220mm
                            Ps = 91 International C5 162mm x 229mm
          &lt;esc&gt;&amp; l Pn P   Page Length
                            Pn = Number of Lines
          &lt;esc&gt;&amp; a Pn L   Left Margin
                            Pn = Column Number
          &lt;esc&gt;&amp; a Pn M   Right Margin
                            Pn = Column Number
          &lt;esc&gt;&amp; 9        Clear Left And Right Margins
          &lt;esc&gt;&amp; l Pn E   Top Margin
                            Pn = Number of Lines
          &lt;esc&gt;&amp; l Pn F   Text Length
                            Pn = Number of Lines
          &lt;esc&gt;&amp; l Ps L   Perforation Region
                            Ps = 0 Disable
                            Ps = 1 Enable
          &lt;esc&gt;&amp; l Pn U   Left Offset Registration
                            Pn = Number of decipoints to shift the logical
                                 page across the width of the physical page.
          &lt;esc&gt;&amp; l Pn Z   Top Offset Registration
                            Pn = Number of decipoints to shift the logical
                                 page down the length of the physical page.
 
                                                            section title  1
 
 
 
  PCL Command Summary
 
 
   Table 1 (Cont.):  Commands listed by function
  _____________________________________________________________________
    Type size and spacing, managing implicit cursor motion
  _____________________________________________________________________
    &lt;esc&gt;&amp; s Ps C   End of line Wrap
                      Ps = 0 Enables end of line wrap
                      Ps = 1 Disables end of line wrap
    &lt;esc&gt;&amp; k Ps G   Line Termination
                      Ps = 0 CR -&gt; CR;   LF -&gt; LF;   FF -&gt; FF
                      Ps = 1 CR -&gt; CRLF; LF -&gt; LF;   FF -&gt; FF
                      Ps = 2 CR -&gt; CR;   LF -&gt; CRLF; FF -&gt; CRFF
                      Ps = 3 CR -&gt; CRLF; LF -&gt; CRLF; FF -&gt; CRFF
    &lt;esc&gt;&amp; k Pn H   Horizontal Motion Index
                      Pn = Number of 1/120 inch increments
    &lt;esc&gt;&amp; l Pn C   Vertical Motion Index
                      Pn = Number of 1/48 inch increments
    &lt;esc&gt;&amp; l Pn D   Line Spacing
                      Pn = 1   Lines Per Inch
                      Pn = 2     "    "    "
                      Pn = 3     "    "    "
                      Pn = 4     "    "    "
                      Pn = 6     "    "    "
                      Pn = 8     "    "    "
                      Pn = 12    "    "    "
                      Pn = 16    "    "    "
                      Pn = 24    "    "    "
                      Pn = 48    "    "    "
    &lt;esc&gt;( s Ps P   Primary Spacing
    &lt;esc&gt;) s Ps P   Secondary Spacing
                      Ps = 0 Fixed Spacing
                      Ps = 1 Proportional Spacing
    &lt;esc&gt;( s Pn H   Primary Pitch
    &lt;esc&gt;) s Pn H   Secondary Pitch
                      Pn = Number of characters per inch
    &lt;esc&gt;) s Pn V   Primary Height
    &lt;esc&gt;) s Pn V   Secondary Height
                      Pn = Height in points
  _____________________________________________________________________
          Font management and attribute selection
  _____________________________________________________________________
    &lt;esc&gt;( s Ps S   Primary Style
    &lt;esc&gt;) s Ps S   Secondary Style
                      Ps = 0 Upright
                      Ps = 1 Italic
    &lt;esc&gt;( s Ps B   Primary Stroke weight
    &lt;esc&gt;) s Ps B   Secondary Stroke weight
                      Ps = -3 Light
                      Ps =  0 Medium or Book
                      Ps = +3 Bold
 
 
 
 
 
 
    2  section title
 
 
 
                                                         PCL Command Summary
 
         Table 1 (Cont.):  Commands listed by function
        _____________________________________________________________________
          Font management and attribute selection (Cont.)
        _____________________________________________________________________
          &lt;esc&gt;&amp; d Ps D   Enable Underline
                            Ps = 0 Fixed Position
                            Ps = 3 Floating Position
          &lt;esc&gt;&amp; d @      Disable Underline
          &lt;esc&gt;( s Ps T   Primary Typeface
          &lt;esc&gt;) s Ps T   Secondary Typeface
                            Ps =  0 Line Printer
                            Ps =  3 Courier
                            Ps =  4 Helvetica
                            Ps =  5 Times-Roman
                            Ps =  6 Letter Gothic
                            Ps =  8 Prestige
                            Ps = 11 Presentation
                            Ps = 45 ITC Zapf Dingbats**
                            Ps = 52 Univers**
    **These typeface names are registered trademarks of a third party
 
          &lt;esc&gt;( 3 @      Default Primary Font Characteristics
          &lt;esc&gt;) 3 @      Default Secondary Font Characteristics
          &lt;esc&gt;* c Pn D   Font ID (This font number used for subsequent
                            actions such as delete, load, make permanent)
                            Pn = Font ID Number
          &lt;esc&gt;* c Ps F   Font Control
                            Ps = 0 Delete All Soft Fonts
                            Ps = 1 Delete All Temporary Soft Fonts
                            Ps = 2 Delete Soft Font (Last ID Specified)
                            Ps = 3 Delete Character Code
                                   (Last Character Code and ID Specified)
                            Ps = 4 Make Soft Font Temporary
                                   (Last ID Specified)
                            Ps = 5 Make Soft Font Permanent
                                   (Last ID Specified)
                            Ps = 6 Copy/Assign Current Invoked Font as
                                   Temporary (Last ID Specified)
          &lt;esc&gt;&amp; p Pn X   Transparent Print Data
                            Pn = Number of Bytes of Transparent Data
          &lt;esc&gt;( Pn X     Font Selection by ID - Primary
          &lt;esc&gt;) Pn X     Font Selection by ID - Secondary
                            Pn = Font ID Number
          &lt;esc&gt;) s Pn W [font descriptor]
                          Font Descriptor Command
                            Pn = Number of bytes in the font descriptor
          &lt;esc&gt;* c Pn E   Character Code Command
                            Pn = Character code, decimal
          &lt;esc&gt;( s Pn W [character descriptor and data]
                          Character Descriptor and Data Command
                            Pn = Number of bytes in the character descriptor
                                 &amp; data
 
 
 
 
                                                            section title  3
 
 
 
  PCL Command Summary
 
   Table 1 (Cont.):  Commands listed by function
  _____________________________________________________________________
    Selecting character sets
  _____________________________________________________________________
      &lt;esc&gt;( Ps       Symbol Set - Primary, Ps = set number
      &lt;esc&gt;) Ps       Symbol Set - Secondary, Ps = set number
 
                Symbol Set Name     Symbol Set Number
                       BarCode 3of9               0Y
                       DeskTop                    7J
                       DownLoad Font n            nX
                       ECMA-94 Latin 1            0N
                       EAN/UPC                    8Y
                       *HP German                 0G
                       HP Legal                   1U
                       HP Line Draw               0B
                       HP Math-7                  0A
                       HP Math-8                  8M
                       HP Pi Font                15U
                       HP Roman-8                 8U
                       *HP Spanish                1S
                       ISO 2 Interntl Refer Vers  2U
                       ISO 4 UK                   1E
                       ISO 6 ASCII                0U
                       ISO 10 Swedish             3S
                       ISO 11 Swedish             0S
                       ISO 14 JIS ASCII           0K
                       ISO 15 Italian             0I
                       ISO 16 Portuguese          4S
                       ISO 17 Spanish             2S
                       ISO 21 German              1G
                       ISO 25 French              0F
                       ISO 57 Chinese             2K
                       ISO 60 Norwegian version 1 0D
                       ISO 61 Norwegian version 2 1D
                       ISO 69 French              1F
                       ISO 84 Portuguese          5S
                       ISO 85 Spanish             6S
                       OCR A                      0O
                       OCR B                      1O
                       PC Line                    4Q
                       PC-8                      10U
                       PC-8 (Danish/Norwegian)   11U
                       PC 850                    12U
                       Z-Bats                    11L
                       ZipCode                   15Y
                     *Not recommended for future use
 
 
 
 
 
 
 
 
 
   4  section title
 
 
 
                                                         PCL Command Summary
 
         Table 1 (Cont.):  Commands listed by function
        _____________________________________________________________________
          Explicit cursor movement
        _____________________________________________________________________
          &lt;esc&gt;&amp; a Pn C   Horizontal Cursor Positioning - Columns
                            Pn = Number of Columns
          &lt;esc&gt;&amp; a Pn H   Horizontal Cursor Positioning - Decipoints
                            Pn = Number of Decipoints (1/720 inch)
          &lt;esc&gt;* p Pn X   Horizontal Cursor Positioning - Dots
                            Pn = Number of Dots
          &lt;esc&gt;&amp; a Pn R   Vertical Cursor Positioning - Rows
                            Pn = Number of Rows
          &lt;esc&gt;&amp; a Pn V   Vertical Cursor Positioning - Decipoints
                            Pn = Number of Decipoints (1/720 inch)
          &lt;esc&gt;* p Pn Y   Vertical Cursor Positioning - Dots
                            Pn = Number of Dots
          &lt;esc&gt;=          Half-Line Feed (down)
          &lt;esc&gt;&amp; f Ps S   Push/Pop Cursor Position
                            Ps = 0 Push (Store Cursor Position)
                            Ps = 1 Pop (Recall Cursor Position)
        _____________________________________________________________________
          Raster Graphics
        _____________________________________________________________________
          &lt;esc&gt;* t Pn R   Raster Graphics Resolution
                            Pn = Dots per inch, 75, 100, 150, or 300.
          &lt;esc&gt;* r Ps F    Raster Graphics Presentation Mode
                            Ps = 0 Raster Graphics will be printed in the
                                   orientation of the logical page.
                            Ps = 3 Raster Graphics will be printed along the
                                   width of the physical page, regardless of
                                   logical page orientation.
          &lt;esc&gt;* b Ps M   Set Compression Mode
                            PS = 0 Not Encoded (Binary)
                            PS = 1 Run Length Encoding
                            PS = 2 Tagged Image File Format
          &lt;esc&gt;* r Ps A   Start Raster Graphics
                            Ps = 0 Left graphics margin is x-position 0
                            Ps = 1 Left graphics margin is current x-position
          &lt;esc&gt;* b Pn W [raster data]
                          Transfer Raster Data
                             Pn = Number of bytes in the raster row.
          &lt;esc&gt;* r B      End Raster Graphics
 
 
 
 
 
 
 
 
 
 
 
 
 
 
                                                            section title  5
 
 
 
  PCL Command Summary
 
   Table 1 (Cont.):  Commands listed by function
  _____________________________________________________________________
    Rectangles
  _____________________________________________________________________
    &lt;esc&gt;* c Pn H   Horizontal Rectangle Size - Decipoints
                      Pn = Number of Decipoints
    &lt;esc&gt;* c Pn A   Horizontal Rectangle Size - Dots
                      Pn = Number of Dots
    &lt;esc&gt;* c Pn V   Vertical Rectangle Size - Decipoints
                      Pn = Number of Decipoints
    &lt;esc&gt;* c Pn B   Vertical Rectangle Size - Dots
                      Pn = Number of Dots
    &lt;esc&gt;* c Ps P   Fill Rectangle Area
                      Ps = 0 Solid Fill
                      Ps = 2 Shaded Fill
                      Ps = 3 HP defined pattern fill
    &lt;esc&gt;* c Ps G   Area Fill Id
                      Ps = 1 - 6 Pattern number to use for fill
                      Ps = 1 - 100 level of shading to use for fill.
 _____________________________________________________________________
   Macros
 _____________________________________________________________________
    &lt;esc&gt;&amp; f Pn Y   Macro ID (This number used for subsequent macro
                              commands)
                      Pn = Macro ID number
    &lt;esc&gt;&amp; f Ps X   Macro Control (Use Last ID Specified)
                      Ps = 0 Start macro definition
                      Ps = 1 Stop macro definition
                      Ps = 2 Execute macro
                      Ps = 3 Call macro
                      Ps = 4 Enable macro for automatic overlay
                      Ps = 5 Disable automatic overlay
                      Ps = 6 Delete all macros
                      Ps = 7 Delete all temporary macros
                      Ps = 8 Delete macro (Last ID Specified)
                      Ps = 9 Make macro temporary
                      Ps = 10 Make macro permanent
  _____________________________________________________________________
    Miscellaneous
  _____________________________________________________________________
    &lt;esc&gt;&amp; l Pn X   Number of Copies
                      Pn = the number
    &lt;esc&gt;&amp; l Ps O   Orientation
                      Ps = 0 Portrait
                      Ps = 1 Landscape
    &lt;esc&gt; Y         Enables Display Functions Mode
    &lt;esc&gt; Z         Disables Display Functions Mode
 
 
 
 
 
 
 
 
 
   6  section title
 
 
 
                                                         PCL Command Summary
 
         Table 1 (Cont.):  Commands listed by function
        _____________________________________________________________________
          Resets and Emulation Mode Changes
        _____________________________________________________________________
          &lt;esc&gt;E          Reset
          &lt;esc&gt;@          Emulation Mode Reset
          &lt;esc&gt;% @        Return to DEC mode
          &lt;esc&gt;[ ? 58 l   DECIPEM
          &lt;esc&gt;[ ! p      DECSTR
          &lt;esc&gt;%&gt;         LJ11 mode
          &lt;esc&gt;%8         LJ11D mode
          &lt;esc&gt;%?         LJ11P mode
          &lt;esc&gt;%=         X24E mode
          &lt;esc&gt;[?58h      X24E mode
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
                                                            section title  7
 
 
 
  PCL Command Summary
 
  Commands in Alphabetical Order by Final Character
  _____________________________________________________________________
 
   Table 2:  ESC Sequences Sorted by Final Character
  _____________________________________________________________________
    Coding           Name
  _____________________________________________________________________
    &lt;esc&gt;&amp; l Ps A   Page Size
                      Ps = 1  Executive 7.25 x 10.5 inches
                      Ps = 2  Letter 8.5 x 11 inches
                      Ps = 3  Legal 8.5 x 14 inches
                      Ps = 26 A4 210mm x 297mm
                      Ps = 80 Monarch Envelope 3 7/8 x 7 1/2 inches
                      Ps = 81 Commercial Size 10/4 1/8 x 9 1/2 inches
                      Ps = 90 International DL 110mm x 220mm
                      Ps = 91 International C5 162mm x 229mm
    &lt;esc&gt;* c Pn A   Horizontal Rectangle Size - Dots
                      Pn = Number of Dots
    &lt;esc&gt;* r Ps A   Start Raster Graphics
                      Ps = 0 Left graphics margin is x-position 0
                      Ps = 1 Left graphics margin is current x-position
    &lt;esc&gt;( s Ps B   Primary Stroke weight
    &lt;esc&gt;) s Ps B   Secondary Stroke weight
                      Ps = -7 Ultra Thin
                      Ps = -5 Thin
                      Ps = -3 Light
                      Ps =  0 Medium or Book
                      Ps = +3 Bold
                      Ps = +5 Black
                      Ps = +7 Ultra Black
    &lt;esc&gt;* c Pn B   Vertical Rectangle Size - Dots
                      Pn = Number of Dots
    &lt;esc&gt;* r B      End Raster Graphics
    &lt;esc&gt;&amp; a Pn C   Horizontal Cursor Positioning - Columns
                      Pn = Number of Columns
    &lt;esc&gt;&amp; l Pn C   Vertical Motion Index
                      Pn = Number of 1/48 inch increments
    &lt;esc&gt;&amp; s Ps C   End of line Wrap
                      Ps = 0 Enables end of line wrap
                      Ps = 1 Disables end of line wrap
    &lt;esc&gt;&amp; d Ps D   Enable Underline
                      Ps = 0 Fixed Position
                      Ps = 3 Floating Position
    &lt;esc&gt;&amp; l Pn D   Line Spacing
                      Pn = 1   Lines Per Inch
                      Pn = 2     "    "    "
                      Pn = 3     "    "    "
                      Pn = 4     "    "    "
                      Pn = 6     "    "    "
                      Pn = 8     "    "    "
                      Pn = 12    "    "    "
                      Pn = 16    "    "    "
                      Pn = 24    "    "    "
                      Pn = 48    "    "    "
 
 
   8  section title
 
 
 
                                                         PCL Command Summary
 
 
         Table 2 (Cont.):  ESC Sequences Sorted by Final Character
        _____________________________________________________________________
          Coding       Name
        _____________________________________________________________________
          &lt;esc&gt;* c Pn D   Font ID (This font number used for subsequent
                            actions such as delete, load, make permanent)
                            Pn = Font ID Number
          &lt;esc&gt;E          Reset
          &lt;esc&gt;&amp; l Pn E   Top Margin
                            Pn = Number of Lines
          &lt;esc&gt;* c Pn E   Character Code Command
                            Pn = Character code, decimal
          &lt;esc&gt;&amp; l Pn F   Text Length
                            Pn = Number of Lines
          &lt;esc&gt;* c Ps F   Font Control
                            Ps = 0 Delete All Soft Fonts
                            Ps = 1 Delete All Temporary Soft Fonts
                            Ps = 2 Delete Soft Font (Last ID Specified)
                            Ps = 3 Delete Character Code
                                   (Last ID and Character Code Specified)
                            Ps = 4 Make Soft Font Temporary (Last ID Specified)
                            Ps = 5 Make Soft Font Permanent (Last ID Specified)
                            Ps = 6 Copy/Assign Current Invoked Font as
                                   Temporary (Last ID Specified)
          &lt;esc&gt;* r Ps F   Raster Graphics Presentation Mode
                            Ps = 0 Raster Graphics will be printed in the
                                   orientation of the logical page.
                            Ps = 3 Raster Graphics will be printed along the
                                   width of the physical page, regardless of
                                   logical page orientation.
          &lt;esc&gt;&amp; a Ps G   Duplex Page Side Selection
                            Ps = 0 Select the next side
                            Ps = 1 Select the front side
                            Ps = 2 Select the back side
          &lt;esc&gt;&amp; k Ps G   Line Termination
                            Ps = 0 CR -&gt; CR;   LF -&gt; LF;   FF -&gt; FF
                            Ps = 1 CR -&gt; CRLF; LF -&gt; LF;   FF -&gt; FF
                            Ps = 2 CR -&gt; CR;   LF -&gt; CRLF; FF -&gt; CRFF
                            Ps = 3 CR -&gt; CRLF; LF -&gt; CRLF; FF -&gt; CRFF
          &lt;esc&gt;* c Ps G   Area Fill Id
                            Ps = 1 - 6 Pattern number to use for fill
                            Ps = 1 - 100 level of shading to use for fill.
          &lt;esc&gt;&amp; a Pn H   Horizontal Cursor Positioning - Decipoints
                            Pn = Number of Decipoints (1/720 inch)
          &lt;esc&gt;&amp; k Pn H   Horizontal Motion Index
                            Pn = Number of 1/120 inch increments
          &lt;esc&gt;&amp; l Ps H   Paper Source
                            Ps = 0 Print the current page
                            Ps = 1 Upper tray
                            Ps = 2 Manual Input paper
                            Ps = 3 Manual input envelope
                            Ps = 4 Lower tray
                            Ps = 6 Envelope feeder
 
 
                                                            section title  9
 
 
 
  PCL Command Summary
 
   Table 2 (Cont.):  ESC Sequences Sorted by Final Character
  _____________________________________________________________________
    Coding           Name
  _____________________________________________________________________
    &lt;esc&gt;( s Pn H   Primary Pitch
    &lt;esc&gt;) s Pn H   Secondary Pitch
                      Pn = Number of characters per inch
    &lt;esc&gt;* c Pn H   Horizontal Rectangle Size - Decipoints
                      Pn = Number of Decipoints
    &lt;esc&gt;&amp; a Pn L   Left Margin
                      Pn = Column Number
    &lt;esc&gt;&amp; l Ps L   Perforation Region
                      Ps = 0 Disable
                      Ps = 1 Enable
    &lt;esc&gt;&amp; a Pn M   Right Margin
                      Pn = Column Number
    &lt;esc&gt;&amp; l Ps O   Orientation
                      Ps = 0 Portrait
                      Ps = 1 Landscape
    &lt;esc&gt;&amp; l Pn P   Page Length
                      Pn = Number of Lines
    &lt;esc&gt;( s Ps P   Primary Spacing
    &lt;esc&gt;) s Ps P   Secondary Spacing
                      Ps = 0 Fixed Spacing
                      Ps = 1 Proportional Spacing
    &lt;esc&gt;* c Ps P   Fill Rectangle Area
                      Ps = 0 Solid Fill
                      Ps = 2 Shaded Fill
                      Ps = 3 HP defined pattern fill
    &lt;esc&gt;&amp; a Pn R   Vertical Cursor Positioning - Rows
                      Pn = Number of Rows
    &lt;esc&gt;* t Pn R   Raster Graphics Resolution
                      Pn = dots per inch, 75, 100, 150, or 300.
    &lt;esc&gt;&amp; f Ps S   Push/Pop Cursor Position
                      Ps = 0 Push (Store Cursor Position)
                      Ps = 1 Pop (Recall Cursor Position)
    &lt;esc&gt;&amp; l Ps S   Simplex/duplex mode
                      Ps = 0 Simplex
                      Ps = 1 Duplex, long edge binding
                      Ps = 2 Duplex, short edge binding
    &lt;esc&gt;( s Ps S   Primary Style
    &lt;esc&gt;) s Ps S   Secondary Style
                      Ps = 0 Upright
                      Ps = 1 Italic
    &lt;esc&gt;( s Ps T   Primary Typeface
    &lt;esc&gt;) s Ps T   Secondary Typeface
                      Ps =  0 Line Printer
                      Ps =  3 Courier
                      Ps =  4 Helvetica
                      Ps =  5 Times-Roman
                      Ps =  6 Letter Gothic
                      Ps =  8 Prestige
                      Ps = 11 Presentations
                      Ps = 45 ITC Zapf Dingbats**
         **These typeface names are registered trademarks of a third party
 
   10 section title
 
 
                                                          PCL Command Summary
 
 
         Table 2 (Cont.):  ESC Sequences Sorted by Final Character
        _____________________________________________________________________
          Coding       Name
        _____________________________________________________________________
          &lt;esc&gt;&amp; l Pn U   Left Offset Registration
                            Pn = Number of decipoints to shift the logical
                            page across the width of the physical page.
          &lt;esc&gt;&amp; a Pn V   Vertical Cursor Positioning - Decipoints
                            Pn = Number of Decipoints (1/720 inch)
          &lt;esc&gt;) s Pn V   Primary Height
          &lt;esc&gt;) s Pn V   Secondary Pitch
                            Pn = Height in points
          &lt;esc&gt;* c Pn V   Vertical Rectangle Size - Decipoints
                            Pn = Number of Decipoints
          &lt;esc&gt;) s Pn W [font descriptor]  Font Descriptor Command
                            Pn = Number of bytes in the font descriptor
          &lt;esc&gt;( s Pn W [character descriptor and data]
                          Character Descriptor and Data Command
                            Pn = Number of bytes in the character descriptor
                                 &amp; data
          &lt;esc&gt;* b Pn W [raster data]  Transfer Raster Data
                            Pn = Number of bytes in the raster row.
          &lt;esc&gt;&amp; f Ps X   Font Control (Use Last ID Specified)
                            Ps = 0 Start macro definition
                            Ps = 1 Stop macro definition
                            Ps = 2 Execute macro
                            Ps = 3 Call macro
                            Ps = 4 Enable macro for automatic overlay
                            Ps = 5 Disable automatic overlay
                            Ps = 6 Delete all macros
                            Ps = 7 Delete all temporary macros
                            Ps = 8 Delete macro (Last ID Specified)
                            Ps = 9 Make macro temporary
                            Ps = 10 Make macro permanent
          &lt;esc&gt;&amp; l Pn X   Number of copies where Pn is replaced by the number
          &lt;esc&gt;&amp; p Pn X   Transparent Print Data
                            Pn = Number of Bytes of Transparent Data
          &lt;esc&gt;( Pn X     Font Selection by ID - Primary
          &lt;esc&gt;) Pn X     Font Selection by ID - Secondary
                            Pn = Font ID Number
          &lt;esc&gt;* p Pn X   Horizontal Cursor Positioning - Dots
                            Pn = Number of Dots
          &lt;esc&gt; Y         Enables Display Functions Mode
          &lt;esc&gt;&amp; f Pn Y   Macro ID (This number used for subsequent macro
                                    commands)
                            Pn = Macro ID number
          &lt;esc&gt;* p Pn Y   Vertical Cursor Positioning - Dots
                            Pn = Number of Dots
          &lt;esc&gt; Z         Disables Display Functions Mode
          &lt;esc&gt;&amp; l Pn Z   Top Offset Registration
                            Pn = Number of decipoints to shift the logical
                                 page down the length of the physical page.
          &lt;esc&gt;=          Half-Line Feed (down)
          &lt;esc&gt;( 3 @      Default Primary Font Characteristics
          &lt;esc&gt;) 3 @      Default Secondary Font Characteristics
 
                                                            section title 11
 
 
 
  PCL Command Summary
 
   Table 2 (Cont.):  ESC Sequences Sorted by Final Character
  _____________________________________________________________________
    Coding           Name
  _____________________________________________________________________
          &lt;esc&gt;&amp; 9        Clear Left And Right Margins
          &lt;esc&gt;( Ps       Symbol Set - Primary, Ps = set number
          &lt;esc&gt;) Ps       Symbol Set - Secondary, Ps = set number
 
                     Symbol Set Name     Symbol Set Number
                        HP Math-7                  0A
                        HP Line Draw               0B
                        ISO 60 Norwegian version 1 0D
                        ISO 61 Norwegian version 2 1D
                        ISO 4 UK                   1E
                        ISO 25 French              0F
                        ISO 69 French              1F
                        *HP German                 0G
                        ISO 21 German              1G
                        ISO 15 Italian             0I
                        DeskTop                    7J
                        ISO 14 JIS ASCII           0K
                        ISO 57 Chinese             2K
                        Z-Bats                    11L
                        HP Math-8                  8M
                        ECMA-94 Latin 1            0N
                        OCR A                      0O
                        OCR B                      1O
                        PC Line                    4Q
                        Special                    xQ
                        ISO 11 Swedish             0S
                        *HP Spanish                1S
                        ISO 17 Spanish             2S
                        ISO 10 Swedish             3S
                        ISO 16 Portuguese          4S
                        ISO 84 Portuguese          5S
                        ISO 85 Spanish             6S
                        ISO 6 ASCII                0U
                        HP Legal                   1U
                        ISO 2 Interntl Refer Vers  2U
                        HP Roman-8                 8U
                        PC-8                      10U
                        PC-8 (Danish/Norwegian)   11U
                        PC 850                    12U
                        HP Pi Font                15U
                        DownLoad Font n            nX
                        BarCode 3of9               0Y
                        EAN/UPC                    8Y
                        ZipCode                   15Y
                        Reserved                   xY
                     *Not recommended for future use
 
 
 
 
 
 
