  DECnet and multiple controllers? 
 The Question is:
 
I have an Alphastation 500/400 running OpenVMS v7.2-1.  It has two Ethernet
 cards (resolves to EWA-0, EWA-1), each connected to a different network.  I
 need TCP access to both, but I don't want to route my DECnet traffic thru EWA-0.
 
I'm thinking that DECnet is routing thru EWA-0 because I have been experiencing
 some network lag over DECnet.  When I have a remote DECTerm opened on a server
 (display set back to my workstation), I will have several "network" pauses
 each minute.  The ter
m will not repaint, but there is no load on that server.  And the load on my
 workstation is at priority 0.  This lag only started when I fired up the new
 network card.
 
Thanks!
 
 The Answer is :
 
  SET and DEFINE the LINE and the CIRCUIT to STATE OFF, using NCP.
 
 Answer written or last revised on  26-NOV-2001 
