  DCL command negation? SET DEVICE/[NO]SPOOL? 
 The Question is:
 
how do you unspool a printer
 
que name is qclab
 
Thanks Ian
 
 The Answer is :
 
  Please consider using the on-line help (HELP SET DEVICE /SPOOL)
  or the OpenVMS DCL documentation (via the OpenVMS website).
  As is the typical case with OpenVMS, DCL uses [NO] to negate;
  SET DEVICE/NOSPOOL to negate.
 
 Answer written or last revised on  14-JUN-2002 
