  Assistance with Cisco products? 
 The Question is:
 
I am trying to replace our old Vitalink Translans
(which are joined by ISDN circuits) with Cisco routers
using ISDN and transparent bridging (only - no
DECnet routing).  When I try
to load a DEC 200 over the router link the
load never works.  My protocol analyzer shows
that the DEC 200 is responding with the following
error:  Error=Image Data Not Properly Loaded.
It looks like the MOP load server is sending
the same packets twice even though the DEC 200
responds with an Error=No Error message after the
first time the packet is sent.  This DEC 200 loads
fine when on a local segment.  Any help is appreciated.
 
 The Answer is:
 
  Check with Cisco support, checking particularly for any known problems
  they may have.  There was a potentially related Cisco bug -- CSCDI38595
  was the Cisco identifer.  Disabling the LAT compression was a potential
  workaround.
