  Zero error counts? 
 The Question is:
 
Is it possible to clear/reset device error counts. I get regular flagged errors
 fro HSZ controllers due to mirroring operations and this hides genuine error
 increases since the numbers get too big.
 
I want to be able to see genuine large increases in the error count as a way of
 monitoring problems.
 
 The Answer is :
 
  Please review the OpenVMS Frequently Asked Questions (FAQ) for
  some details on this topic.  Alternatively, a copy of the ZDEC tool
  was posted to comp.os.vms within the past few months.
 
  Alternatively, code some DCL using f$getdvi or an application
  using sys$getdvi[w].
 
  And if you have a hardware maintenance contract, predictive hardware
  fault analysis tools are available.
 
 Answer written or last revised on  22-OCT-2001 
