  DECnet channels to network device? (NETACP) 
 The Question is:
 
How do I get NETACP to let go of device EWB1?
 
 The Answer is :
 
  By shutting down the particular DECnet protocol running on EWB1:,
  or (of course) by shutting down the associated line and circuit,
  or by shutting down DECnet.
 
 Answer written or last revised on  2-AUG-2001 
