  DECss7 and X.21 bis (V.35, V.36)? 
 The Question is:
 
Hi,
 
We have a DNBC4 card with DECss7 3.1-8. What are the available cables to
 connect this card ending in V.35 or V.36?
 
Thank you.
 
 The Answer is :
 
  The DNBC4 controller is delivered with a V.35 cable with the part
  number DNBC4-T4.  This cable provides four V.35 connections.
 
  For information on adapting X.21 bis cabling and signalling from
  V.35 to V.36, please contact the customer support center directly
  -- discussions of DECss7, and the related wiring and cabling is
  (well) outside the domain of the OpenVMS Wizard.
 
 Answer written or last revised on  5-MAR-2003 
