  SRM Console Environment Variable? (EWA0_MODE) 
 The Question is:
 
Can I find the value of the Console Variable EWA0_MODE (e.g. AUI or TWISTED
 PAIR)without shutting the system down to the &gt;&gt;&gt; prompt?
Is there a lexical or a SHOW perhaps?
 
 The Answer is :
 
  You can set the mode to what you want on-line, using LANCP.  In LANCP,
  see the SET DEVICE EWA0 command.  The LANCP command SHOW DEVICE can
  be used to display the current settings.
 
  Those Alpha SRM console variables that are accessable via documented
  means are referenced in the f$getenv/sys$getenv call documentation.
 
 Answer written or last revised on  9-OCT-2001 
