  VAXstation console (hardware) error? 
 The Question is:
 
Is this a hardware error, or can I do something to get rid of this error?  I
 can't get Standalone back to work with this error (and therefore can't load
 VMS.)
 
Thanks,
patrick
 
 The Answer is :
 
  This appears to be a console-reported fatal error, though
  there are usually cryptic letter codes included.  What is
  provided is not an OpenVMS error.
 
  This VAXstation offers various console diagnostics and it runs
  some basic diagnostics at power-up; are any errors reported?
 
  OpenVMS V7.1-2 is only available for OpenVMS Alph, thus the
  OpenVMS Wizard will assume this is OpenVMS VAX V7.1.  (Though
  you are not getting to OpenVMS here.)
 
  If this is a CD-ROM bootstrap, Please review the 512-byte sector
  size requirements discussed in the OpenVMS FAQ.
 
  Please contact your hardware support organization for assistance
  in resolving this problem.  Expect to be asked details of the
  hardware configuration, including details of the bootstrap device
  and of the SCSI bus configuration and termination.
 
 Answer written or last revised on  28-MAY-2002 
