  Third-party hardware? (DECserver modem) 
 The Question is:
 
Hi all,
I need to connect a serial modem on a port of the DECserver 900TM but,
 disaccording with the Wizard FAQ, I can't put the /MODEM option in the LAT
 Port configuration.
Although I can send AT commands to the modem, I recive a error message that
 hang the terminal. This error is due to the fact that the LAT port lowers the
 signal on DTR with a 30 seconds period causing the off-line gone of the modem
 and the hang-up of line
..
So I need:
- Port settings for the DECserver.
- Terminal settings for LTA Terminal.
- a QIO example (or what needed) to send AT commands to modem from a program.
 
Thank you very much.
Diego
 
 The Answer is :
 
  Please contact Digital Network Products Group for assistance
  with the DECserver 900 series, and for access to documentation.
 
  Pleae reas the Digital Networks documentation on this device,
  and please consider enabling the modem setting out on the
  DECserver port.
 
 Answer written or last revised on  11-APR-2003 
