  DECserver Configuration? 
 The Question is:
 
I am currently replacing two 8 port Emulex terminal servers with a 16 port
DECServer 700. I have managed to configure the ports as per the old servers,
but have been told that I will need to remove the service groups from the
old servers and then add them
 to the new one. Could you tell me how this is easily done? The old servers
are called SRV01A and SRV01B, with the replacement server being called SRV01
 
Thanks, Paul Coombs
 
 
 The Answer is:
 
  The OpenVMS Wizard is not familiar with the operations of Emulex devices.
 
  Service groups are normally established at the DECserver Local prompt.
  Enable privileged access, then see the available HELP for assistance.
 
  On most DECserver devices, the commands are similar to:
 
    SET PRIVILEGE password
    HELP
    DEFINE SERVER
    SET SERVER
 
  The displayed HELP text can be sensitive to the current privilege mode.
 
