  Meaning of LKWSETFUL error? 
 The Question is:
 
I have  Compaq TCP/IP Services for OpenVMS Alpha Version V5.1
  on a AlphaServer ES40 running OpenVMS V7.3
 
 Working Set (pagelets)  /Limit=131072  /Quota=524288  /Extent=524288
  Adjustment enabled      Authorized Quota=524288  Authorized Extent=524288
 
  Working Set (8Kb pages) /Limit=8192  /Quota=32768  /Extent=32768
                          Authorized Quota=32768  Authorized Extent=32768
 
 
when I issue this command  TCPTRACE
 17x.xx.xx.xx/FULL/buffer=5535/packet=30/PORT=LOCAL=25003
 
 
I get  TCPIPTRACE-W-BUFFERSFULL, TCPIPtrace could not save 1 packets.
 
if I increase the buffer  I get the following
 
TCPTRACE 17x.xx.xx.xx/FULL/buffer=65535/packet=30/PORT=LOCAL=25003
%SYSTEM-F-LKWSETFUL, locked portion of working set is full
 
 
I have search for help on this so far no joy. Please help.
 
 
 
 The Answer is :
 
 LKWSETFUL,  locked portion of working set is full
 
  Facility:     SYSTEM, System Services
 
  Explanation:  No more pages can be locked in the working set because there
                would not be enough remaining pages available dynamically for
                the image to continue execution.
 
  User Action:  Use the DCL command SET WORKING_SET to increase the working
                set limit, if the limit is not already set at the maximum
                allowed. If the working set limit is already at the maximum
                allowed, correct the program that attempted to lock too many
                pages in the working set.
 
 
 Answer written or last revised on  17-DEC-2003 
