  Making DECss7 GTT rules static? 
 The Question is:
 
I manage distributed SS7 platforms consisting of either several BEP and FEP
 nodes or a dual monolith (BEP+FEP) nodes. When making a change into the GTT
 Rules tables and applying it from a single node, I succeed in activating that
 change. Though I neverthe
less MUST re-apply the change again on the event of ss7$shutdown/ss7$startup.
 
I tried to find on the Internet what is the correct procedure to make a change
 into the GTT Rules tables across all nodes of a distributed SS7 platform and
 make it static rather than dynamic as it seems to be. I had no success. Could
 you please give me an
y hint? TIA
 
 The Answer is :
 
  The procedure described -- populating the standby table, and then
  making it active with the "switch_table" command -- is correct.
 
  Once the changes are made, the settings should survive over any
  IN7 shutdown-restart sequences.
 
  The OpenVMS Wizard strongly encourages you to report this behavior
  to the organization supporting your IN7 environment.
 
 Answer written or last revised on  19-DEC-2001 
