  Multinet DSN$LOGS:DSN_SRA_SERVER.LOG failure mes 
 The Question is:
 
We recently noticed this error messages in operator.log file.
Can you give us a hint how can we clear this errors and what do they mean?
%%%%%%%%%%%  OPCOM   3-FEB-1999 13:33:42.04  %%%%%%%%%%%
Message from user SYSTEM on UMPGAM
MultiNet Server: Log_Open("DSN$LOGS:DSN_SRA_SERVER.LOG") failed: error in
device
 name or inappropriate device type for operation
 
%%%%%%%%%%%  OPCOM   3-FEB-1999 13:33:42.18  %%%%%%%%%%%
Message from user SYSTEM on UMPGAM
MultiNet Server: Log_Open("DSN$LOGS:DSN_NSD_SERVER.LOG") failed: error in
device
 name or inappropriate device type for operation
 
%%%%%%%%%%%  OPCOM   3-FEB-1999 13:33:42.18  %%%%%%%%%%%
Message from user SYSTEM on UMPGAM
MultiNet Server: Log_Open("DSN$LOGS:DSN_NETEX_SERVER.LOG") failed: error in
devi
ce name or inappropriate device type for operation
 
%%%%%%%%%%%  OPCOM   3-FEB-1999 13:33:42.19  %%%%%%%%%%%
Message from user SYSTEM on UMPGAM
MultiNet Server: Log_Open("DSN$LOGS:DSN_MAIL_SERVER.LOG") failed: error in
devic
e name or inappropriate device type for operation
 
%%%%%%%%%%%  OPCOM   3-FEB-1999 13:33:42.19  %%%%%%%%%%%
Message from user SYSTEM on UMPGAM
MultiNet Server: Log_Open("DSN$LOGS:DSN_LOGIN_SERVER.LOG") failed: error in
devi
ce name or inappropriate device type for operation
****************************************************************************
 
 
 The Answer is:
 
  The OpenVMS Wizard would check the logical name DSN$LOGS to make sure
  that it is visible to the process that wants to use it.  This logical
  name may need to be defined with /SYSTEM/EXECUTIVE, so check the value
  with SHOW LOGICAL/FULL DSN$LOGS.
 
  Apart from that, you might want to ask the MultiNet Wizard.
 
  If this is the Compaq DSN support network package, please contact the
  customer support center for assistance.
 
