  AlphaServer 800 minimum OpenVMS version? 
 The Question is:
 
Can OpenVMS 6.2 be run on an Blue box Alphaserver 800, if so which release
do I need.
 
 
 The Answer is:
 
  AlphaServer 800 have an integrated UltraSCSI controller and thus require
  OpenVMS Alpha V7.1-1H1 or later, or can operate on OpenVMS Alpha V6.2-1H3
  with the addition of an UltraSCSI ECO kit -- ALPSCSI*.
 
  Note that the AlphaServer 800 systems cannot boot off a standard OpenVMS
  Alpha V6.2-1H3 distribution, as this release does not include the necessary
  UltraSCSI ECO kit -- alternate mechanisms for standalone operations -- such
  as using a V7.1-1H1 or later OpenVMS Alpha kit or using another system
  sharing the same system disk -- for the initial bootstrap (prior to the
  application of the necessary kit), upgrades (to any releases prior to
  V7.1-1H1, which is the first release with UltraSCSI sypport) and for
  system disk restoration in the event of a failure must be made.
