  Machine Check (MCHK) IOD Detected Hard Error? 
 The Question is:
 
i have AS4100 which crash sometime with a error iod detected hard error . this
 error occured only on the second pci iod1 .in this bus pci i have DE600 and
 KZPSA-BB .
thank for your help
best regards
 
 The Answer is :
 
  Please contact your hardware support organization for assistance with
  this and with any other apparently-hardware-related errors -- this
  message is usually associated with DECevent or Compaq Analyze output
  for a machine check, with the usual supporting text for the machine
  check -- as displayed by the bit-to-text error log translation -- being
  "IOD-Detected Hard Error -OR- DTag Parity Error (If Cached CPU)" or
  similar.  Machine checks are -- as previously discussed here in the
  Ask The Wizard area -- usually either hardware errors or (potentially)
  very low-level software errors.
 Answer written or last revised on  13-JAN-2003 
