  One network name for OpenVMS Cluster? (alias) 
 The Question is:
 
We have a system consisting of two AXP 1200's and one DEC 3000 running in a
non-homogenous cluster. However, we would like to find a solution that would
allow us to run this system as a homogenous cluster, WITHOUT setting up a
LAT-service. We really don't
 want to use LAT over our WAN-links, for obvious reasons. But we would like
to be able to just log in to "the cluster", rather than manually selecting
the node. We thought about setting up a router that would translate our
IP-commmunication to a LAT-servi
ce, but that would leave us with a single-point of failure at the router.
 
Is there a way to set this up without a LAT-service?
 
 
 The Answer is:
 
  LAT, DECnet, and IP all support a cluster alias mechanism.
